(kicad_pcb (version 20221018) (generator pcbnew)
  (general
    (thickness 0.92424)
  )
  (paper "A4")
  (layers
    (0 "F.Cu" signal "Front")
    (31 "B.Cu" signal "Back")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (49 "F.Fab" user)
  )
  (setup
    (stackup
      (layer "F.SilkS" (type "Top Silk Screen"))
      (layer "F.Paste" (type "Top Solder Paste"))
      (layer "F.Mask" (type "Top Solder Mask") (thickness 0.01))
      (layer "F.Cu" (type "copper") (thickness 0.07112))
      (layer "dielectric 1" (type "core") (thickness 0.762) (material "FR4") (epsilon_r 4.5) (loss_tangent 0.02))
      (layer "B.Cu" (type "copper") (thickness 0.07112))
      (layer "B.Mask" (type "Bottom Solder Mask") (thickness 0.01))
      (layer "B.Paste" (type "Bottom Solder Paste"))
      (layer "B.SilkS" (type "Bottom Silk Screen"))
      (copper_finish "None")
      (dielectric_constraints no)
    )
    (pad_to_mask_clearance 0.0508)
    (grid_origin 99.06 88.9)
    (pcbplotparams
      (layerselection 0x00010fc_ffffffff)
      (plot_on_all_layers_selection 0x0000000_00000000)
      (disableapertmacros false)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (dashed_line_dash_ratio 12.000000)
      (dashed_line_gap_ratio 3.000000)
      (svgprecision 6)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory "")
    )
  )
  (net 0 "")
  (net 1 "GND")
  (net 2 "FAN")
  (net 3 "+12V")
  (net 4 "BTN")
  (footprint "Connector_PinSocket_2.54mm:PinSocket_2x02_P2.54mm_Vertical" (layer "B.Cu")
    (at 99.06 88.9 180)
    (descr "Through hole straight socket strip, 2x02, 2.54mm pitch, double cols (from Kicad 4.0.7), script generated")
    (tags "Through hole socket strip THT 2x02 2.54mm double row")
    (property "Sheetfile" "power_conn.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, double row, 02x02, odd/even pin numbering scheme (row 1 odd numbers, row 2 even numbers), script generated (kicad-library-utils/schlib/autogen/connector/)")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "X1" (at -1.27 -5.588) (layer "B.SilkS"))
    (fp_text value "Conn_02x02_Odd_Even" (at -1.27 -5.31) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at -1.27 -1.27 90) (layer "B.Fab"))
    (pad "1" thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 4 "BTN") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at -2.54 0 180) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 3 "+12V") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 -2.54 180) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 2 "FAN") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole oval (at -2.54 -2.54 180) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 1 "GND") (pinfunction "Pin_4") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_2x02_P2.54mm_Vertical.wrl" hide
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model "${KIPRJMOD}/PARTS/BCS-102-L-D-TE.step"
      (offset (xyz -1.27 -1.27 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )
  (footprint "Connector_PinHeader_2.54mm:PinHeader_2x03_P2.54mm_Horizontal" (layer "B.Cu")
    (at 78.74 88.9 -90)
    (descr "Through hole angled pin header, 2x03, 2.54mm pitch, 6mm pin length, double rows")
    (tags "Through hole angled pin header THT 2x03 2.54mm double row")
    (property "Sheetfile" "power_conn.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, double row, 02x03, odd/even pin numbering scheme (row 1 odd numbers, row 2 even numbers), script generated (kicad-library-utils/schlib/autogen/connector/)")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "X2" (at 5.334 -7.62 90) (layer "B.SilkS"))
    (fp_text value "Conn_02x03_Odd_Even" (at 5.655 -7.35 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 5.31 -2.54) (layer "B.Fab"))
    (pad "1" thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 3 "+12V") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 2.54 0 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 2 "FAN") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 -2.54 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 3 "+12V") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole oval (at 2.54 -2.54 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 1 "GND") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" thru_hole oval (at 0 -5.08 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 3 "+12V") (pinfunction "Pin_5") (pintype "passive"))
    (pad "6" thru_hole oval (at 2.54 -5.08 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 4 "BTN") (pinfunction "Pin_6") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_2x03_P2.54mm_Horizontal.wrl" hide
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model "${KIPRJMOD}/PARTS/HTSW-103-08-L-D-NA.step"
      (offset (xyz 4.064 -2.54 2.54))
      (scale (xyz 1 1 1))
      (rotate (xyz 180 0 -90))
    )
  )
  (gr_arc (start 104.14 87.122) (mid 104.678815 87.345185) (end 104.902 87.884)
    (layer "Edge.Cuts"))
  (gr_arc (start 76.962 87.884) (mid 77.185185 87.345185) (end 77.724 87.122)
    (layer "Edge.Cuts"))
  (gr_line (start 104.902 87.884) (end 104.902 95.25)
    (layer "Edge.Cuts"))
  (gr_arc (start 104.902 95.25) (mid 104.678815 95.788815) (end 104.14 96.012)
    (layer "Edge.Cuts"))
  (gr_arc (start 77.724 96.012) (mid 77.185185 95.788815) (end 76.962 95.25)
    (layer "Edge.Cuts"))
  (gr_line (start 104.14 96.012) (end 77.724 96.012)
    (layer "Edge.Cuts"))
  (gr_line (start 77.724 87.122) (end 104.14 87.122)
    (layer "Edge.Cuts"))
  (gr_line (start 76.962 95.25) (end 76.962 87.884)
    (layer "Edge.Cuts"))
  (gr_text "+" (at 91.3638 92.7354 90) (layer "B.SilkS"))
  (gr_text "BTN\n" (at 93.7514 87.63 90) (layer "B.SilkS"))
  (gr_text "-" (at 91.3638 94.5134 90) (layer "B.SilkS"))
  (gr_text "-" (at 89.0778 94.5134 90) (layer "B.SilkS"))
  (gr_text "+" (at 93.6498 92.7354 90) (layer "B.SilkS"))
  (gr_text "PWR" (at 91.4654 87.63 90) (layer "B.SilkS"))
  (gr_text "-" (at 93.6498 94.5134 90) (layer "B.SilkS"))
  (gr_text "FAN\n" (at 89.1794 87.63 90) (layer "B.SilkS"))
  (gr_text "+" (at 89.0778 92.7354 90) (layer "B.SilkS"))
  (gr_text "-" (at 93.6498 92.6846 90) (layer "F.SilkS"))
  (gr_text "+" (at 93.6498 94.4626 90) (layer "F.SilkS"))
  (gr_text "-" (at 89.0778 92.6846 90) (layer "F.SilkS"))
  (gr_text "FAN\n" (at 89.2048 91.186 90) (layer "F.SilkS"))
  (gr_text "+" (at 91.3638 94.4626 90) (layer "F.SilkS"))
  (gr_text "-" (at 91.3638 92.6846 90) (layer "F.SilkS"))
  (gr_text "+" (at 89.0778 94.4626 90) (layer "F.SilkS"))
  (gr_text "PWR" (at 91.4908 91.186 90) (layer "F.SilkS"))
  (gr_text "BTN\n" (at 93.7768 91.186 90) (layer "F.SilkS"))
  (dimension (type aligned) (layer "Edge.Cuts")
    (pts (xy 104.14 87.122) (xy 104.14 96.012))
    (height -3.556)
    (gr_text "350,0000 mils" (at 106.546 91.567 90) (layer "Edge.Cuts"))
    (format (prefix "") (suffix "") (units 3) (units_format 1) (precision 4))
    (style (thickness 0.0381) (arrow_length 1.27) (text_position_mode 0) (extension_height 0.58642) (extension_offset 0.5) keep_text_aligned)
  )
  (dimension (type aligned) (layer "Edge.Cuts")
    (pts (xy 76.962 87.884) (xy 104.902 87.884))
    (height -2.54)
    (gr_text "1100,0000 mils" (at 90.932 84.194) (layer "Edge.Cuts"))
    (format (prefix "") (suffix "") (units 3) (units_format 1) (precision 4))
    (style (thickness 0.0381) (arrow_length 1.27) (text_position_mode 0) (extension_height 0.58642) (extension_offset 0.5) keep_text_aligned)
  )
  (zone (net 3) (net_name "+12V") (layer "F.Cu") (name "GND") (hatch edge 0.508)
    (connect_pads yes (clearance 0.2))
    (min_thickness 0.2) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.22) (thermal_bridge_width 0.4))
    (polygon
      (pts
        (xy 104.902 96.012)
        (xy 76.962 96.012)
        (xy 76.962 87.122)
        (xy 104.902 87.122)
      )
    )
  )
  (zone (net 1) (net_name "GND") (layer "B.Cu") (name "GND") (hatch edge 0.508)
    (connect_pads yes (clearance 0.2))
    (min_thickness 0.2) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.22) (thermal_bridge_width 0.4))
    (polygon
      (pts
        (xy 104.902 96.012)
        (xy 76.962 96.012)
        (xy 76.962 87.122)
        (xy 104.902 87.122)
      )
    )
  )
)
