(kicad_pcb (version 20221018) (generator pcbnew)
  (general
    (thickness 0.92424)
  )
  (paper "A4")
  (layers
    (0 "F.Cu" signal "Front")
    (31 "B.Cu" signal "Back")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (49 "F.Fab" user)
  )
  (setup
    (stackup
      (layer "F.SilkS" (type "Top Silk Screen"))
      (layer "F.Paste" (type "Top Solder Paste"))
      (layer "F.Mask" (type "Top Solder Mask") (thickness 0.01))
      (layer "F.Cu" (type "copper") (thickness 0.07112))
      (layer "dielectric 1" (type "core") (thickness 0.762) (material "FR4") (epsilon_r 4.5) (loss_tangent 0.02))
      (layer "B.Cu" (type "copper") (thickness 0.07112))
      (layer "B.Mask" (type "Bottom Solder Mask") (thickness 0.01))
      (layer "B.Paste" (type "Bottom Solder Paste"))
      (layer "B.SilkS" (type "Bottom Silk Screen"))
      (copper_finish "None")
      (dielectric_constraints no)
    )
    (pad_to_mask_clearance 0.0508)
    (aux_axis_origin 149.926776 93.92816)
    (grid_origin 150 93.92816)
    (pcbplotparams
      (layerselection 0x00010fc_ffffffff)
      (plot_on_all_layers_selection 0x0000000_00000000)
      (disableapertmacros false)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (dashed_line_dash_ratio 12.000000)
      (dashed_line_gap_ratio 3.000000)
      (svgprecision 6)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory "")
    )
  )
  (net 0 "")
  (net 1 "IOVDD")
  (net 2 "XIN")
  (net 3 "SWCLK")
  (net 4 "RUN")
  (net 5 "SWDIO")
  (net 6 "GNDD")
  (net 7 "DVDD")
  (net 8 "DM")
  (net 9 "DP")
  (net 10 "ADC_AVDD")
  (net 11 "VREG_IN")
  (net 12 "VBUS")
  (net 13 "/Peripherials/GPIO16")
  (net 14 "/Peripherials/GPIO17")
  (net 15 "/Peripherials/GPIO18")
  (net 16 "/Peripherials/GPIO19")
  (net 17 "/Peripherials/GPIO20")
  (net 18 "/Peripherials/GPIO21")
  (net 19 "/Peripherials/GPIO22")
  (net 20 "/Peripherials/GPIO23")
  (net 21 "/Peripherials/GPIO24")
  (net 22 "/Peripherials/GPIO25")
  (net 23 "/Peripherials/GPIO26")
  (net 24 "/Peripherials/GPIO27")
  (net 25 "/Peripherials/GPIO28")
  (net 26 "/Peripherials/GPIO29")
  (net 27 "/Peripherials/QSPI.SCLK")
  (net 28 "/Peripherials/QSPI.D0")
  (net 29 "/Peripherials/QSPI.SS")
  (net 30 "/Peripherials/GPIO0")
  (net 31 "/Peripherials/GPIO1")
  (net 32 "/Peripherials/GPIO2")
  (net 33 "/Peripherials/GPIO3")
  (net 34 "/Peripherials/GPIO4")
  (net 35 "/Peripherials/GPIO5")
  (net 36 "/Peripherials/GPIO6")
  (net 37 "/Peripherials/GPIO7")
  (net 38 "/Peripherials/GPIO8")
  (net 39 "/Peripherials/GPIO9")
  (net 40 "/Peripherials/GPIO10")
  (net 41 "/Peripherials/GPIO11")
  (net 42 "/Peripherials/GPIO12")
  (net 43 "/Peripherials/GPIO13")
  (net 44 "/Peripherials/GPIO14")
  (net 45 "/Peripherials/GPIO15")
  (net 46 "/Peripherials/QSPI.D1")
  (net 47 "/Peripherials/QSPI.D2")
  (net 48 "/Peripherials/QSPI.D3")
  (net 49 "Net-(U201-USB_DP)")
  (net 50 "Net-(U201-USB_DM)")
  (net 51 "Net-(X201-ID)")
  (net 52 "unconnected-(U201-XOUT-Pad21)")
  (net 53 "/Interface/GPIO16")
  (net 54 "/Interface/GPIO17")
  (net 55 "/Interface/GPIO18")
  (net 56 "/Interface/GPIO19")
  (net 57 "/Interface/GPIO20")
  (net 58 "/Interface/GPIO21")
  (net 59 "/Interface/GPIO22")
  (net 60 "/Interface/GPIO23")
  (net 61 "/Interface/GPIO24")
  (net 62 "/Interface/GPIO25")
  (net 63 "/Interface/GPIO26")
  (net 64 "/Interface/GPIO27")
  (net 65 "/Interface/GPIO28")
  (net 66 "/Interface/GPIO29")
  (net 67 "/Interface/QSPI.SCLK")
  (net 68 "/Interface/QSPI.D0")
  (net 69 "/Interface/QSPI.SS")
  (net 70 "/Interface/GPIO0")
  (net 71 "/Interface/GPIO1")
  (net 72 "/Interface/GPIO2")
  (net 73 "/Interface/GPIO3")
  (net 74 "/Interface/GPIO4")
  (net 75 "/Interface/GPIO5")
  (net 76 "/Interface/GPIO6")
  (net 77 "/Interface/GPIO7")
  (net 78 "/Interface/GPIO8")
  (net 79 "/Interface/GPIO9")
  (net 80 "/Interface/GPIO10")
  (net 81 "/Interface/GPIO11")
  (net 82 "/Interface/GPIO12")
  (net 83 "/Interface/GPIO13")
  (net 84 "/Interface/GPIO14")
  (net 85 "/Interface/GPIO15")
  (net 86 "/Interface/QSPI.D1")
  (net 87 "/Interface/QSPI.D2")
  (net 88 "/Interface/QSPI.D3")
  (net 89 "Net-(U301-USB_DP)")
  (net 90 "Net-(U301-USB_DM)")
  (net 91 "Net-(X301-ID)")
  (net 92 "unconnected-(U301-XOUT-Pad21)")
  (net 93 "unconnected-(X1-Pad1)")
  (net 94 "unconnected-(X1-Pad2)")
  (net 95 "unconnected-(X1-Pad3)")
  (net 96 "unconnected-(X1-Pad4)")
  (net 97 "unconnected-(X1-Pad5)")
  (net 98 "unconnected-(X1-Pad6)")
  (net 99 "unconnected-(X1-Pad7)")
  (net 100 "unconnected-(X1-Pad8)")
  (net 101 "unconnected-(X1-Pad9)")
  (net 102 "unconnected-(X1-Pad10)")
  (net 103 "unconnected-(X2-Pad1)")
  (net 104 "unconnected-(X2-Pad2)")
  (net 105 "unconnected-(X2-Pad3)")
  (net 106 "unconnected-(X2-Pad4)")
  (net 107 "unconnected-(X2-Pad5)")
  (net 108 "unconnected-(X2-Pad6)")
  (net 109 "unconnected-(X2-Pad7)")
  (net 110 "unconnected-(X2-Pad8)")
  (net 111 "unconnected-(X2-Pad9)")
  (net 112 "unconnected-(X2-Pad10)")
  (net 113 "Net-(X3-GND-PadA1)")
  (net 114 "Net-(X3-VBUS-PadA4)")
  (net 115 "unconnected-(X3-CC1-PadA5)")
  (net 116 "unconnected-(X3-D+-PadA6)")
  (net 117 "unconnected-(X3-D--PadA7)")
  (net 118 "unconnected-(X3-SBU1-PadA8)")
  (net 119 "unconnected-(X3-CC2-PadB5)")
  (net 120 "unconnected-(X3-D+-PadB6)")
  (net 121 "unconnected-(X3-D--PadB7)")
  (net 122 "unconnected-(X3-SBU2-PadB8)")
  (net 123 "unconnected-(X3-SHIELD-PadS1)")
  (footprint "MCU_RaspberryPi_and_Boards:RP2040-QFN-56" (layer "F.Cu")
    (at 50 143.92816 -90)
    (descr "QFN, 56 Pin (http://www.cypress.com/file/416486/download#page=40), generated with kicad-footprint-generator ipc_dfn_qfn_generator.py")
    (tags "QFN DFN_QFN")
    (property "Field2" "")
    (property "Sheetfile" "peripherials_sch.kicad_sch")
    (property "Sheetname" "Peripherials")
    (zone_connect 2)
    (attr smd)
    (fp_text reference "U201" (at -4.2 -4.82) (layer "F.SilkS"))
    (fp_text value "RP2040" (at -3.4 5.02 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "" smd roundrect (at -0.6375 -0.6375 270) (size 1.084435 1.084435) (layers "F.Paste") (roundrect_rratio 0.230535))
    (pad "" smd roundrect (at -0.6375 0.6375 270) (size 1.084435 1.084435) (layers "F.Paste") (roundrect_rratio 0.230535))
    (pad "" smd roundrect (at 0.6375 -0.6375 270) (size 1.084435 1.084435) (layers "F.Paste") (roundrect_rratio 0.230535))
    (pad "" smd roundrect (at 0.6375 0.6375 270) (size 1.084435 1.084435) (layers "F.Paste") (roundrect_rratio 0.230535))
    (pad "1" smd roundrect (at -3.4375 -2.6 270) (size 0.875 0.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "IOVDD") (pinfunction "IOVDD") (pintype "power_in"))
    (pad "2" smd roundrect (at -3.4375 -2.2 270) (size 0.875 0.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 30 "/Peripherials/GPIO0") (pinfunction "GPIO0") (pintype "bidirectional"))
    (pad "3" smd roundrect (at -3.4375 -1.8 270) (size 0.875 0.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 31 "/Peripherials/GPIO1") (pinfunction "GPIO1") (pintype "bidirectional"))
    (pad "4" smd roundrect (at -3.4375 -1.4 270) (size 0.875 0.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 32 "/Peripherials/GPIO2") (pinfunction "GPIO2") (pintype "bidirectional"))
    (pad "5" smd roundrect (at -3.4375 -1 270) (size 0.875 0.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 33 "/Peripherials/GPIO3") (pinfunction "GPIO3") (pintype "bidirectional"))
    (pad "6" smd roundrect (at -3.4375 -0.6 270) (size 0.875 0.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 34 "/Peripherials/GPIO4") (pinfunction "GPIO4") (pintype "bidirectional"))
    (pad "7" smd roundrect (at -3.4375 -0.2 270) (size 0.875 0.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 35 "/Peripherials/GPIO5") (pinfunction "GPIO5") (pintype "bidirectional"))
    (pad "8" smd roundrect (at -3.4375 0.2 270) (size 0.875 0.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 36 "/Peripherials/GPIO6") (pinfunction "GPIO6") (pintype "bidirectional"))
    (pad "9" smd roundrect (at -3.4375 0.6 270) (size 0.875 0.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 37 "/Peripherials/GPIO7") (pinfunction "GPIO7") (pintype "bidirectional"))
    (pad "10" smd roundrect (at -3.4375 1 270) (size 0.875 0.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "IOVDD") (pinfunction "IOVDD") (pintype "power_in"))
    (pad "11" smd roundrect (at -3.4375 1.4 270) (size 0.875 0.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 38 "/Peripherials/GPIO8") (pinfunction "GPIO8") (pintype "bidirectional"))
    (pad "12" smd roundrect (at -3.4375 1.8 270) (size 0.875 0.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 39 "/Peripherials/GPIO9") (pinfunction "GPIO9") (pintype "bidirectional"))
    (pad "13" smd roundrect (at -3.4375 2.2 270) (size 0.875 0.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 40 "/Peripherials/GPIO10") (pinfunction "GPIO10") (pintype "bidirectional"))
    (pad "14" smd roundrect (at -3.4375 2.6 270) (size 0.875 0.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 41 "/Peripherials/GPIO11") (pinfunction "GPIO11") (pintype "bidirectional"))
    (pad "15" smd roundrect (at -2.6 3.4375 270) (size 0.2 0.875) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 42 "/Peripherials/GPIO12") (pinfunction "GPIO12") (pintype "bidirectional"))
    (pad "16" smd roundrect (at -2.2 3.4375 270) (size 0.2 0.875) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 43 "/Peripherials/GPIO13") (pinfunction "GPIO13") (pintype "bidirectional"))
    (pad "17" smd roundrect (at -1.8 3.4375 270) (size 0.2 0.875) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 44 "/Peripherials/GPIO14") (pinfunction "GPIO14") (pintype "bidirectional"))
    (pad "18" smd roundrect (at -1.4 3.4375 270) (size 0.2 0.875) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 45 "/Peripherials/GPIO15") (pinfunction "GPIO15") (pintype "bidirectional"))
    (pad "19" smd roundrect (at -1 3.4375 270) (size 0.2 0.875) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 6 "GNDD") (pinfunction "TESTEN") (pintype "passive"))
    (pad "20" smd roundrect (at -0.6 3.4375 270) (size 0.2 0.875) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "XIN") (pinfunction "XIN") (pintype "input"))
    (pad "21" smd roundrect (at -0.2 3.4375 270) (size 0.2 0.875) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 52 "unconnected-(U201-XOUT-Pad21)") (pinfunction "XOUT") (pintype "passive"))
    (pad "22" smd roundrect (at 0.2 3.4375 270) (size 0.2 0.875) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "IOVDD") (pinfunction "IOVDD") (pintype "power_in"))
    (pad "23" smd roundrect (at 0.6 3.4375 270) (size 0.2 0.875) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 7 "DVDD") (pinfunction "DVDD") (pintype "power_in"))
    (pad "24" smd roundrect (at 1 3.4375 270) (size 0.2 0.875) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 3 "SWCLK") (pinfunction "SWCLK") (pintype "output"))
    (pad "25" smd roundrect (at 1.4 3.4375 270) (size 0.2 0.875) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 5 "SWDIO") (pinfunction "SWD") (pintype "bidirectional"))
    (pad "26" smd roundrect (at 1.8 3.4375 270) (size 0.2 0.875) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "RUN") (pinfunction "RUN") (pintype "input"))
    (pad "27" smd roundrect (at 2.2 3.4375 270) (size 0.2 0.875) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 13 "/Peripherials/GPIO16") (pinfunction "GPIO16") (pintype "bidirectional"))
    (pad "28" smd roundrect (at 2.6 3.4375 270) (size 0.2 0.875) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 14 "/Peripherials/GPIO17") (pinfunction "GPIO17") (pintype "bidirectional"))
    (pad "29" smd roundrect (at 3.4375 2.6 270) (size 0.875 0.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 15 "/Peripherials/GPIO18") (pinfunction "GPIO18") (pintype "bidirectional"))
    (pad "30" smd roundrect (at 3.4375 2.2 270) (size 0.875 0.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 16 "/Peripherials/GPIO19") (pinfunction "GPIO19") (pintype "bidirectional"))
    (pad "31" smd roundrect (at 3.4375 1.8 270) (size 0.875 0.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 17 "/Peripherials/GPIO20") (pinfunction "GPIO20") (pintype "bidirectional"))
    (pad "32" smd roundrect (at 3.4375 1.4 270) (size 0.875 0.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 18 "/Peripherials/GPIO21") (pinfunction "GPIO21") (pintype "bidirectional"))
    (pad "33" smd roundrect (at 3.4375 1 270) (size 0.875 0.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "IOVDD") (pinfunction "IOVDD") (pintype "power_in"))
    (pad "34" smd roundrect (at 3.4375 0.6 270) (size 0.875 0.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 19 "/Peripherials/GPIO22") (pinfunction "GPIO22") (pintype "bidirectional"))
    (pad "35" smd roundrect (at 3.4375 0.2 270) (size 0.875 0.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 20 "/Peripherials/GPIO23") (pinfunction "GPIO23") (pintype "bidirectional"))
    (pad "36" smd roundrect (at 3.4375 -0.2 270) (size 0.875 0.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 21 "/Peripherials/GPIO24") (pinfunction "GPIO24") (pintype "bidirectional"))
    (pad "37" smd roundrect (at 3.4375 -0.6 270) (size 0.875 0.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 22 "/Peripherials/GPIO25") (pinfunction "GPIO25") (pintype "bidirectional"))
    (pad "38" smd roundrect (at 3.4375 -1 270) (size 0.875 0.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 23 "/Peripherials/GPIO26") (pinfunction "GPIO26_ADC0") (pintype "bidirectional"))
    (pad "39" smd roundrect (at 3.4375 -1.4 270) (size 0.875 0.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 24 "/Peripherials/GPIO27") (pinfunction "GPIO27_ADC1") (pintype "bidirectional"))
    (pad "40" smd roundrect (at 3.4375 -1.8 270) (size 0.875 0.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 25 "/Peripherials/GPIO28") (pinfunction "GPIO28_ADC2") (pintype "bidirectional"))
    (pad "41" smd roundrect (at 3.4375 -2.2 270) (size 0.875 0.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 26 "/Peripherials/GPIO29") (pinfunction "GPIO29_ADC3") (pintype "bidirectional"))
    (pad "42" smd roundrect (at 3.4375 -2.6 270) (size 0.875 0.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "IOVDD") (pinfunction "IOVDD") (pintype "power_in"))
    (pad "43" smd roundrect (at 2.6 -3.4375 270) (size 0.2 0.875) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 10 "ADC_AVDD") (pinfunction "ADC_AVDD") (pintype "power_in"))
    (pad "44" smd roundrect (at 2.2 -3.4375 270) (size 0.2 0.875) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 11 "VREG_IN") (pinfunction "VREG_IN") (pintype "power_in"))
    (pad "45" smd roundrect (at 1.8 -3.4375 270) (size 0.2 0.875) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 7 "DVDD") (pinfunction "VREG_VOUT") (pintype "power_out"))
    (pad "46" smd roundrect (at 1.4 -3.4375 270) (size 0.2 0.875) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 50 "Net-(U201-USB_DM)") (pinfunction "USB_DM") (pintype "bidirectional"))
    (pad "47" smd roundrect (at 1 -3.4375 270) (size 0.2 0.875) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 49 "Net-(U201-USB_DP)") (pinfunction "USB_DP") (pintype "bidirectional"))
    (pad "48" smd roundrect (at 0.6 -3.4375 270) (size 0.2 0.875) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "IOVDD") (pinfunction "USB_VDD") (pintype "power_in"))
    (pad "49" smd roundrect (at 0.2 -3.4375 270) (size 0.2 0.875) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "IOVDD") (pinfunction "IOVDD") (pintype "power_in"))
    (pad "50" smd roundrect (at -0.2 -3.4375 270) (size 0.2 0.875) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 7 "DVDD") (pinfunction "DVDD") (pintype "power_in"))
    (pad "51" smd roundrect (at -0.6 -3.4375 270) (size 0.2 0.875) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 48 "/Peripherials/QSPI.D3") (pinfunction "QSPI_SD3") (pintype "bidirectional"))
    (pad "52" smd roundrect (at -1 -3.4375 270) (size 0.2 0.875) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 27 "/Peripherials/QSPI.SCLK") (pinfunction "QSPI_SCLK") (pintype "output"))
    (pad "53" smd roundrect (at -1.4 -3.4375 270) (size 0.2 0.875) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 28 "/Peripherials/QSPI.D0") (pinfunction "QSPI_SD0") (pintype "bidirectional"))
    (pad "54" smd roundrect (at -1.8 -3.4375 270) (size 0.2 0.875) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 47 "/Peripherials/QSPI.D2") (pinfunction "QSPI_SD2") (pintype "bidirectional"))
    (pad "55" smd roundrect (at -2.2 -3.4375 270) (size 0.2 0.875) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 46 "/Peripherials/QSPI.D1") (pinfunction "QSPI_SD1") (pintype "bidirectional"))
    (pad "56" smd roundrect (at -2.6 -3.4375 270) (size 0.2 0.875) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 29 "/Peripherials/QSPI.SS") (pinfunction "QSPI_SS") (pintype "bidirectional"))
    (pad "57" thru_hole circle (at -1.275 -1.275 270) (size 0.6 0.6) (drill 0.35) (layers "*.Cu")
      (net 6 "GNDD") (pinfunction "GND") (pintype "power_in"))
    (pad "57" thru_hole circle (at -1.275 0 270) (size 0.6 0.6) (drill 0.35) (layers "*.Cu")
      (net 6 "GNDD") (pinfunction "GND") (pintype "power_in"))
    (pad "57" thru_hole circle (at -1.275 1.275 270) (size 0.6 0.6) (drill 0.35) (layers "*.Cu")
      (net 6 "GNDD") (pinfunction "GND") (pintype "power_in"))
    (pad "57" thru_hole circle (at 0 -1.275 270) (size 0.6 0.6) (drill 0.35) (layers "*.Cu")
      (net 6 "GNDD") (pinfunction "GND") (pintype "power_in"))
    (pad "57" thru_hole circle (at 0 0 270) (size 0.6 0.6) (drill 0.35) (layers "*.Cu")
      (net 6 "GNDD") (pinfunction "GND") (pintype "power_in"))
    (pad "57" smd roundrect (at 0 0 270) (size 3.2 3.2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.045)
      (net 6 "GNDD") (pinfunction "GND") (pintype "power_in"))
    (pad "57" thru_hole circle (at 0 1.275 270) (size 0.6 0.6) (drill 0.35) (layers "*.Cu")
      (net 6 "GNDD") (pinfunction "GND") (pintype "power_in"))
    (pad "57" thru_hole circle (at 1.275 -1.275 270) (size 0.6 0.6) (drill 0.35) (layers "*.Cu")
      (net 6 "GNDD") (pinfunction "GND") (pintype "power_in"))
    (pad "57" thru_hole circle (at 1.275 0 270) (size 0.6 0.6) (drill 0.35) (layers "*.Cu")
      (net 6 "GNDD") (pinfunction "GND") (pintype "power_in"))
    (pad "57" thru_hole circle (at 1.275 1.275 270) (size 0.6 0.6) (drill 0.35) (layers "*.Cu")
      (net 6 "GNDD") (pinfunction "GND") (pintype "power_in"))
    (model "${KISYS3DMOD}/Package_DFN_QFN.3dshapes/QFN-56-1EP_7x7mm_P0.4mm_EP5.6x5.6mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model "RP2040_QFN56_04.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0402_1005Metric" (layer "F.Cu")
    (at 57.2 170.62816)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Field2" "")
    (property "Sheetfile" "interface_sch.kicad_sch")
    (property "Sheetname" "Interface")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R302" (at 2.4 0.4) (layer "F.SilkS"))
    (fp_text value "27R" (at 0 1.17) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.51 0) (size 0.54 0.64) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 90 "Net-(U301-USB_DM)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.51 0) (size 0.54 0.64) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 8 "DM") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinHeader_2.54mm:PinHeader_1x03_P2.54mm_Vertical" (layer "F.Cu")
    (at 33.49 141.38816 90)
    (descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x03 2.54mm single row")
    (property "Field2" "")
    (property "Sheetfile" "peripherials_sch.kicad_sch")
    (property "Sheetname" "Peripherials")
    (property "ki_description" "Generic connector, single row, 01x03, script generated (kicad-library-utils/schlib/autogen/connector/)")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "J205" (at -0.889 7.874) (layer "F.SilkS"))
    (fp_text value "Conn_01x03" (at -3.048 2.54) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 2.54) (layer "F.Fab"))
    (pad "1" thru_hole roundrect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask") (roundrect_rratio 0.25)
      (net 2 "XIN") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 6 "GNDD") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 4 "RUN") (pinfunction "Pin_3") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x03_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0402_1005Metric" (layer "F.Cu")
    (at 57.2 144.62816)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Field2" "")
    (property "Sheetfile" "peripherials_sch.kicad_sch")
    (property "Sheetname" "Peripherials")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R201" (at 2.4 -0.4) (layer "F.SilkS"))
    (fp_text value "27R" (at 0 -1.23) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.51 0) (size 0.54 0.64) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 49 "Net-(U201-USB_DP)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.51 0) (size 0.54 0.64) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 9 "DP") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinHeader_2.54mm:PinHeader_1x20_P2.54mm_Vertical" (layer "F.Cu")
    (at 76.67 135.03816 -90)
    (descr "Through hole straight pin header, 1x20, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x20 2.54mm single row")
    (property "Field2" "")
    (property "Sheetfile" "peripherials_sch.kicad_sch")
    (property "Sheetname" "Peripherials")
    (property "ki_description" "Generic connector, single row, 01x20, script generated (kicad-library-utils/schlib/autogen/connector/)")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "J202" (at 3.048 48.514) (layer "F.SilkS"))
    (fp_text value "Conn_01x20" (at 2.794 24.13) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 24.13) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 27 "/Peripherials/QSPI.SCLK") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 2.54 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 28 "/Peripherials/QSPI.D0") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 5.08 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 29 "/Peripherials/QSPI.SS") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole oval (at 0 7.62 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 6 "GNDD") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" thru_hole oval (at 0 10.16 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 30 "/Peripherials/GPIO0") (pinfunction "Pin_5") (pintype "passive"))
    (pad "6" thru_hole oval (at 0 12.7 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 31 "/Peripherials/GPIO1") (pinfunction "Pin_6") (pintype "passive"))
    (pad "7" thru_hole oval (at 0 15.24 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 32 "/Peripherials/GPIO2") (pinfunction "Pin_7") (pintype "passive"))
    (pad "8" thru_hole oval (at 0 17.78 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 33 "/Peripherials/GPIO3") (pinfunction "Pin_8") (pintype "passive"))
    (pad "9" thru_hole oval (at 0 20.32 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 34 "/Peripherials/GPIO4") (pinfunction "Pin_9") (pintype "passive"))
    (pad "10" thru_hole oval (at 0 22.86 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 35 "/Peripherials/GPIO5") (pinfunction "Pin_10") (pintype "passive"))
    (pad "11" thru_hole oval (at 0 25.4 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 36 "/Peripherials/GPIO6") (pinfunction "Pin_11") (pintype "passive"))
    (pad "12" thru_hole oval (at 0 27.94 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 37 "/Peripherials/GPIO7") (pinfunction "Pin_12") (pintype "passive"))
    (pad "13" thru_hole oval (at 0 30.48 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 38 "/Peripherials/GPIO8") (pinfunction "Pin_13") (pintype "passive"))
    (pad "14" thru_hole oval (at 0 33.02 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 39 "/Peripherials/GPIO9") (pinfunction "Pin_14") (pintype "passive"))
    (pad "15" thru_hole oval (at 0 35.56 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 40 "/Peripherials/GPIO10") (pinfunction "Pin_15") (pintype "passive"))
    (pad "16" thru_hole oval (at 0 38.1 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 41 "/Peripherials/GPIO11") (pinfunction "Pin_16") (pintype "passive"))
    (pad "17" thru_hole oval (at 0 40.64 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 42 "/Peripherials/GPIO12") (pinfunction "Pin_17") (pintype "passive"))
    (pad "18" thru_hole oval (at 0 43.18 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 43 "/Peripherials/GPIO13") (pinfunction "Pin_18") (pintype "passive"))
    (pad "19" thru_hole oval (at 0 45.72 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 44 "/Peripherials/GPIO14") (pinfunction "Pin_19") (pintype "passive"))
    (pad "20" thru_hole oval (at 0 48.26 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 45 "/Peripherials/GPIO15") (pinfunction "Pin_20") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x20_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinHeader_2.54mm:PinHeader_1x20_P2.54mm_Vertical" (layer "F.Cu")
    (at 76.67 160.03816 -90)
    (descr "Through hole straight pin header, 1x20, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x20 2.54mm single row")
    (property "Field2" "")
    (property "Sheetfile" "interface_sch.kicad_sch")
    (property "Sheetname" "Interface")
    (property "ki_description" "Generic connector, single row, 01x20, script generated (kicad-library-utils/schlib/autogen/connector/)")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "J302" (at 3.048 48.514) (layer "F.SilkS"))
    (fp_text value "Conn_01x20" (at 2.794 24.13) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 24.13) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 67 "/Interface/QSPI.SCLK") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 2.54 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 68 "/Interface/QSPI.D0") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 5.08 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 69 "/Interface/QSPI.SS") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole oval (at 0 7.62 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 6 "GNDD") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" thru_hole oval (at 0 10.16 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 70 "/Interface/GPIO0") (pinfunction "Pin_5") (pintype "passive"))
    (pad "6" thru_hole oval (at 0 12.7 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 71 "/Interface/GPIO1") (pinfunction "Pin_6") (pintype "passive"))
    (pad "7" thru_hole oval (at 0 15.24 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 72 "/Interface/GPIO2") (pinfunction "Pin_7") (pintype "passive"))
    (pad "8" thru_hole oval (at 0 17.78 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 73 "/Interface/GPIO3") (pinfunction "Pin_8") (pintype "passive"))
    (pad "9" thru_hole oval (at 0 20.32 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 74 "/Interface/GPIO4") (pinfunction "Pin_9") (pintype "passive"))
    (pad "10" thru_hole oval (at 0 22.86 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 75 "/Interface/GPIO5") (pinfunction "Pin_10") (pintype "passive"))
    (pad "11" thru_hole oval (at 0 25.4 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 76 "/Interface/GPIO6") (pinfunction "Pin_11") (pintype "passive"))
    (pad "12" thru_hole oval (at 0 27.94 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 77 "/Interface/GPIO7") (pinfunction "Pin_12") (pintype "passive"))
    (pad "13" thru_hole oval (at 0 30.48 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 78 "/Interface/GPIO8") (pinfunction "Pin_13") (pintype "passive"))
    (pad "14" thru_hole oval (at 0 33.02 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 79 "/Interface/GPIO9") (pinfunction "Pin_14") (pintype "passive"))
    (pad "15" thru_hole oval (at 0 35.56 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 80 "/Interface/GPIO10") (pinfunction "Pin_15") (pintype "passive"))
    (pad "16" thru_hole oval (at 0 38.1 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 81 "/Interface/GPIO11") (pinfunction "Pin_16") (pintype "passive"))
    (pad "17" thru_hole oval (at 0 40.64 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 82 "/Interface/GPIO12") (pinfunction "Pin_17") (pintype "passive"))
    (pad "18" thru_hole oval (at 0 43.18 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 83 "/Interface/GPIO13") (pinfunction "Pin_18") (pintype "passive"))
    (pad "19" thru_hole oval (at 0 45.72 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 84 "/Interface/GPIO14") (pinfunction "Pin_19") (pintype "passive"))
    (pad "20" thru_hole oval (at 0 48.26 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 85 "/Interface/GPIO15") (pinfunction "Pin_20") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x20_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinHeader_2.54mm:PinHeader_1x20_P2.54mm_Vertical" (layer "F.Cu")
    (at 28.41 152.81816 90)
    (descr "Through hole straight pin header, 1x20, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x20 2.54mm single row")
    (property "Field2" "")
    (property "Sheetfile" "peripherials_sch.kicad_sch")
    (property "Sheetname" "Peripherials")
    (property "ki_description" "Generic connector, single row, 01x20, script generated (kicad-library-utils/schlib/autogen/connector/)")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "J201" (at 3.048 -0.254) (layer "F.SilkS"))
    (fp_text value "Conn_01x20" (at -2.794 24.13) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 24.13) (layer "F.Fab"))
    (pad "1" thru_hole roundrect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask") (roundrect_rratio 0.25)
      (net 13 "/Peripherials/GPIO16") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 14 "/Peripherials/GPIO17") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 15 "/Peripherials/GPIO18") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole oval (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 16 "/Peripherials/GPIO19") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" thru_hole oval (at 0 10.16 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 17 "/Peripherials/GPIO20") (pinfunction "Pin_5") (pintype "passive"))
    (pad "6" thru_hole oval (at 0 12.7 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 18 "/Peripherials/GPIO21") (pinfunction "Pin_6") (pintype "passive"))
    (pad "7" thru_hole oval (at 0 15.24 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 19 "/Peripherials/GPIO22") (pinfunction "Pin_7") (pintype "passive"))
    (pad "8" thru_hole oval (at 0 17.78 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 20 "/Peripherials/GPIO23") (pinfunction "Pin_8") (pintype "passive"))
    (pad "9" thru_hole oval (at 0 20.32 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 21 "/Peripherials/GPIO24") (pinfunction "Pin_9") (pintype "passive"))
    (pad "10" thru_hole oval (at 0 22.86 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 22 "/Peripherials/GPIO25") (pinfunction "Pin_10") (pintype "passive"))
    (pad "11" thru_hole oval (at 0 25.4 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 23 "/Peripherials/GPIO26") (pinfunction "Pin_11") (pintype "passive"))
    (pad "12" thru_hole oval (at 0 27.94 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 24 "/Peripherials/GPIO27") (pinfunction "Pin_12") (pintype "passive"))
    (pad "13" thru_hole oval (at 0 30.48 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 25 "/Peripherials/GPIO28") (pinfunction "Pin_13") (pintype "passive"))
    (pad "14" thru_hole oval (at 0 33.02 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 26 "/Peripherials/GPIO29") (pinfunction "Pin_14") (pintype "passive"))
    (pad "15" thru_hole oval (at 0 35.56 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 1 "IOVDD") (pinfunction "Pin_15") (pintype "passive"))
    (pad "16" thru_hole oval (at 0 38.1 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 10 "ADC_AVDD") (pinfunction "Pin_16") (pintype "passive"))
    (pad "17" thru_hole oval (at 0 40.64 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 6 "GNDD") (pinfunction "Pin_17") (pintype "passive"))
    (pad "18" thru_hole oval (at 0 43.18 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 1 "IOVDD") (pinfunction "Pin_18") (pintype "passive"))
    (pad "19" thru_hole oval (at 0 45.72 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 11 "VREG_IN") (pinfunction "Pin_19") (pintype "passive"))
    (pad "20" thru_hole oval (at 0 48.26 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 12 "VBUS") (pinfunction "Pin_20") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x20_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinHeader_2.54mm:PinHeader_1x03_P2.54mm_Vertical" (layer "F.Cu")
    (at 61.43 141.38816 90)
    (descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x03 2.54mm single row")
    (property "Field2" "")
    (property "Sheetfile" "peripherials_sch.kicad_sch")
    (property "Sheetname" "Peripherials")
    (property "ki_description" "Generic connector, single row, 01x03, script generated (kicad-library-utils/schlib/autogen/connector/)")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "J203" (at -0.889 -2.794) (layer "F.SilkS"))
    (fp_text value "Conn_01x03" (at -3.048 2.54) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 2.54) (layer "F.Fab"))
    (pad "1" thru_hole roundrect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask") (roundrect_rratio 0.25)
      (net 46 "/Peripherials/QSPI.D1") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 47 "/Peripherials/QSPI.D2") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 48 "/Peripherials/QSPI.D3") (pinfunction "Pin_3") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x03_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinHeader_2.54mm:PinHeader_1x20_P2.54mm_Vertical" (layer "F.Cu")
    (at 28.41 177.81816 90)
    (descr "Through hole straight pin header, 1x20, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x20 2.54mm single row")
    (property "Field2" "")
    (property "Sheetfile" "interface_sch.kicad_sch")
    (property "Sheetname" "Interface")
    (property "ki_description" "Generic connector, single row, 01x20, script generated (kicad-library-utils/schlib/autogen/connector/)")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "J301" (at 3.048 -0.254 180) (layer "F.SilkS"))
    (fp_text value "Conn_01x20" (at -2.794 24.13) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 24.13) (layer "F.Fab"))
    (pad "1" thru_hole roundrect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask") (roundrect_rratio 0.25)
      (net 53 "/Interface/GPIO16") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 54 "/Interface/GPIO17") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 55 "/Interface/GPIO18") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole oval (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 56 "/Interface/GPIO19") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" thru_hole oval (at 0 10.16 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 57 "/Interface/GPIO20") (pinfunction "Pin_5") (pintype "passive"))
    (pad "6" thru_hole oval (at 0 12.7 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 58 "/Interface/GPIO21") (pinfunction "Pin_6") (pintype "passive"))
    (pad "7" thru_hole oval (at 0 15.24 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 59 "/Interface/GPIO22") (pinfunction "Pin_7") (pintype "passive"))
    (pad "8" thru_hole oval (at 0 17.78 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 60 "/Interface/GPIO23") (pinfunction "Pin_8") (pintype "passive"))
    (pad "9" thru_hole oval (at 0 20.32 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 61 "/Interface/GPIO24") (pinfunction "Pin_9") (pintype "passive"))
    (pad "10" thru_hole oval (at 0 22.86 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 62 "/Interface/GPIO25") (pinfunction "Pin_10") (pintype "passive"))
    (pad "11" thru_hole oval (at 0 25.4 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 63 "/Interface/GPIO26") (pinfunction "Pin_11") (pintype "passive"))
    (pad "12" thru_hole oval (at 0 27.94 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 64 "/Interface/GPIO27") (pinfunction "Pin_12") (pintype "passive"))
    (pad "13" thru_hole oval (at 0 30.48 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 65 "/Interface/GPIO28") (pinfunction "Pin_13") (pintype "passive"))
    (pad "14" thru_hole oval (at 0 33.02 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 66 "/Interface/GPIO29") (pinfunction "Pin_14") (pintype "passive"))
    (pad "15" thru_hole oval (at 0 35.56 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 1 "IOVDD") (pinfunction "Pin_15") (pintype "passive"))
    (pad "16" thru_hole oval (at 0 38.1 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 10 "ADC_AVDD") (pinfunction "Pin_16") (pintype "passive"))
    (pad "17" thru_hole oval (at 0 40.64 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 6 "GNDD") (pinfunction "Pin_17") (pintype "passive"))
    (pad "18" thru_hole oval (at 0 43.18 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 1 "IOVDD") (pinfunction "Pin_18") (pintype "passive"))
    (pad "19" thru_hole oval (at 0 45.72 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 11 "VREG_IN") (pinfunction "Pin_19") (pintype "passive"))
    (pad "20" thru_hole oval (at 0 48.26 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 12 "VBUS") (pinfunction "Pin_20") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x20_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0402_1005Metric" (layer "F.Cu")
    (at 70.4 166.38816 -90)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Field2" "")
    (property "Sheetfile" "interface_sch.kicad_sch")
    (property "Sheetname" "Interface")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R303" (at -1.96 -0.1 90) (layer "F.SilkS"))
    (fp_text value "0R" (at -2 -0.03 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.51 0 270) (size 0.54 0.64) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 6 "GNDD") (pintype "passive"))
    (pad "2" smd roundrect (at 0.51 0 270) (size 0.54 0.64) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 91 "Net-(X301-ID)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MCU_RaspberryPi_and_Boards:RP2040-QFN-56" (layer "F.Cu")
    (at 50 168.92816 -90)
    (descr "QFN, 56 Pin (http://www.cypress.com/file/416486/download#page=40), generated with kicad-footprint-generator ipc_dfn_qfn_generator.py")
    (tags "QFN DFN_QFN")
    (property "Field2" "")
    (property "Sheetfile" "interface_sch.kicad_sch")
    (property "Sheetname" "Interface")
    (zone_connect 2)
    (attr smd)
    (fp_text reference "U301" (at -4.2 -4.82 180) (layer "F.SilkS"))
    (fp_text value "RP2040" (at -3.4 5.02 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "" smd roundrect (at -0.6375 -0.6375 270) (size 1.084435 1.084435) (layers "F.Paste") (roundrect_rratio 0.230535))
    (pad "" smd roundrect (at -0.6375 0.6375 270) (size 1.084435 1.084435) (layers "F.Paste") (roundrect_rratio 0.230535))
    (pad "" smd roundrect (at 0.6375 -0.6375 270) (size 1.084435 1.084435) (layers "F.Paste") (roundrect_rratio 0.230535))
    (pad "" smd roundrect (at 0.6375 0.6375 270) (size 1.084435 1.084435) (layers "F.Paste") (roundrect_rratio 0.230535))
    (pad "1" smd roundrect (at -3.4375 -2.6 270) (size 0.875 0.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "IOVDD") (pinfunction "IOVDD") (pintype "power_in"))
    (pad "2" smd roundrect (at -3.4375 -2.2 270) (size 0.875 0.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 70 "/Interface/GPIO0") (pinfunction "GPIO0") (pintype "bidirectional"))
    (pad "3" smd roundrect (at -3.4375 -1.8 270) (size 0.875 0.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 71 "/Interface/GPIO1") (pinfunction "GPIO1") (pintype "bidirectional"))
    (pad "4" smd roundrect (at -3.4375 -1.4 270) (size 0.875 0.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 72 "/Interface/GPIO2") (pinfunction "GPIO2") (pintype "bidirectional"))
    (pad "5" smd roundrect (at -3.4375 -1 270) (size 0.875 0.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 73 "/Interface/GPIO3") (pinfunction "GPIO3") (pintype "bidirectional"))
    (pad "6" smd roundrect (at -3.4375 -0.6 270) (size 0.875 0.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 74 "/Interface/GPIO4") (pinfunction "GPIO4") (pintype "bidirectional"))
    (pad "7" smd roundrect (at -3.4375 -0.2 270) (size 0.875 0.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 75 "/Interface/GPIO5") (pinfunction "GPIO5") (pintype "bidirectional"))
    (pad "8" smd roundrect (at -3.4375 0.2 270) (size 0.875 0.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 76 "/Interface/GPIO6") (pinfunction "GPIO6") (pintype "bidirectional"))
    (pad "9" smd roundrect (at -3.4375 0.6 270) (size 0.875 0.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 77 "/Interface/GPIO7") (pinfunction "GPIO7") (pintype "bidirectional"))
    (pad "10" smd roundrect (at -3.4375 1 270) (size 0.875 0.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "IOVDD") (pinfunction "IOVDD") (pintype "power_in"))
    (pad "11" smd roundrect (at -3.4375 1.4 270) (size 0.875 0.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 78 "/Interface/GPIO8") (pinfunction "GPIO8") (pintype "bidirectional"))
    (pad "12" smd roundrect (at -3.4375 1.8 270) (size 0.875 0.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 79 "/Interface/GPIO9") (pinfunction "GPIO9") (pintype "bidirectional"))
    (pad "13" smd roundrect (at -3.4375 2.2 270) (size 0.875 0.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 80 "/Interface/GPIO10") (pinfunction "GPIO10") (pintype "bidirectional"))
    (pad "14" smd roundrect (at -3.4375 2.6 270) (size 0.875 0.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 81 "/Interface/GPIO11") (pinfunction "GPIO11") (pintype "bidirectional"))
    (pad "15" smd roundrect (at -2.6 3.4375 270) (size 0.2 0.875) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 82 "/Interface/GPIO12") (pinfunction "GPIO12") (pintype "bidirectional"))
    (pad "16" smd roundrect (at -2.2 3.4375 270) (size 0.2 0.875) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 83 "/Interface/GPIO13") (pinfunction "GPIO13") (pintype "bidirectional"))
    (pad "17" smd roundrect (at -1.8 3.4375 270) (size 0.2 0.875) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 84 "/Interface/GPIO14") (pinfunction "GPIO14") (pintype "bidirectional"))
    (pad "18" smd roundrect (at -1.4 3.4375 270) (size 0.2 0.875) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 85 "/Interface/GPIO15") (pinfunction "GPIO15") (pintype "bidirectional"))
    (pad "19" smd roundrect (at -1 3.4375 270) (size 0.2 0.875) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 6 "GNDD") (pinfunction "TESTEN") (pintype "passive"))
    (pad "20" smd roundrect (at -0.6 3.4375 270) (size 0.2 0.875) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "XIN") (pinfunction "XIN") (pintype "input"))
    (pad "21" smd roundrect (at -0.2 3.4375 270) (size 0.2 0.875) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 92 "unconnected-(U301-XOUT-Pad21)") (pinfunction "XOUT") (pintype "passive"))
    (pad "22" smd roundrect (at 0.2 3.4375 270) (size 0.2 0.875) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "IOVDD") (pinfunction "IOVDD") (pintype "power_in"))
    (pad "23" smd roundrect (at 0.6 3.4375 270) (size 0.2 0.875) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 7 "DVDD") (pinfunction "DVDD") (pintype "power_in"))
    (pad "24" smd roundrect (at 1 3.4375 270) (size 0.2 0.875) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 3 "SWCLK") (pinfunction "SWCLK") (pintype "output"))
    (pad "25" smd roundrect (at 1.4 3.4375 270) (size 0.2 0.875) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 5 "SWDIO") (pinfunction "SWD") (pintype "bidirectional"))
    (pad "26" smd roundrect (at 1.8 3.4375 270) (size 0.2 0.875) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "RUN") (pinfunction "RUN") (pintype "input"))
    (pad "27" smd roundrect (at 2.2 3.4375 270) (size 0.2 0.875) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 53 "/Interface/GPIO16") (pinfunction "GPIO16") (pintype "bidirectional"))
    (pad "28" smd roundrect (at 2.6 3.4375 270) (size 0.2 0.875) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 54 "/Interface/GPIO17") (pinfunction "GPIO17") (pintype "bidirectional"))
    (pad "29" smd roundrect (at 3.4375 2.6 270) (size 0.875 0.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 55 "/Interface/GPIO18") (pinfunction "GPIO18") (pintype "bidirectional"))
    (pad "30" smd roundrect (at 3.4375 2.2 270) (size 0.875 0.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 56 "/Interface/GPIO19") (pinfunction "GPIO19") (pintype "bidirectional"))
    (pad "31" smd roundrect (at 3.4375 1.8 270) (size 0.875 0.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 57 "/Interface/GPIO20") (pinfunction "GPIO20") (pintype "bidirectional"))
    (pad "32" smd roundrect (at 3.4375 1.4 270) (size 0.875 0.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 58 "/Interface/GPIO21") (pinfunction "GPIO21") (pintype "bidirectional"))
    (pad "33" smd roundrect (at 3.4375 1 270) (size 0.875 0.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "IOVDD") (pinfunction "IOVDD") (pintype "power_in"))
    (pad "34" smd roundrect (at 3.4375 0.6 270) (size 0.875 0.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 59 "/Interface/GPIO22") (pinfunction "GPIO22") (pintype "bidirectional"))
    (pad "35" smd roundrect (at 3.4375 0.2 270) (size 0.875 0.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 60 "/Interface/GPIO23") (pinfunction "GPIO23") (pintype "bidirectional"))
    (pad "36" smd roundrect (at 3.4375 -0.2 270) (size 0.875 0.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 61 "/Interface/GPIO24") (pinfunction "GPIO24") (pintype "bidirectional"))
    (pad "37" smd roundrect (at 3.4375 -0.6 270) (size 0.875 0.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 62 "/Interface/GPIO25") (pinfunction "GPIO25") (pintype "bidirectional"))
    (pad "38" smd roundrect (at 3.4375 -1 270) (size 0.875 0.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 63 "/Interface/GPIO26") (pinfunction "GPIO26_ADC0") (pintype "bidirectional"))
    (pad "39" smd roundrect (at 3.4375 -1.4 270) (size 0.875 0.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 64 "/Interface/GPIO27") (pinfunction "GPIO27_ADC1") (pintype "bidirectional"))
    (pad "40" smd roundrect (at 3.4375 -1.8 270) (size 0.875 0.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 65 "/Interface/GPIO28") (pinfunction "GPIO28_ADC2") (pintype "bidirectional"))
    (pad "41" smd roundrect (at 3.4375 -2.2 270) (size 0.875 0.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 66 "/Interface/GPIO29") (pinfunction "GPIO29_ADC3") (pintype "bidirectional"))
    (pad "42" smd roundrect (at 3.4375 -2.6 270) (size 0.875 0.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "IOVDD") (pinfunction "IOVDD") (pintype "power_in"))
    (pad "43" smd roundrect (at 2.6 -3.4375 270) (size 0.2 0.875) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 10 "ADC_AVDD") (pinfunction "ADC_AVDD") (pintype "power_in"))
    (pad "44" smd roundrect (at 2.2 -3.4375 270) (size 0.2 0.875) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 11 "VREG_IN") (pinfunction "VREG_IN") (pintype "power_in"))
    (pad "45" smd roundrect (at 1.8 -3.4375 270) (size 0.2 0.875) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 7 "DVDD") (pinfunction "VREG_VOUT") (pintype "power_out"))
    (pad "46" smd roundrect (at 1.4 -3.4375 270) (size 0.2 0.875) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 90 "Net-(U301-USB_DM)") (pinfunction "USB_DM") (pintype "bidirectional"))
    (pad "47" smd roundrect (at 1 -3.4375 270) (size 0.2 0.875) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 89 "Net-(U301-USB_DP)") (pinfunction "USB_DP") (pintype "bidirectional"))
    (pad "48" smd roundrect (at 0.6 -3.4375 270) (size 0.2 0.875) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "IOVDD") (pinfunction "USB_VDD") (pintype "power_in"))
    (pad "49" smd roundrect (at 0.2 -3.4375 270) (size 0.2 0.875) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "IOVDD") (pinfunction "IOVDD") (pintype "power_in"))
    (pad "50" smd roundrect (at -0.2 -3.4375 270) (size 0.2 0.875) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 7 "DVDD") (pinfunction "DVDD") (pintype "power_in"))
    (pad "51" smd roundrect (at -0.6 -3.4375 270) (size 0.2 0.875) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 88 "/Interface/QSPI.D3") (pinfunction "QSPI_SD3") (pintype "bidirectional"))
    (pad "52" smd roundrect (at -1 -3.4375 270) (size 0.2 0.875) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 67 "/Interface/QSPI.SCLK") (pinfunction "QSPI_SCLK") (pintype "output"))
    (pad "53" smd roundrect (at -1.4 -3.4375 270) (size 0.2 0.875) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 68 "/Interface/QSPI.D0") (pinfunction "QSPI_SD0") (pintype "bidirectional"))
    (pad "54" smd roundrect (at -1.8 -3.4375 270) (size 0.2 0.875) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 87 "/Interface/QSPI.D2") (pinfunction "QSPI_SD2") (pintype "bidirectional"))
    (pad "55" smd roundrect (at -2.2 -3.4375 270) (size 0.2 0.875) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 86 "/Interface/QSPI.D1") (pinfunction "QSPI_SD1") (pintype "bidirectional"))
    (pad "56" smd roundrect (at -2.6 -3.4375 270) (size 0.2 0.875) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 69 "/Interface/QSPI.SS") (pinfunction "QSPI_SS") (pintype "bidirectional"))
    (pad "57" thru_hole circle (at -1.275 -1.275 270) (size 0.6 0.6) (drill 0.35) (layers "*.Cu")
      (net 6 "GNDD") (pinfunction "GND") (pintype "power_in"))
    (pad "57" thru_hole circle (at -1.275 0 270) (size 0.6 0.6) (drill 0.35) (layers "*.Cu")
      (net 6 "GNDD") (pinfunction "GND") (pintype "power_in"))
    (pad "57" thru_hole circle (at -1.275 1.275 270) (size 0.6 0.6) (drill 0.35) (layers "*.Cu")
      (net 6 "GNDD") (pinfunction "GND") (pintype "power_in"))
    (pad "57" thru_hole circle (at 0 -1.275 270) (size 0.6 0.6) (drill 0.35) (layers "*.Cu")
      (net 6 "GNDD") (pinfunction "GND") (pintype "power_in"))
    (pad "57" thru_hole circle (at 0 0 270) (size 0.6 0.6) (drill 0.35) (layers "*.Cu")
      (net 6 "GNDD") (pinfunction "GND") (pintype "power_in"))
    (pad "57" smd roundrect (at 0 0 270) (size 3.2 3.2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.045)
      (net 6 "GNDD") (pinfunction "GND") (pintype "power_in"))
    (pad "57" thru_hole circle (at 0 1.275 270) (size 0.6 0.6) (drill 0.35) (layers "*.Cu")
      (net 6 "GNDD") (pinfunction "GND") (pintype "power_in"))
    (pad "57" thru_hole circle (at 1.275 -1.275 270) (size 0.6 0.6) (drill 0.35) (layers "*.Cu")
      (net 6 "GNDD") (pinfunction "GND") (pintype "power_in"))
    (pad "57" thru_hole circle (at 1.275 0 270) (size 0.6 0.6) (drill 0.35) (layers "*.Cu")
      (net 6 "GNDD") (pinfunction "GND") (pintype "power_in"))
    (pad "57" thru_hole circle (at 1.275 1.275 270) (size 0.6 0.6) (drill 0.35) (layers "*.Cu")
      (net 6 "GNDD") (pinfunction "GND") (pintype "power_in"))
    (model "${KISYS3DMOD}/Package_DFN_QFN.3dshapes/QFN-56-1EP_7x7mm_P0.4mm_EP5.6x5.6mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model "RP2040_QFN56_04.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )
  (footprint "Connector_PinHeader_2.54mm:PinHeader_1x03_P2.54mm_Vertical" (layer "F.Cu")
    (at 28.41 166.38816)
    (descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x03 2.54mm single row")
    (property "Field2" "")
    (property "Sheetfile" "interface_sch.kicad_sch")
    (property "Sheetname" "Interface")
    (property "ki_description" "Generic connector, single row, 01x03, script generated (kicad-library-utils/schlib/autogen/connector/)")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "J304" (at 2.921 5.08) (layer "F.SilkS"))
    (fp_text value "Conn_01x03" (at -2.794 2.54 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 2.54 90) (layer "F.Fab"))
    (pad "1" thru_hole roundrect (at 0 0) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask") (roundrect_rratio 0.25)
      (net 3 "SWCLK") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 6 "GNDD") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 5 "SWDIO") (pinfunction "Pin_3") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x03_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinHeader_2.54mm:PinHeader_1x03_P2.54mm_Vertical" (layer "F.Cu")
    (at 33.49 166.38816 90)
    (descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x03 2.54mm single row")
    (property "Field2" "")
    (property "Sheetfile" "interface_sch.kicad_sch")
    (property "Sheetname" "Interface")
    (property "ki_description" "Generic connector, single row, 01x03, script generated (kicad-library-utils/schlib/autogen/connector/)")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "J305" (at -0.889 7.874 180) (layer "F.SilkS"))
    (fp_text value "Conn_01x03" (at -3.048 2.54 180) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 2.54) (layer "F.Fab"))
    (pad "1" thru_hole roundrect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask") (roundrect_rratio 0.25)
      (net 2 "XIN") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 6 "GNDD") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 4 "RUN") (pinfunction "Pin_3") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x03_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0402_1005Metric" (layer "F.Cu")
    (at 57.2 169.62816)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Field2" "")
    (property "Sheetfile" "interface_sch.kicad_sch")
    (property "Sheetname" "Interface")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R301" (at 2.4 -0.4) (layer "F.SilkS"))
    (fp_text value "27R" (at 0 -1.23) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.51 0) (size 0.54 0.64) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 89 "Net-(U301-USB_DP)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.51 0) (size 0.54 0.64) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 9 "DP") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinHeader_2.54mm:PinHeader_1x03_P2.54mm_Vertical" (layer "F.Cu")
    (at 28.41 141.38816)
    (descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x03 2.54mm single row")
    (property "Field2" "")
    (property "Sheetfile" "peripherials_sch.kicad_sch")
    (property "Sheetname" "Peripherials")
    (property "ki_description" "Generic connector, single row, 01x03, script generated (kicad-library-utils/schlib/autogen/connector/)")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "J204" (at 2.921 5.08) (layer "F.SilkS"))
    (fp_text value "Conn_01x03" (at -2.794 2.54 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 2.54 90) (layer "F.Fab"))
    (pad "1" thru_hole roundrect (at 0 0) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask") (roundrect_rratio 0.25)
      (net 3 "SWCLK") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 6 "GNDD") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 5 "SWDIO") (pinfunction "Pin_3") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x03_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_USB:USB_C_Receptacle_GCT_USB4085" (layer "F.Cu")
    (at 115.5 111.85316 -90)
    (descr "USB 2.0 Type C Receptacle, https://gct.co/Files/Drawings/USB4085.pdf")
    (tags "USB Type-C Receptacle Through-hole Right angle")
    (property "Sheetfile" "AXIOM_Remote.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "USB 2.0-only Type-C Receptacle connector")
    (property "ki_keywords" "usb universal serial bus type-C USB2.0")
    (attr through_hole)
    (fp_text reference "X3" (at 2.975 -1.8 90) (layer "F.SilkS"))
    (fp_text value "USB_C_Receptacle_GCT_USB4085" (at 2.975 9.925 90) (layer "F.Fab"))
    (fp_text user "PCB Edge" (at 2.975 6.1 90) (layer "Dwgs.User"))
    (fp_text user "${REFERENCE}" (at 2.975 4.025 90) (layer "F.Fab"))
    (pad "A1" thru_hole circle (at 0 0 270) (size 0.7 0.7) (drill 0.4) (layers "*.Cu" "*.Mask")
      (net 113 "Net-(X3-GND-PadA1)") (pinfunction "GND") (pintype "passive"))
    (pad "A4" thru_hole circle (at 0.85 0 270) (size 0.7 0.7) (drill 0.4) (layers "*.Cu" "*.Mask")
      (net 114 "Net-(X3-VBUS-PadA4)") (pinfunction "VBUS") (pintype "passive"))
    (pad "A5" thru_hole circle (at 1.7 0 270) (size 0.7 0.7) (drill 0.4) (layers "*.Cu" "*.Mask")
      (net 115 "unconnected-(X3-CC1-PadA5)") (pinfunction "CC1") (pintype "bidirectional"))
    (pad "A6" thru_hole circle (at 2.55 0 270) (size 0.7 0.7) (drill 0.4) (layers "*.Cu" "*.Mask")
      (net 116 "unconnected-(X3-D+-PadA6)") (pinfunction "D+") (pintype "bidirectional"))
    (pad "A7" thru_hole circle (at 3.4 0 270) (size 0.7 0.7) (drill 0.4) (layers "*.Cu" "*.Mask")
      (net 117 "unconnected-(X3-D--PadA7)") (pinfunction "D-") (pintype "bidirectional"))
    (pad "A8" thru_hole circle (at 4.25 0 270) (size 0.7 0.7) (drill 0.4) (layers "*.Cu" "*.Mask")
      (net 118 "unconnected-(X3-SBU1-PadA8)") (pinfunction "SBU1") (pintype "bidirectional"))
    (pad "A9" thru_hole circle (at 5.1 0 270) (size 0.7 0.7) (drill 0.4) (layers "*.Cu" "*.Mask")
      (net 114 "Net-(X3-VBUS-PadA4)") (pinfunction "VBUS") (pintype "passive"))
    (pad "A12" thru_hole circle (at 5.95 0 270) (size 0.7 0.7) (drill 0.4) (layers "*.Cu" "*.Mask")
      (net 113 "Net-(X3-GND-PadA1)") (pinfunction "GND") (pintype "passive"))
    (pad "B1" thru_hole circle (at 5.95 1.35 270) (size 0.7 0.7) (drill 0.4) (layers "*.Cu" "*.Mask")
      (net 113 "Net-(X3-GND-PadA1)") (pinfunction "GND") (pintype "passive"))
    (pad "B4" thru_hole circle (at 5.1 1.35 270) (size 0.7 0.7) (drill 0.4) (layers "*.Cu" "*.Mask")
      (net 114 "Net-(X3-VBUS-PadA4)") (pinfunction "VBUS") (pintype "passive"))
    (pad "B5" thru_hole circle (at 4.25 1.35 270) (size 0.7 0.7) (drill 0.4) (layers "*.Cu" "*.Mask")
      (net 119 "unconnected-(X3-CC2-PadB5)") (pinfunction "CC2") (pintype "bidirectional"))
    (pad "B6" thru_hole circle (at 3.4 1.35 270) (size 0.7 0.7) (drill 0.4) (layers "*.Cu" "*.Mask")
      (net 120 "unconnected-(X3-D+-PadB6)") (pinfunction "D+") (pintype "bidirectional"))
    (pad "B7" thru_hole circle (at 2.55 1.35 270) (size 0.7 0.7) (drill 0.4) (layers "*.Cu" "*.Mask")
      (net 121 "unconnected-(X3-D--PadB7)") (pinfunction "D-") (pintype "bidirectional"))
    (pad "B8" thru_hole circle (at 1.7 1.35 270) (size 0.7 0.7) (drill 0.4) (layers "*.Cu" "*.Mask")
      (net 122 "unconnected-(X3-SBU2-PadB8)") (pinfunction "SBU2") (pintype "bidirectional"))
    (pad "B9" thru_hole circle (at 0.85 1.35 270) (size 0.7 0.7) (drill 0.4) (layers "*.Cu" "*.Mask")
      (net 114 "Net-(X3-VBUS-PadA4)") (pinfunction "VBUS") (pintype "passive"))
    (pad "B12" thru_hole circle (at 0 1.35 270) (size 0.7 0.7) (drill 0.4) (layers "*.Cu" "*.Mask")
      (net 113 "Net-(X3-GND-PadA1)") (pinfunction "GND") (pintype "passive"))
    (pad "S1" thru_hole oval (at -1.35 0.98 270) (size 0.9 2.4) (drill oval 0.6 2.1) (layers "*.Cu" "*.Mask")
      (net 123 "unconnected-(X3-SHIELD-PadS1)") (pinfunction "SHIELD") (pintype "passive"))
    (pad "S1" thru_hole oval (at -1.35 4.36 270) (size 0.9 1.7) (drill oval 0.6 1.4) (layers "*.Cu" "*.Mask")
      (net 123 "unconnected-(X3-SHIELD-PadS1)") (pinfunction "SHIELD") (pintype "passive"))
    (pad "S1" thru_hole oval (at 7.3 0.98 270) (size 0.9 2.4) (drill oval 0.6 2.1) (layers "*.Cu" "*.Mask")
      (net 123 "unconnected-(X3-SHIELD-PadS1)") (pinfunction "SHIELD") (pintype "passive"))
    (pad "S1" thru_hole oval (at 7.3 4.36 270) (size 0.9 1.7) (drill oval 0.6 1.4) (layers "*.Cu" "*.Mask")
      (net 123 "unconnected-(X3-SHIELD-PadS1)") (pinfunction "SHIELD") (pintype "passive"))
    (model "Molex_213716-0001/213716-0001.stp"
      (offset (xyz 3 -3.6 1))
      (scale (xyz 1 1 1))
      (rotate (xyz 90 0 180))
    )
  )
  (footprint "IPT1-105-01-XX-D-RA:IPT1-105-01-XX-D-RA" (layer "F.Cu")
    (at 223 68.57816 90)
    (descr "0.100\" DOUBLE ROW SHROUDED TERMINAL ASSEMBLY,10PINS.")
    (property "Sheetfile" "AXIOM_Remote.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "X1" (at -0.127 -12.065 90) (layer "F.SilkS"))
    (fp_text value "IPT1-105-01-XX-D-RA" (at 0 1 90) (layer "F.Fab"))
    (fp_text user "2" (at -7.112 -10.16 90) (layer "F.SilkS"))
    (fp_text user "1" (at -7.112 -7.62 90) (layer "F.SilkS"))
    (pad "1" thru_hole circle (at -5.08 -7.874 90) (size 1.524 1.524) (drill 1.016) (layers "*.Cu" "*.Mask")
      (net 93 "unconnected-(X1-Pad1)") (pinfunction "1") (pintype "bidirectional") (solder_mask_margin 0.102))
    (pad "2" thru_hole circle (at -5.08 -10.414 90) (size 1.524 1.524) (drill 1.016) (layers "*.Cu" "*.Mask")
      (net 94 "unconnected-(X1-Pad2)") (pinfunction "2") (pintype "bidirectional") (solder_mask_margin 0.102))
    (pad "3" thru_hole circle (at -2.54 -7.874 90) (size 1.524 1.524) (drill 1.016) (layers "*.Cu" "*.Mask")
      (net 95 "unconnected-(X1-Pad3)") (pinfunction "3") (pintype "bidirectional") (solder_mask_margin 0.102))
    (pad "4" thru_hole circle (at -2.54 -10.414 90) (size 1.524 1.524) (drill 1.016) (layers "*.Cu" "*.Mask")
      (net 96 "unconnected-(X1-Pad4)") (pinfunction "4") (pintype "bidirectional") (solder_mask_margin 0.102))
    (pad "5" thru_hole circle (at 0 -7.874 90) (size 1.524 1.524) (drill 1.016) (layers "*.Cu" "*.Mask")
      (net 97 "unconnected-(X1-Pad5)") (pinfunction "5") (pintype "bidirectional") (solder_mask_margin 0.102))
    (pad "6" thru_hole circle (at 0 -10.414 90) (size 1.524 1.524) (drill 1.016) (layers "*.Cu" "*.Mask")
      (net 98 "unconnected-(X1-Pad6)") (pinfunction "6") (pintype "bidirectional") (solder_mask_margin 0.102))
    (pad "7" thru_hole circle (at 2.54 -7.874 90) (size 1.524 1.524) (drill 1.016) (layers "*.Cu" "*.Mask")
      (net 99 "unconnected-(X1-Pad7)") (pinfunction "7") (pintype "bidirectional") (solder_mask_margin 0.102))
    (pad "8" thru_hole circle (at 2.54 -10.414 90) (size 1.524 1.524) (drill 1.016) (layers "*.Cu" "*.Mask")
      (net 100 "unconnected-(X1-Pad8)") (pinfunction "8") (pintype "bidirectional") (solder_mask_margin 0.102))
    (pad "9" thru_hole circle (at 5.08 -7.874 90) (size 1.524 1.524) (drill 1.016) (layers "*.Cu" "*.Mask")
      (net 101 "unconnected-(X1-Pad9)") (pinfunction "9") (pintype "bidirectional") (solder_mask_margin 0.102))
    (pad "10" thru_hole circle (at 5.08 -10.414 90) (size 1.524 1.524) (drill 1.016) (layers "*.Cu" "*.Mask")
      (net 102 "unconnected-(X1-Pad10)") (pinfunction "10") (pintype "bidirectional") (solder_mask_margin 0.102))
    (model "IPT1-105-01-XX-D-RA/IPT1-105-01-XX-D-RA.step"
      (offset (xyz 0 6.5 2.5))
      (scale (xyz 1 1 1))
      (rotate (xyz 180 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0402_1005Metric" (layer "F.Cu")
    (at 57.2 145.62816)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Field2" "")
    (property "Sheetfile" "peripherials_sch.kicad_sch")
    (property "Sheetname" "Peripherials")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R202" (at 2.4 0.4) (layer "F.SilkS"))
    (fp_text value "27R" (at 0 1.17) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.51 0) (size 0.54 0.64) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 50 "Net-(U201-USB_DM)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.51 0) (size 0.54 0.64) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 8 "DM") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_USB:USB_Micro-B_Amphenol_10104110_Horizontal" (layer "F.Cu")
    (at 75.146 168.92816 90)
    (descr "USB Micro-B, horizontal, https://cdn.amphenol-icc.com/media/wysiwyg/files/drawing/10104110.pdf")
    (tags "USB Micro B horizontal")
    (property "Field2" "")
    (property "Sheetfile" "interface_sch.kicad_sch")
    (property "Sheetname" "Interface")
    (property "ki_description" "USB Micro Type B connector")
    (property "ki_keywords" "connector USB micro")
    (attr smd)
    (fp_text reference "X301" (at -2.54 -3.556 90) (layer "F.SilkS"))
    (fp_text value "USB_B_Micro" (at 0 5.35 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -0.2 90) (layer "F.Fab"))
    (pad "1" smd rect (at -1.3 -1.55 90) (size 0.4 1.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "VBUS") (pinfunction "VBUS") (pintype "power_out"))
    (pad "2" smd rect (at -0.65 -1.55 90) (size 0.4 1.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 8 "DM") (pinfunction "D-") (pintype "bidirectional"))
    (pad "3" smd rect (at 0 -1.55 90) (size 0.4 1.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 9 "DP") (pinfunction "D+") (pintype "bidirectional"))
    (pad "4" smd rect (at 0.65 -1.55 90) (size 0.4 1.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 91 "Net-(X301-ID)") (pinfunction "ID") (pintype "passive"))
    (pad "5" smd rect (at 1.3 -1.55 90) (size 0.4 1.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 6 "GNDD") (pinfunction "GND") (pintype "power_out"))
    (pad "6" smd rect (at -3.75 1.3 90) (size 2.3 1.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 6 "GNDD") (pinfunction "Shield") (pintype "passive"))
    (pad "6" smd rect (at -1.15 1.3 90) (size 1.8 1.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 6 "GNDD") (pinfunction "Shield") (pintype "passive"))
    (pad "6" smd rect (at 1.15 1.3 90) (size 1.8 1.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 6 "GNDD") (pinfunction "Shield") (pintype "passive"))
    (pad "6" smd rect (at 3.75 1.3 90) (size 2.3 1.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 6 "GNDD") (pinfunction "Shield") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_USB.3dshapes/USB_Micro-B_Amphenol_10104110_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model "Amphenol_10104110.stp"
      (offset (xyz 0 1.27 6.985))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "IPT1-105-01-XX-D-RA:IPT1-105-01-XX-D-RA" (layer "F.Cu")
    (at 223 119.27816 90)
    (descr "0.100\" DOUBLE ROW SHROUDED TERMINAL ASSEMBLY,10PINS.")
    (property "Sheetfile" "AXIOM_Remote.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "X2" (at -0.127 -12.065 90) (layer "F.SilkS"))
    (fp_text value "IPT1-105-01-XX-D-RA" (at 0 1 90) (layer "F.Fab"))
    (fp_text user "1" (at -7.112 -7.62 90) (layer "F.SilkS"))
    (fp_text user "2" (at -7.112 -10.16 90) (layer "F.SilkS"))
    (pad "1" thru_hole circle (at -5.08 -7.874 90) (size 1.524 1.524) (drill 1.016) (layers "*.Cu" "*.Mask")
      (net 103 "unconnected-(X2-Pad1)") (pinfunction "1") (pintype "bidirectional") (solder_mask_margin 0.102))
    (pad "2" thru_hole circle (at -5.08 -10.414 90) (size 1.524 1.524) (drill 1.016) (layers "*.Cu" "*.Mask")
      (net 104 "unconnected-(X2-Pad2)") (pinfunction "2") (pintype "bidirectional") (solder_mask_margin 0.102))
    (pad "3" thru_hole circle (at -2.54 -7.874 90) (size 1.524 1.524) (drill 1.016) (layers "*.Cu" "*.Mask")
      (net 105 "unconnected-(X2-Pad3)") (pinfunction "3") (pintype "bidirectional") (solder_mask_margin 0.102))
    (pad "4" thru_hole circle (at -2.54 -10.414 90) (size 1.524 1.524) (drill 1.016) (layers "*.Cu" "*.Mask")
      (net 106 "unconnected-(X2-Pad4)") (pinfunction "4") (pintype "bidirectional") (solder_mask_margin 0.102))
    (pad "5" thru_hole circle (at 0 -7.874 90) (size 1.524 1.524) (drill 1.016) (layers "*.Cu" "*.Mask")
      (net 107 "unconnected-(X2-Pad5)") (pinfunction "5") (pintype "bidirectional") (solder_mask_margin 0.102))
    (pad "6" thru_hole circle (at 0 -10.414 90) (size 1.524 1.524) (drill 1.016) (layers "*.Cu" "*.Mask")
      (net 108 "unconnected-(X2-Pad6)") (pinfunction "6") (pintype "bidirectional") (solder_mask_margin 0.102))
    (pad "7" thru_hole circle (at 2.54 -7.874 90) (size 1.524 1.524) (drill 1.016) (layers "*.Cu" "*.Mask")
      (net 109 "unconnected-(X2-Pad7)") (pinfunction "7") (pintype "bidirectional") (solder_mask_margin 0.102))
    (pad "8" thru_hole circle (at 2.54 -10.414 90) (size 1.524 1.524) (drill 1.016) (layers "*.Cu" "*.Mask")
      (net 110 "unconnected-(X2-Pad8)") (pinfunction "8") (pintype "bidirectional") (solder_mask_margin 0.102))
    (pad "9" thru_hole circle (at 5.08 -7.874 90) (size 1.524 1.524) (drill 1.016) (layers "*.Cu" "*.Mask")
      (net 111 "unconnected-(X2-Pad9)") (pinfunction "9") (pintype "bidirectional") (solder_mask_margin 0.102))
    (pad "10" thru_hole circle (at 5.08 -10.414 90) (size 1.524 1.524) (drill 1.016) (layers "*.Cu" "*.Mask")
      (net 112 "unconnected-(X2-Pad10)") (pinfunction "10") (pintype "bidirectional") (solder_mask_margin 0.102))
    (model "IPT1-105-01-XX-D-RA/IPT1-105-01-XX-D-RA.step"
      (offset (xyz 0 6.5 2.5))
      (scale (xyz 1 1 1))
      (rotate (xyz 180 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0402_1005Metric" (layer "F.Cu")
    (at 70.4 141.38816 -90)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Field2" "")
    (property "Sheetfile" "peripherials_sch.kicad_sch")
    (property "Sheetname" "Peripherials")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R203" (at -1.96 -0.1 90) (layer "F.SilkS"))
    (fp_text value "0R" (at -2 -0.03 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.51 0 270) (size 0.54 0.64) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 6 "GNDD") (pintype "passive"))
    (pad "2" smd roundrect (at 0.51 0 270) (size 0.54 0.64) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 51 "Net-(X201-ID)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_USB:USB_Micro-B_Amphenol_10104110_Horizontal" (layer "F.Cu")
    (at 75.146 143.92816 90)
    (descr "USB Micro-B, horizontal, https://cdn.amphenol-icc.com/media/wysiwyg/files/drawing/10104110.pdf")
    (tags "USB Micro B horizontal")
    (property "Field2" "")
    (property "Sheetfile" "peripherials_sch.kicad_sch")
    (property "Sheetname" "Peripherials")
    (property "ki_description" "USB Micro Type B connector")
    (property "ki_keywords" "connector USB micro")
    (attr smd)
    (fp_text reference "X201" (at -2.54 -3.556 90) (layer "F.SilkS"))
    (fp_text value "USB_B_Micro" (at 0 5.35 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -0.2 90) (layer "F.Fab"))
    (pad "1" smd rect (at -1.3 -1.55 90) (size 0.4 1.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "VBUS") (pinfunction "VBUS") (pintype "power_out"))
    (pad "2" smd rect (at -0.65 -1.55 90) (size 0.4 1.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 8 "DM") (pinfunction "D-") (pintype "bidirectional"))
    (pad "3" smd rect (at 0 -1.55 90) (size 0.4 1.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 9 "DP") (pinfunction "D+") (pintype "bidirectional"))
    (pad "4" smd rect (at 0.65 -1.55 90) (size 0.4 1.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 51 "Net-(X201-ID)") (pinfunction "ID") (pintype "passive"))
    (pad "5" smd rect (at 1.3 -1.55 90) (size 0.4 1.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 6 "GNDD") (pinfunction "GND") (pintype "power_out"))
    (pad "6" smd rect (at -3.75 1.3 90) (size 2.3 1.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 6 "GNDD") (pinfunction "Shield") (pintype "passive"))
    (pad "6" smd rect (at -1.15 1.3 90) (size 1.8 1.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 6 "GNDD") (pinfunction "Shield") (pintype "passive"))
    (pad "6" smd rect (at 1.15 1.3 90) (size 1.8 1.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 6 "GNDD") (pinfunction "Shield") (pintype "passive"))
    (pad "6" smd rect (at 3.75 1.3 90) (size 2.3 1.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 6 "GNDD") (pinfunction "Shield") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_USB.3dshapes/USB_Micro-B_Amphenol_10104110_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model "Amphenol_10104110.stp"
      (offset (xyz 0 1.27 6.985))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinHeader_2.54mm:PinHeader_1x03_P2.54mm_Vertical" (layer "F.Cu")
    (at 61.43 166.38816 90)
    (descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x03 2.54mm single row")
    (property "Field2" "")
    (property "Sheetfile" "interface_sch.kicad_sch")
    (property "Sheetname" "Interface")
    (property "ki_description" "Generic connector, single row, 01x03, script generated (kicad-library-utils/schlib/autogen/connector/)")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "J303" (at -0.889 -2.794 180) (layer "F.SilkS"))
    (fp_text value "Conn_01x03" (at -3.048 2.54 180) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 2.54) (layer "F.Fab"))
    (pad "1" thru_hole roundrect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask") (roundrect_rratio 0.25)
      (net 86 "/Interface/QSPI.D1") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 87 "/Interface/QSPI.D2") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 88 "/Interface/QSPI.D3") (pinfunction "Pin_3") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x03_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0402_1005Metric" (layer "B.Cu")
    (at 50 163.12816 90)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Field2" "")
    (property "Sheetfile" "interface_sch.kicad_sch")
    (property "Sheetname" "Interface")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C307" (at 0 1.16 90) (layer "B.SilkS"))
    (fp_text value "1u" (at 0 -1.16 90) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.48 0 90) (size 0.56 0.62) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 1 "IOVDD") (pintype "passive"))
    (pad "2" smd roundrect (at 0.48 0 90) (size 0.56 0.62) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 6 "GNDD") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0402_1005Metric" (layer "B.Cu")
    (at 47.6 142.72816 90)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Field2" "")
    (property "Sheetfile" "peripherials_sch.kicad_sch")
    (property "Sheetname" "Peripherials")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C211" (at 0 -1.04 90) (layer "B.SilkS"))
    (fp_text value "100n" (at 0 -1.16 90) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.48 0 90) (size 0.56 0.62) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 7 "DVDD") (pintype "passive"))
    (pad "2" smd roundrect (at 0.48 0 90) (size 0.56 0.62) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 6 "GNDD") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "B.Cu")
    (at 63.97 148.52816 90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Field2" "")
    (property "Sheetfile" "peripherials_sch.kicad_sch")
    (property "Sheetname" "Peripherials")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C208" (at 0 1.43 90) (layer "B.SilkS"))
    (fp_text value "10u" (at 0 -1.43 90) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.775 0 90) (size 0.9 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 1 "IOVDD") (pintype "passive"))
    (pad "2" smd roundrect (at 0.775 0 90) (size 0.9 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 6 "GNDD") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0402_1005Metric" (layer "B.Cu")
    (at 44.2 168.92816 180)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Field2" "")
    (property "Sheetfile" "interface_sch.kicad_sch")
    (property "Sheetname" "Interface")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C303" (at 0 1.16) (layer "B.SilkS"))
    (fp_text value "100n" (at 0 -1.16) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.48 0 180) (size 0.56 0.62) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 1 "IOVDD") (pintype "passive"))
    (pad "2" smd roundrect (at 0.48 0 180) (size 0.56 0.62) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 6 "GNDD") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0402_1005Metric" (layer "B.Cu")
    (at 50 146.80816 -90)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Field2" "")
    (property "Sheetfile" "peripherials_sch.kicad_sch")
    (property "Sheetname" "Peripherials")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C212" (at 0 1.16 90) (layer "B.SilkS"))
    (fp_text value "1u" (at 0 -1.16 90) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.48 0 270) (size 0.56 0.62) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 7 "DVDD") (pintype "passive"))
    (pad "2" smd roundrect (at 0.48 0 270) (size 0.56 0.62) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 6 "GNDD") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0402_1005Metric" (layer "B.Cu")
    (at 50 174.72816 -90)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Field2" "")
    (property "Sheetfile" "interface_sch.kicad_sch")
    (property "Sheetname" "Interface")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C306" (at 0 1.16 90) (layer "B.SilkS"))
    (fp_text value "1u" (at 0 -1.16 90) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.48 0 270) (size 0.56 0.62) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 1 "IOVDD") (pintype "passive"))
    (pad "2" smd roundrect (at 0.48 0 270) (size 0.56 0.62) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 6 "GNDD") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0402_1005Metric" (layer "B.Cu")
    (at 53 163.12816 90)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Field2" "")
    (property "Sheetfile" "interface_sch.kicad_sch")
    (property "Sheetname" "Interface")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C301" (at 0 1.16 90) (layer "B.SilkS"))
    (fp_text value "100n" (at 0 -1.16 90) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.48 0 90) (size 0.56 0.62) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 1 "IOVDD") (pintype "passive"))
    (pad "2" smd roundrect (at 0.48 0 90) (size 0.56 0.62) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 6 "GNDD") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0402_1005Metric" (layer "B.Cu")
    (at 54.6 167.72816 90)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Field2" "")
    (property "Sheetfile" "interface_sch.kicad_sch")
    (property "Sheetname" "Interface")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C309" (at 0 1.16 90) (layer "B.SilkS"))
    (fp_text value "100n" (at 0 -1.16 90) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.48 0 90) (size 0.56 0.62) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 1 "IOVDD") (pintype "passive"))
    (pad "2" smd roundrect (at 0.48 0 90) (size 0.56 0.62) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 6 "GNDD") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "B.Cu")
    (at 63.97 173.52816 90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Field2" "")
    (property "Sheetfile" "interface_sch.kicad_sch")
    (property "Sheetname" "Interface")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C308" (at 0 1.43 90) (layer "B.SilkS"))
    (fp_text value "10u" (at 0 -1.43 90) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.775 0 90) (size 0.9 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 1 "IOVDD") (pintype "passive"))
    (pad "2" smd roundrect (at 0.775 0 90) (size 0.9 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 6 "GNDD") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0402_1005Metric" (layer "B.Cu")
    (at 50 149.72816 -90)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Field2" "")
    (property "Sheetfile" "peripherials_sch.kicad_sch")
    (property "Sheetname" "Peripherials")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C206" (at 0 1.16 90) (layer "B.SilkS"))
    (fp_text value "1u" (at 0 -1.16 90) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.48 0 270) (size 0.56 0.62) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 1 "IOVDD") (pintype "passive"))
    (pad "2" smd roundrect (at 0.48 0 270) (size 0.56 0.62) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 6 "GNDD") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0402_1005Metric" (layer "B.Cu")
    (at 52.4 167.72816 90)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Field2" "")
    (property "Sheetfile" "interface_sch.kicad_sch")
    (property "Sheetname" "Interface")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C310" (at 0 1.16 90) (layer "B.SilkS"))
    (fp_text value "100n" (at 0 -1.16 90) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.48 0 90) (size 0.56 0.62) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 7 "DVDD") (pintype "passive"))
    (pad "2" smd roundrect (at 0.48 0 90) (size 0.56 0.62) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 6 "GNDD") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0402_1005Metric" (layer "B.Cu")
    (at 47 163.12816 90)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Field2" "")
    (property "Sheetfile" "interface_sch.kicad_sch")
    (property "Sheetname" "Interface")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C302" (at 0 1.16 90) (layer "B.SilkS"))
    (fp_text value "100n" (at 0 -1.16 90) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.48 0 90) (size 0.56 0.62) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 1 "IOVDD") (pintype "passive"))
    (pad "2" smd roundrect (at 0.48 0 90) (size 0.56 0.62) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 6 "GNDD") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0402_1005Metric" (layer "B.Cu")
    (at 57.2 146.92816)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Field2" "")
    (property "Sheetfile" "peripherials_sch.kicad_sch")
    (property "Sheetname" "Peripherials")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C214" (at 2.4 0) (layer "B.SilkS"))
    (fp_text value "1u" (at 0 -1.16) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.48 0) (size 0.56 0.62) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 11 "VREG_IN") (pintype "passive"))
    (pad "2" smd roundrect (at 0.48 0) (size 0.56 0.62) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 6 "GNDD") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0402_1005Metric" (layer "B.Cu")
    (at 50 171.80816 -90)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Field2" "")
    (property "Sheetfile" "interface_sch.kicad_sch")
    (property "Sheetname" "Interface")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C312" (at 0 1.16 90) (layer "B.SilkS"))
    (fp_text value "1u" (at 0 -1.16 90) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.48 0 270) (size 0.56 0.62) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 7 "DVDD") (pintype "passive"))
    (pad "2" smd roundrect (at 0.48 0 270) (size 0.56 0.62) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 6 "GNDD") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0402_1005Metric" (layer "B.Cu")
    (at 50 138.12816 90)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Field2" "")
    (property "Sheetfile" "peripherials_sch.kicad_sch")
    (property "Sheetname" "Peripherials")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C207" (at 0 1.16 90) (layer "B.SilkS"))
    (fp_text value "1u" (at 0 -1.16 90) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.48 0 90) (size 0.56 0.62) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 1 "IOVDD") (pintype "passive"))
    (pad "2" smd roundrect (at 0.48 0 90) (size 0.56 0.62) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 6 "GNDD") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0402_1005Metric" (layer "B.Cu")
    (at 47 149.72816 -90)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Field2" "")
    (property "Sheetfile" "peripherials_sch.kicad_sch")
    (property "Sheetname" "Peripherials")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C204" (at 0 1.16 90) (layer "B.SilkS"))
    (fp_text value "100n" (at 0 -1.16 90) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.48 0 270) (size 0.56 0.62) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 1 "IOVDD") (pintype "passive"))
    (pad "2" smd roundrect (at 0.48 0 270) (size 0.56 0.62) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 6 "GNDD") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0402_1005Metric" (layer "B.Cu")
    (at 47 138.12816 90)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Field2" "")
    (property "Sheetfile" "peripherials_sch.kicad_sch")
    (property "Sheetname" "Peripherials")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C202" (at 0 1.16 90) (layer "B.SilkS"))
    (fp_text value "100n" (at 0 -1.16 90) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.48 0 90) (size 0.56 0.62) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 1 "IOVDD") (pintype "passive"))
    (pad "2" smd roundrect (at 0.48 0 90) (size 0.56 0.62) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 6 "GNDD") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0402_1005Metric" (layer "B.Cu")
    (at 47 174.72816 -90)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Field2" "")
    (property "Sheetfile" "interface_sch.kicad_sch")
    (property "Sheetname" "Interface")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C304" (at 0 1.16 90) (layer "B.SilkS"))
    (fp_text value "100n" (at 0 -1.16 90) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.48 0 270) (size 0.56 0.62) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 1 "IOVDD") (pintype "passive"))
    (pad "2" smd roundrect (at 0.48 0 270) (size 0.56 0.62) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 6 "GNDD") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0402_1005Metric" (layer "B.Cu")
    (at 57.2 171.92816)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Field2" "")
    (property "Sheetfile" "interface_sch.kicad_sch")
    (property "Sheetname" "Interface")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C314" (at 2.4 0) (layer "B.SilkS"))
    (fp_text value "1u" (at 0 -1.16) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.48 0) (size 0.56 0.62) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 11 "VREG_IN") (pintype "passive"))
    (pad "2" smd roundrect (at 0.48 0) (size 0.56 0.62) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 6 "GNDD") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0402_1005Metric" (layer "B.Cu")
    (at 54.6 142.72816 90)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Field2" "")
    (property "Sheetfile" "peripherials_sch.kicad_sch")
    (property "Sheetname" "Peripherials")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C209" (at 0 1.16 90) (layer "B.SilkS"))
    (fp_text value "100n" (at 0 -1.16 90) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.48 0 90) (size 0.56 0.62) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 1 "IOVDD") (pintype "passive"))
    (pad "2" smd roundrect (at 0.48 0 90) (size 0.56 0.62) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 6 "GNDD") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0402_1005Metric" (layer "B.Cu")
    (at 53 149.72816 -90)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Field2" "")
    (property "Sheetfile" "peripherials_sch.kicad_sch")
    (property "Sheetname" "Peripherials")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C205" (at 0 1.16 90) (layer "B.SilkS"))
    (fp_text value "100n" (at 0 -1.16 90) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.48 0 270) (size 0.56 0.62) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 1 "IOVDD") (pintype "passive"))
    (pad "2" smd roundrect (at 0.48 0 270) (size 0.56 0.62) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 6 "GNDD") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0402_1005Metric" (layer "B.Cu")
    (at 57.2 173.12816)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Field2" "")
    (property "Sheetfile" "interface_sch.kicad_sch")
    (property "Sheetname" "Interface")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C313" (at 2.4 0) (layer "B.SilkS"))
    (fp_text value "100n" (at 0 -1.16) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.48 0) (size 0.56 0.62) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 10 "ADC_AVDD") (pintype "passive"))
    (pad "2" smd roundrect (at 0.48 0) (size 0.56 0.62) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 6 "GNDD") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0402_1005Metric" (layer "B.Cu")
    (at 47.6 167.72816 90)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Field2" "")
    (property "Sheetfile" "interface_sch.kicad_sch")
    (property "Sheetname" "Interface")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C311" (at 0 -1.04 90) (layer "B.SilkS"))
    (fp_text value "100n" (at 0 -1.16 90) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.48 0 90) (size 0.56 0.62) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 7 "DVDD") (pintype "passive"))
    (pad "2" smd roundrect (at 0.48 0 90) (size 0.56 0.62) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 6 "GNDD") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0402_1005Metric" (layer "B.Cu")
    (at 53 138.12816 90)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Field2" "")
    (property "Sheetfile" "peripherials_sch.kicad_sch")
    (property "Sheetname" "Peripherials")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C201" (at 0 1.16 90) (layer "B.SilkS"))
    (fp_text value "100n" (at 0 -1.16 90) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.48 0 90) (size 0.56 0.62) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 1 "IOVDD") (pintype "passive"))
    (pad "2" smd roundrect (at 0.48 0 90) (size 0.56 0.62) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 6 "GNDD") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0402_1005Metric" (layer "B.Cu")
    (at 57.2 148.12816)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Field2" "")
    (property "Sheetfile" "peripherials_sch.kicad_sch")
    (property "Sheetname" "Peripherials")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C213" (at 2.4 0) (layer "B.SilkS"))
    (fp_text value "100n" (at 0 -1.16) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.48 0) (size 0.56 0.62) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 10 "ADC_AVDD") (pintype "passive"))
    (pad "2" smd roundrect (at 0.48 0) (size 0.56 0.62) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 6 "GNDD") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0402_1005Metric" (layer "B.Cu")
    (at 53 174.72816 -90)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Field2" "")
    (property "Sheetfile" "interface_sch.kicad_sch")
    (property "Sheetname" "Interface")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C305" (at 0 1.16 90) (layer "B.SilkS"))
    (fp_text value "100n" (at 0 -1.16 90) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.48 0 270) (size 0.56 0.62) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 1 "IOVDD") (pintype "passive"))
    (pad "2" smd roundrect (at 0.48 0 270) (size 0.56 0.62) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 6 "GNDD") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0402_1005Metric" (layer "B.Cu")
    (at 52.4 142.72816 90)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Field2" "")
    (property "Sheetfile" "peripherials_sch.kicad_sch")
    (property "Sheetname" "Peripherials")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C210" (at 0 1.16 90) (layer "B.SilkS"))
    (fp_text value "100n" (at 0 -1.16 90) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.48 0 90) (size 0.56 0.62) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 7 "DVDD") (pintype "passive"))
    (pad "2" smd roundrect (at 0.48 0 90) (size 0.56 0.62) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 6 "GNDD") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0402_1005Metric" (layer "B.Cu")
    (at 44.2 143.92816 180)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Field2" "")
    (property "Sheetfile" "peripherials_sch.kicad_sch")
    (property "Sheetname" "Peripherials")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C203" (at 0 1.16) (layer "B.SilkS"))
    (fp_text value "100n" (at 0 -1.16) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.48 0 180) (size 0.56 0.62) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 1 "IOVDD") (pintype "passive"))
    (pad "2" smd roundrect (at 0.48 0 180) (size 0.56 0.62) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 6 "GNDD") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_line (start 27.14 133.51416) (end 77.94 133.51416)
    (layer "Edge.Cuts"))
  (gr_circle (center 218 55.92816) (end 220.25 55.92816)
    (fill none) (layer "Edge.Cuts"))
  (gr_arc (start 78.194 154.08816) (mid 78.119605 154.267765) (end 77.94 154.34216)
    (layer "Edge.Cuts"))
  (gr_arc (start 26.886 158.76816) (mid 26.960395 158.588555) (end 27.14 158.51416)
    (layer "Edge.Cuts"))
  (gr_arc (start 104 105.92816) (mid 106.828411 107.099749) (end 108 109.92816)
    (layer "Edge.Cuts"))
  (gr_line (start 222 55.92816) (end 222 131.92816)
    (layer "Edge.Cuts"))
  (gr_arc (start 77.94 158.51416) (mid 78.119605 158.588555) (end 78.194 158.76816)
    (layer "Edge.Cuts"))
  (gr_arc (start 26.886 133.76816) (mid 26.960395 133.588555) (end 27.14 133.51416)
    (layer "Edge.Cuts"))
  (gr_arc (start 27.14 179.34216) (mid 26.960395 179.267765) (end 26.886 179.08816)
    (layer "Edge.Cuts"))
  (gr_line (start 82 51.92816) (end 218 51.92816)
    (layer "Edge.Cuts"))
  (gr_circle (center 179.15 71.92816) (end 180.65 71.92816)
    (fill none) (layer "Edge.Cuts"))
  (gr_line (start 77.94 179.34216) (end 27.14 179.34216)
    (layer "Edge.Cuts"))
  (gr_arc (start 77.94 133.51416) (mid 78.119605 133.588555) (end 78.194 133.76816)
    (layer "Edge.Cuts"))
  (gr_line (start 27.14 158.51416) (end 77.94 158.51416)
    (layer "Edge.Cuts"))
  (gr_arc (start 222 131.92816) (mid 220.828449 134.756609) (end 218 135.92816)
    (layer "Edge.Cuts"))
  (gr_arc (start 78.194 179.08816) (mid 78.119605 179.267765) (end 77.94 179.34216)
    (layer "Edge.Cuts"))
  (gr_line (start 108 131.92816) (end 108 109.72816)
    (layer "Edge.Cuts"))
  (gr_circle (center 179.15 115.92816) (end 180.65 115.92816)
    (fill none) (layer "Edge.Cuts"))
  (gr_circle (center 218 131.92816) (end 220.25 131.92816)
    (fill none) (layer "Edge.Cuts"))
  (gr_arc (start 112 135.92816) (mid 109.171556 134.756604) (end 108 131.92816)
    (layer "Edge.Cuts"))
  (gr_circle (center 82 55.92816) (end 84.25 55.92816)
    (fill none) (layer "Edge.Cuts"))
  (gr_line (start 78.194 133.76816) (end 78.194 154.08816)
    (layer "Edge.Cuts"))
  (gr_line (start 26.886 179.08816) (end 26.886 158.76816)
    (layer "Edge.Cuts"))
  (gr_circle (center 139.15 115.92816) (end 140.65 115.92816)
    (fill none) (layer "Edge.Cuts"))
  (gr_arc (start 218 51.92816) (mid 220.828412 53.099748) (end 222 55.92816)
    (layer "Edge.Cuts"))
  (gr_line (start 104 105.92816) (end 82 105.92816)
    (layer "Edge.Cuts"))
  (gr_line (start 77.94 154.34216) (end 27.14 154.34216)
    (layer "Edge.Cuts"))
  (gr_arc (start 27.14 154.34216) (mid 26.960395 154.267765) (end 26.886 154.08816)
    (layer "Edge.Cuts"))
  (gr_line (start 78.194 158.76816) (end 78.194 179.08816)
    (layer "Edge.Cuts"))
  (gr_line (start 26.886 154.08816) (end 26.886 133.76816)
    (layer "Edge.Cuts"))
  (gr_arc (start 82 105.92816) (mid 79.171573 104.756587) (end 78 101.92816)
    (layer "Edge.Cuts"))
  (gr_line (start 78 55.92816) (end 78 101.92816)
    (layer "Edge.Cuts"))
  (gr_circle (center 202.15 71.92816) (end 203.65 71.92816)
    (fill none) (layer "Edge.Cuts"))
  (gr_arc (start 78 55.92816) (mid 79.171574 53.099734) (end 82 51.92816)
    (layer "Edge.Cuts"))
  (gr_line (start 112 135.92816) (end 218 135.92816)
    (layer "Edge.Cuts"))
  (gr_circle (center 112 131.92816) (end 114.25 131.92816)
    (fill none) (layer "Edge.Cuts"))
  (gr_circle (center 139.15 71.92816) (end 140.65 71.92816)
    (fill none) (layer "Edge.Cuts"))
  (gr_text "© 2023\nH. Poetzl" (at 75 148.52816) (layer "B.SilkS"))
  (gr_text "© 2023\nH. Poetzl" (at 75 173.52816) (layer "B.SilkS"))
  (gr_text "RP2040\nBreakout V1.0" (at 31 173.72816) (layer "B.SilkS"))
  (gr_text "RP2040\nBreakout V1.0" (at 31 148.72816) (layer "B.SilkS"))
  (zone (net 6) (net_name "GNDD") (layers "F&B.Cu") (name "GND") (hatch edge 0.508)
    (connect_pads (clearance 0.2))
    (min_thickness 0.2) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.22) (thermal_bridge_width 0.4))
    (polygon
      (pts
        (xy 77.94 154.08816)
        (xy 27.14 154.08816)
        (xy 27.14 133.76816)
        (xy 77.94 133.76816)
      )
    )
  )
  (zone (net 6) (net_name "GNDD") (layers "F&B.Cu") (name "GND") (hatch edge 0.508)
    (connect_pads (clearance 0.2))
    (min_thickness 0.2) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.22) (thermal_bridge_width 0.4))
    (polygon
      (pts
        (xy 77.94 179.08816)
        (xy 27.14 179.08816)
        (xy 27.14 158.76816)
        (xy 77.94 158.76816)
      )
    )
  )
)
