(kicad_symbol_lib (version 20211014) (generator kicad_symbol_editor)
  (symbol "Pico" (pin_names (offset 1.016)) (in_bom yes) (on_board yes)
    (property "Reference" "U" (id 0) (at -13.97 27.94 0))
    (property "Value" "Pico" (id 1) (at 0 19.05 0))
    (property "Footprint" "RPi_Pico:RPi_Pico_SMD_TH" (id 2) (at 0 0 90))
    (property "Datasheet" "" (id 3) (at 0 0 0))
    (symbol "Pico_0_0"
      (text "Raspberry Pi" (at 0 21.59 0))
    )
    (symbol "Pico_0_1")
    (symbol "Pico_1_1"
      (pin bidirectional line (at -17.78 24.13 0) (length 2.54)
        (name "GPIO0")
        (number "1")
      )
      (pin bidirectional line (at -17.78 1.27 0) (length 2.54)
        (name "GPIO7")
        (number "10")
      )
      (pin bidirectional line (at -17.78 -1.27 0) (length 2.54)
        (name "GPIO8")
        (number "11")
      )
      (pin bidirectional line (at -17.78 -3.81 0) (length 2.54)
        (name "GPIO9")
        (number "12")
      )
      (pin power_in line (at -17.78 -6.35 0) (length 2.54)
        (name "GND")
        (number "13")
      )
      (pin bidirectional line (at -17.78 -8.89 0) (length 2.54)
        (name "GPIO10")
        (number "14")
      )
      (pin bidirectional line (at -17.78 -11.43 0) (length 2.54)
        (name "GPIO11")
        (number "15")
      )
      (pin bidirectional line (at -17.78 -13.97 0) (length 2.54)
        (name "GPIO12")
        (number "16")
      )
      (pin bidirectional line (at -17.78 -16.51 0) (length 2.54)
        (name "GPIO13")
        (number "17")
      )
      (pin power_in line (at -17.78 -19.05 0) (length 2.54)
        (name "GND")
        (number "18")
      )
      (pin bidirectional line (at -17.78 -21.59 0) (length 2.54)
        (name "GPIO14")
        (number "19")
      )
      (pin bidirectional line (at -17.78 21.59 0) (length 2.54)
        (name "GPIO1")
        (number "2")
      )
      (pin bidirectional line (at -17.78 -24.13 0) (length 2.54)
        (name "GPIO15")
        (number "20")
      )
      (pin bidirectional line (at 17.78 -24.13 180) (length 2.54)
        (name "GPIO16")
        (number "21")
      )
      (pin bidirectional line (at 17.78 -21.59 180) (length 2.54)
        (name "GPIO17")
        (number "22")
      )
      (pin power_in line (at 17.78 -19.05 180) (length 2.54)
        (name "GND")
        (number "23")
      )
      (pin bidirectional line (at 17.78 -16.51 180) (length 2.54)
        (name "GPIO18")
        (number "24")
      )
      (pin bidirectional line (at 17.78 -13.97 180) (length 2.54)
        (name "GPIO19")
        (number "25")
      )
      (pin bidirectional line (at 17.78 -11.43 180) (length 2.54)
        (name "GPIO20")
        (number "26")
      )
      (pin bidirectional line (at 17.78 -8.89 180) (length 2.54)
        (name "GPIO21")
        (number "27")
      )
      (pin power_in line (at 17.78 -6.35 180) (length 2.54)
        (name "GND")
        (number "28")
      )
      (pin bidirectional line (at 17.78 -3.81 180) (length 2.54)
        (name "GPIO22")
        (number "29")
      )
      (pin power_in line (at -17.78 19.05 0) (length 2.54)
        (name "GND")
        (number "3")
      )
      (pin input line (at 17.78 -1.27 180) (length 2.54)
        (name "RUN")
        (number "30")
      )
      (pin bidirectional line (at 17.78 1.27 180) (length 2.54)
        (name "GPIO26_ADC0")
        (number "31")
      )
      (pin bidirectional line (at 17.78 3.81 180) (length 2.54)
        (name "GPIO27_ADC1")
        (number "32")
      )
      (pin power_in line (at 17.78 6.35 180) (length 2.54)
        (name "AGND")
        (number "33")
      )
      (pin bidirectional line (at 17.78 8.89 180) (length 2.54)
        (name "GPIO28_ADC2")
        (number "34")
      )
      (pin unspecified line (at 17.78 11.43 180) (length 2.54)
        (name "ADC_VREF")
        (number "35")
      )
      (pin unspecified line (at 17.78 13.97 180) (length 2.54)
        (name "3V3")
        (number "36")
      )
      (pin input line (at 17.78 16.51 180) (length 2.54)
        (name "3V3_EN")
        (number "37")
      )
      (pin bidirectional line (at 17.78 19.05 180) (length 2.54)
        (name "GND")
        (number "38")
      )
      (pin unspecified line (at 17.78 21.59 180) (length 2.54)
        (name "VSYS")
        (number "39")
      )
      (pin bidirectional line (at -17.78 16.51 0) (length 2.54)
        (name "GPIO2")
        (number "4")
      )
      (pin unspecified line (at 17.78 24.13 180) (length 2.54)
        (name "VBUS")
        (number "40")
      )
      (pin input line (at -2.54 -29.21 90) (length 2.54)
        (name "SWCLK")
        (number "41")
      )
      (pin power_in line (at 0 -29.21 90) (length 2.54)
        (name "GND")
        (number "42")
      )
      (pin bidirectional line (at 2.54 -29.21 90) (length 2.54)
        (name "SWDIO")
        (number "43")
      )
      (pin bidirectional line (at -17.78 13.97 0) (length 2.54)
        (name "GPIO3")
        (number "5")
      )
      (pin bidirectional line (at -17.78 11.43 0) (length 2.54)
        (name "GPIO4")
        (number "6")
      )
      (pin bidirectional line (at -17.78 8.89 0) (length 2.54)
        (name "GPIO5")
        (number "7")
      )
      (pin power_in line (at -17.78 6.35 0) (length 2.54)
        (name "GND")
        (number "8")
      )
      (pin bidirectional line (at -17.78 3.81 0) (length 2.54)
        (name "GPIO6")
        (number "9")
      )
    )
  )
  (symbol "RP2040" (pin_names (offset 1.016)) (in_bom yes) (on_board yes)
    (property "Reference" "U" (id 0) (at -29.21 49.53 0))
    (property "Value" "RP2040" (id 1) (at 24.13 -49.53 0))
    (property "Footprint" "RP2040_minimal:RP2040-QFN-56" (id 2) (at -19.05 0 0))
    (property "Datasheet" "" (id 3) (at -19.05 0 0))
    (symbol "RP2040_0_0"
      (text "Raspberry Pi" (at 0 5.08 0))
      (text "RP2040" (at 0 0 0))
    )
    (symbol "RP2040_0_1")
    (symbol "RP2040_1_1"
      (pin power_in line (at 8.89 50.8 270) (length 2.54)
        (name "IOVDD")
        (number "1")
      )
      (pin power_in line (at 6.35 50.8 270) (length 2.54)
        (name "IOVDD")
        (number "10")
      )
      (pin bidirectional line (at 31.75 12.7 180) (length 2.54)
        (name "GPIO8")
        (number "11")
      )
      (pin bidirectional line (at 31.75 10.16 180) (length 2.54)
        (name "GPIO9")
        (number "12")
      )
      (pin bidirectional line (at 31.75 7.62 180) (length 2.54)
        (name "GPIO10")
        (number "13")
      )
      (pin bidirectional line (at 31.75 5.08 180) (length 2.54)
        (name "GPIO11")
        (number "14")
      )
      (pin bidirectional line (at 31.75 2.54 180) (length 2.54)
        (name "GPIO12")
        (number "15")
      )
      (pin bidirectional line (at 31.75 0 180) (length 2.54)
        (name "GPIO13")
        (number "16")
      )
      (pin bidirectional line (at 31.75 -2.54 180) (length 2.54)
        (name "GPIO14")
        (number "17")
      )
      (pin bidirectional line (at 31.75 -5.08 180) (length 2.54)
        (name "GPIO15")
        (number "18")
      )
      (pin passive line (at -12.7 -50.8 90) (length 2.54)
        (name "TESTEN")
        (number "19")
      )
      (pin bidirectional line (at 31.75 33.02 180) (length 2.54)
        (name "GPIO0")
        (number "2")
      )
      (pin input line (at -31.75 -2.54 0) (length 2.54)
        (name "XIN")
        (number "20")
      )
      (pin passive line (at -31.75 -7.62 0) (length 2.54)
        (name "XOUT")
        (number "21")
      )
      (pin power_in line (at 3.81 50.8 270) (length 2.54)
        (name "IOVDD")
        (number "22")
      )
      (pin power_in line (at -17.78 50.8 270) (length 2.54)
        (name "DVDD")
        (number "23")
      )
      (pin output line (at -31.75 -31.75 0) (length 2.54)
        (name "SWCLK")
        (number "24")
      )
      (pin bidirectional line (at -31.75 -34.29 0) (length 2.54)
        (name "SWD")
        (number "25")
      )
      (pin input line (at -31.75 -20.32 0) (length 2.54)
        (name "RUN")
        (number "26")
      )
      (pin bidirectional line (at 31.75 -7.62 180) (length 2.54)
        (name "GPIO16")
        (number "27")
      )
      (pin bidirectional line (at 31.75 -10.16 180) (length 2.54)
        (name "GPIO17")
        (number "28")
      )
      (pin bidirectional line (at 31.75 -12.7 180) (length 2.54)
        (name "GPIO18")
        (number "29")
      )
      (pin bidirectional line (at 31.75 30.48 180) (length 2.54)
        (name "GPIO1")
        (number "3")
      )
      (pin bidirectional line (at 31.75 -15.24 180) (length 2.54)
        (name "GPIO19")
        (number "30")
      )
      (pin bidirectional line (at 31.75 -17.78 180) (length 2.54)
        (name "GPIO20")
        (number "31")
      )
      (pin bidirectional line (at 31.75 -20.32 180) (length 2.54)
        (name "GPIO21")
        (number "32")
      )
      (pin power_in line (at 1.27 50.8 270) (length 2.54)
        (name "IOVDD")
        (number "33")
      )
      (pin bidirectional line (at 31.75 -22.86 180) (length 2.54)
        (name "GPIO22")
        (number "34")
      )
      (pin bidirectional line (at 31.75 -25.4 180) (length 2.54)
        (name "GPIO23")
        (number "35")
      )
      (pin bidirectional line (at 31.75 -27.94 180) (length 2.54)
        (name "GPIO24")
        (number "36")
      )
      (pin bidirectional line (at 31.75 -30.48 180) (length 2.54)
        (name "GPIO25")
        (number "37")
      )
      (pin bidirectional line (at 31.75 -35.56 180) (length 2.54)
        (name "GPIO26_ADC0")
        (number "38")
      )
      (pin bidirectional line (at 31.75 -38.1 180) (length 2.54)
        (name "GPIO27_ADC1")
        (number "39")
      )
      (pin bidirectional line (at 31.75 27.94 180) (length 2.54)
        (name "GPIO2")
        (number "4")
      )
      (pin bidirectional line (at 31.75 -40.64 180) (length 2.54)
        (name "GPIO28_ADC2")
        (number "40")
      )
      (pin bidirectional line (at 31.75 -43.18 180) (length 2.54)
        (name "GPIO29_ADC3")
        (number "41")
      )
      (pin power_in line (at -1.27 50.8 270) (length 2.54)
        (name "IOVDD")
        (number "42")
      )
      (pin power_in line (at 16.51 50.8 270) (length 2.54)
        (name "ADC_AVDD")
        (number "43")
      )
      (pin power_in line (at -8.89 50.8 270) (length 2.54)
        (name "VREG_IN")
        (number "44")
      )
      (pin power_out line (at -12.7 50.8 270) (length 2.54)
        (name "VREG_VOUT")
        (number "45")
      )
      (pin bidirectional line (at 31.75 40.64 180) (length 2.54)
        (name "USB_DM")
        (number "46")
      )
      (pin bidirectional line (at 31.75 43.18 180) (length 2.54)
        (name "USB_DP")
        (number "47")
      )
      (pin power_in line (at 12.7 50.8 270) (length 2.54)
        (name "USB_VDD")
        (number "48")
      )
      (pin power_in line (at -3.81 50.8 270) (length 2.54)
        (name "IOVDD")
        (number "49")
      )
      (pin bidirectional line (at 31.75 25.4 180) (length 2.54)
        (name "GPIO3")
        (number "5")
      )
      (pin power_in line (at -20.32 50.8 270) (length 2.54)
        (name "DVDD")
        (number "50")
      )
      (pin bidirectional line (at -31.75 20.32 0) (length 2.54)
        (name "QSPI_SD3")
        (number "51")
      )
      (pin output line (at -31.75 16.51 0) (length 2.54)
        (name "QSPI_SCLK")
        (number "52")
      )
      (pin bidirectional line (at -31.75 27.94 0) (length 2.54)
        (name "QSPI_SD0")
        (number "53")
      )
      (pin bidirectional line (at -31.75 22.86 0) (length 2.54)
        (name "QSPI_SD2")
        (number "54")
      )
      (pin bidirectional line (at -31.75 25.4 0) (length 2.54)
        (name "QSPI_SD1")
        (number "55")
      )
      (pin bidirectional line (at -31.75 31.75 0) (length 2.54)
        (name "QSPI_SS")
        (number "56")
      )
      (pin power_in line (at 0 -50.8 90) (length 2.54)
        (name "GND")
        (number "57")
      )
      (pin bidirectional line (at 31.75 22.86 180) (length 2.54)
        (name "GPIO4")
        (number "6")
      )
      (pin bidirectional line (at 31.75 20.32 180) (length 2.54)
        (name "GPIO5")
        (number "7")
      )
      (pin bidirectional line (at 31.75 17.78 180) (length 2.54)
        (name "GPIO6")
        (number "8")
      )
      (pin bidirectional line (at 31.75 15.24 180) (length 2.54)
        (name "GPIO7")
        (number "9")
      )
    )
  )
)
