(kicad_pcb (version 20221018) (generator pcbnew)
  (general
    (thickness 0.92424)
  )
  (paper "A4")
  (layers
    (0 "F.Cu" signal "Front")
    (31 "B.Cu" signal "Back")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (49 "F.Fab" user)
  )
  (setup
    (stackup
      (layer "F.SilkS" (type "Top Silk Screen"))
      (layer "F.Paste" (type "Top Solder Paste"))
      (layer "F.Mask" (type "Top Solder Mask") (thickness 0.01))
      (layer "F.Cu" (type "copper") (thickness 0.07112))
      (layer "dielectric 1" (type "core") (thickness 0.762) (material "FR4") (epsilon_r 4.5) (loss_tangent 0.02))
      (layer "B.Cu" (type "copper") (thickness 0.07112))
      (layer "B.Mask" (type "Bottom Solder Mask") (thickness 0.01))
      (layer "B.Paste" (type "Bottom Solder Paste"))
      (layer "B.SilkS" (type "Bottom Silk Screen"))
      (copper_finish "None")
      (dielectric_constraints no)
    )
    (pad_to_mask_clearance 0.0508)
    (grid_origin 99.06 88.9)
    (pcbplotparams
      (layerselection 0x00010fc_ffffffff)
      (plot_on_all_layers_selection 0x0000000_00000000)
      (disableapertmacros false)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (dashed_line_dash_ratio 12.000000)
      (dashed_line_gap_ratio 3.000000)
      (svgprecision 6)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory "")
    )
  )
  (net 0 "")
  (net 1 "Net-(U1-USB_DP)")
  (net 2 "Net-(U1-USB_DM)")
  (net 3 "Net-(X1-ID)")
  (net 4 "IOVDD")
  (net 5 "/GPIO0")
  (net 6 "/GPIO1")
  (net 7 "/GPIO2")
  (net 8 "/GPIO3")
  (net 9 "/GPIO4")
  (net 10 "/GPIO5")
  (net 11 "/GPIO6")
  (net 12 "/GPIO7")
  (net 13 "/GPIO8")
  (net 14 "/GPIO9")
  (net 15 "/GPIO10")
  (net 16 "/GPIO11")
  (net 17 "/GPIO12")
  (net 18 "/GPIO13")
  (net 19 "/GPIO14")
  (net 20 "/GPIO15")
  (net 21 "/GPIO16")
  (net 22 "/GPIO17")
  (net 23 "/GPIO18")
  (net 24 "/GPIO19")
  (net 25 "/GPIO20")
  (net 26 "/GPIO21")
  (net 27 "/GPIO22")
  (net 28 "/GPIO23")
  (net 29 "/GPIO24")
  (net 30 "/GPIO25")
  (net 31 "/GPIO26")
  (net 32 "/GPIO27")
  (net 33 "/GPIO28")
  (net 34 "/GPIO29")
  (net 35 "/QSPI.SCLK")
  (net 36 "/QSPI.SS")
  (net 37 "/QSPI.D0")
  (net 38 "/QSPI.D3")
  (net 39 "/QSPI.D2")
  (net 40 "/QSPI.D1")
  (net 41 "XIN")
  (net 42 "SWCLK")
  (net 43 "RUN")
  (net 44 "SWDIO")
  (net 45 "GNDD")
  (net 46 "DVDD")
  (net 47 "DM")
  (net 48 "DP")
  (net 49 "ADC_AVDD")
  (net 50 "VREG_IN")
  (net 51 "VBUS")
  (net 52 "unconnected-(U1-XOUT-Pad21)")
  (footprint "MCU_RaspberryPi_and_Boards:RP2040-QFN-56" (layer "F.Cu")
    (at 99.06 88.9 -90)
    (descr "QFN, 56 Pin (http://www.cypress.com/file/416486/download#page=40), generated with kicad-footprint-generator ipc_dfn_qfn_generator.py")
    (tags "QFN DFN_QFN")
    (property "Sheetfile" "RP2040_Breakout.kicad_sch")
    (property "Sheetname" "")
    (zone_connect 2)
    (attr smd)
    (fp_text reference "U1" (at -4.2 -4.82 180) (layer "F.SilkS"))
    (fp_text value "RP2040" (at -3.4 5.02 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "" smd roundrect (at -0.6375 -0.6375 270) (size 1.084435 1.084435) (layers "F.Paste") (roundrect_rratio 0.230535))
    (pad "" smd roundrect (at -0.6375 0.6375 270) (size 1.084435 1.084435) (layers "F.Paste") (roundrect_rratio 0.230535))
    (pad "" smd roundrect (at 0.6375 -0.6375 270) (size 1.084435 1.084435) (layers "F.Paste") (roundrect_rratio 0.230535))
    (pad "" smd roundrect (at 0.6375 0.6375 270) (size 1.084435 1.084435) (layers "F.Paste") (roundrect_rratio 0.230535))
    (pad "1" smd roundrect (at -3.4375 -2.6 270) (size 0.875 0.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "IOVDD") (pinfunction "IOVDD") (pintype "power_in"))
    (pad "2" smd roundrect (at -3.4375 -2.2 270) (size 0.875 0.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 5 "/GPIO0") (pinfunction "GPIO0") (pintype "bidirectional"))
    (pad "3" smd roundrect (at -3.4375 -1.8 270) (size 0.875 0.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 6 "/GPIO1") (pinfunction "GPIO1") (pintype "bidirectional"))
    (pad "4" smd roundrect (at -3.4375 -1.4 270) (size 0.875 0.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 7 "/GPIO2") (pinfunction "GPIO2") (pintype "bidirectional"))
    (pad "5" smd roundrect (at -3.4375 -1 270) (size 0.875 0.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 8 "/GPIO3") (pinfunction "GPIO3") (pintype "bidirectional"))
    (pad "6" smd roundrect (at -3.4375 -0.6 270) (size 0.875 0.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 9 "/GPIO4") (pinfunction "GPIO4") (pintype "bidirectional"))
    (pad "7" smd roundrect (at -3.4375 -0.2 270) (size 0.875 0.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 10 "/GPIO5") (pinfunction "GPIO5") (pintype "bidirectional"))
    (pad "8" smd roundrect (at -3.4375 0.2 270) (size 0.875 0.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 11 "/GPIO6") (pinfunction "GPIO6") (pintype "bidirectional"))
    (pad "9" smd roundrect (at -3.4375 0.6 270) (size 0.875 0.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 12 "/GPIO7") (pinfunction "GPIO7") (pintype "bidirectional"))
    (pad "10" smd roundrect (at -3.4375 1 270) (size 0.875 0.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "IOVDD") (pinfunction "IOVDD") (pintype "power_in"))
    (pad "11" smd roundrect (at -3.4375 1.4 270) (size 0.875 0.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 13 "/GPIO8") (pinfunction "GPIO8") (pintype "bidirectional"))
    (pad "12" smd roundrect (at -3.4375 1.8 270) (size 0.875 0.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 14 "/GPIO9") (pinfunction "GPIO9") (pintype "bidirectional"))
    (pad "13" smd roundrect (at -3.4375 2.2 270) (size 0.875 0.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 15 "/GPIO10") (pinfunction "GPIO10") (pintype "bidirectional"))
    (pad "14" smd roundrect (at -3.4375 2.6 270) (size 0.875 0.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 16 "/GPIO11") (pinfunction "GPIO11") (pintype "bidirectional"))
    (pad "15" smd roundrect (at -2.6 3.4375 270) (size 0.2 0.875) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 17 "/GPIO12") (pinfunction "GPIO12") (pintype "bidirectional"))
    (pad "16" smd roundrect (at -2.2 3.4375 270) (size 0.2 0.875) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 18 "/GPIO13") (pinfunction "GPIO13") (pintype "bidirectional"))
    (pad "17" smd roundrect (at -1.8 3.4375 270) (size 0.2 0.875) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 19 "/GPIO14") (pinfunction "GPIO14") (pintype "bidirectional"))
    (pad "18" smd roundrect (at -1.4 3.4375 270) (size 0.2 0.875) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 20 "/GPIO15") (pinfunction "GPIO15") (pintype "bidirectional"))
    (pad "19" smd roundrect (at -1 3.4375 270) (size 0.2 0.875) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 45 "GNDD") (pinfunction "TESTEN") (pintype "passive"))
    (pad "20" smd roundrect (at -0.6 3.4375 270) (size 0.2 0.875) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 41 "XIN") (pinfunction "XIN") (pintype "input"))
    (pad "21" smd roundrect (at -0.2 3.4375 270) (size 0.2 0.875) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 52 "unconnected-(U1-XOUT-Pad21)") (pinfunction "XOUT") (pintype "passive"))
    (pad "22" smd roundrect (at 0.2 3.4375 270) (size 0.2 0.875) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "IOVDD") (pinfunction "IOVDD") (pintype "power_in"))
    (pad "23" smd roundrect (at 0.6 3.4375 270) (size 0.2 0.875) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 46 "DVDD") (pinfunction "DVDD") (pintype "power_in"))
    (pad "24" smd roundrect (at 1 3.4375 270) (size 0.2 0.875) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 42 "SWCLK") (pinfunction "SWCLK") (pintype "output"))
    (pad "25" smd roundrect (at 1.4 3.4375 270) (size 0.2 0.875) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 44 "SWDIO") (pinfunction "SWD") (pintype "bidirectional"))
    (pad "26" smd roundrect (at 1.8 3.4375 270) (size 0.2 0.875) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 43 "RUN") (pinfunction "RUN") (pintype "input"))
    (pad "27" smd roundrect (at 2.2 3.4375 270) (size 0.2 0.875) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 21 "/GPIO16") (pinfunction "GPIO16") (pintype "bidirectional"))
    (pad "28" smd roundrect (at 2.6 3.4375 270) (size 0.2 0.875) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 22 "/GPIO17") (pinfunction "GPIO17") (pintype "bidirectional"))
    (pad "29" smd roundrect (at 3.4375 2.6 270) (size 0.875 0.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 23 "/GPIO18") (pinfunction "GPIO18") (pintype "bidirectional"))
    (pad "30" smd roundrect (at 3.4375 2.2 270) (size 0.875 0.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 24 "/GPIO19") (pinfunction "GPIO19") (pintype "bidirectional"))
    (pad "31" smd roundrect (at 3.4375 1.8 270) (size 0.875 0.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 25 "/GPIO20") (pinfunction "GPIO20") (pintype "bidirectional"))
    (pad "32" smd roundrect (at 3.4375 1.4 270) (size 0.875 0.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 26 "/GPIO21") (pinfunction "GPIO21") (pintype "bidirectional"))
    (pad "33" smd roundrect (at 3.4375 1 270) (size 0.875 0.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "IOVDD") (pinfunction "IOVDD") (pintype "power_in"))
    (pad "34" smd roundrect (at 3.4375 0.6 270) (size 0.875 0.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 27 "/GPIO22") (pinfunction "GPIO22") (pintype "bidirectional"))
    (pad "35" smd roundrect (at 3.4375 0.2 270) (size 0.875 0.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 28 "/GPIO23") (pinfunction "GPIO23") (pintype "bidirectional"))
    (pad "36" smd roundrect (at 3.4375 -0.2 270) (size 0.875 0.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 29 "/GPIO24") (pinfunction "GPIO24") (pintype "bidirectional"))
    (pad "37" smd roundrect (at 3.4375 -0.6 270) (size 0.875 0.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 30 "/GPIO25") (pinfunction "GPIO25") (pintype "bidirectional"))
    (pad "38" smd roundrect (at 3.4375 -1 270) (size 0.875 0.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 31 "/GPIO26") (pinfunction "GPIO26_ADC0") (pintype "bidirectional"))
    (pad "39" smd roundrect (at 3.4375 -1.4 270) (size 0.875 0.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 32 "/GPIO27") (pinfunction "GPIO27_ADC1") (pintype "bidirectional"))
    (pad "40" smd roundrect (at 3.4375 -1.8 270) (size 0.875 0.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 33 "/GPIO28") (pinfunction "GPIO28_ADC2") (pintype "bidirectional"))
    (pad "41" smd roundrect (at 3.4375 -2.2 270) (size 0.875 0.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 34 "/GPIO29") (pinfunction "GPIO29_ADC3") (pintype "bidirectional"))
    (pad "42" smd roundrect (at 3.4375 -2.6 270) (size 0.875 0.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "IOVDD") (pinfunction "IOVDD") (pintype "power_in"))
    (pad "43" smd roundrect (at 2.6 -3.4375 270) (size 0.2 0.875) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 49 "ADC_AVDD") (pinfunction "ADC_AVDD") (pintype "power_in"))
    (pad "44" smd roundrect (at 2.2 -3.4375 270) (size 0.2 0.875) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 50 "VREG_IN") (pinfunction "VREG_IN") (pintype "power_in"))
    (pad "45" smd roundrect (at 1.8 -3.4375 270) (size 0.2 0.875) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 46 "DVDD") (pinfunction "VREG_VOUT") (pintype "power_out"))
    (pad "46" smd roundrect (at 1.4 -3.4375 270) (size 0.2 0.875) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "Net-(U1-USB_DM)") (pinfunction "USB_DM") (pintype "bidirectional"))
    (pad "47" smd roundrect (at 1 -3.4375 270) (size 0.2 0.875) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "Net-(U1-USB_DP)") (pinfunction "USB_DP") (pintype "bidirectional"))
    (pad "48" smd roundrect (at 0.6 -3.4375 270) (size 0.2 0.875) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "IOVDD") (pinfunction "USB_VDD") (pintype "power_in"))
    (pad "49" smd roundrect (at 0.2 -3.4375 270) (size 0.2 0.875) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "IOVDD") (pinfunction "IOVDD") (pintype "power_in"))
    (pad "50" smd roundrect (at -0.2 -3.4375 270) (size 0.2 0.875) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 46 "DVDD") (pinfunction "DVDD") (pintype "power_in"))
    (pad "51" smd roundrect (at -0.6 -3.4375 270) (size 0.2 0.875) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 38 "/QSPI.D3") (pinfunction "QSPI_SD3") (pintype "bidirectional"))
    (pad "52" smd roundrect (at -1 -3.4375 270) (size 0.2 0.875) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 35 "/QSPI.SCLK") (pinfunction "QSPI_SCLK") (pintype "output"))
    (pad "53" smd roundrect (at -1.4 -3.4375 270) (size 0.2 0.875) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 37 "/QSPI.D0") (pinfunction "QSPI_SD0") (pintype "bidirectional"))
    (pad "54" smd roundrect (at -1.8 -3.4375 270) (size 0.2 0.875) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 39 "/QSPI.D2") (pinfunction "QSPI_SD2") (pintype "bidirectional"))
    (pad "55" smd roundrect (at -2.2 -3.4375 270) (size 0.2 0.875) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 40 "/QSPI.D1") (pinfunction "QSPI_SD1") (pintype "bidirectional"))
    (pad "56" smd roundrect (at -2.6 -3.4375 270) (size 0.2 0.875) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 36 "/QSPI.SS") (pinfunction "QSPI_SS") (pintype "bidirectional"))
    (pad "57" thru_hole circle (at -1.275 -1.275 270) (size 0.6 0.6) (drill 0.35) (layers "*.Cu")
      (net 45 "GNDD") (pinfunction "GND") (pintype "power_in"))
    (pad "57" thru_hole circle (at -1.275 0 270) (size 0.6 0.6) (drill 0.35) (layers "*.Cu")
      (net 45 "GNDD") (pinfunction "GND") (pintype "power_in"))
    (pad "57" thru_hole circle (at -1.275 1.275 270) (size 0.6 0.6) (drill 0.35) (layers "*.Cu")
      (net 45 "GNDD") (pinfunction "GND") (pintype "power_in"))
    (pad "57" thru_hole circle (at 0 -1.275 270) (size 0.6 0.6) (drill 0.35) (layers "*.Cu")
      (net 45 "GNDD") (pinfunction "GND") (pintype "power_in"))
    (pad "57" thru_hole circle (at 0 0 270) (size 0.6 0.6) (drill 0.35) (layers "*.Cu")
      (net 45 "GNDD") (pinfunction "GND") (pintype "power_in"))
    (pad "57" smd roundrect (at 0 0 270) (size 3.2 3.2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.045)
      (net 45 "GNDD") (pinfunction "GND") (pintype "power_in"))
    (pad "57" thru_hole circle (at 0 1.275 270) (size 0.6 0.6) (drill 0.35) (layers "*.Cu")
      (net 45 "GNDD") (pinfunction "GND") (pintype "power_in"))
    (pad "57" thru_hole circle (at 1.275 -1.275 270) (size 0.6 0.6) (drill 0.35) (layers "*.Cu")
      (net 45 "GNDD") (pinfunction "GND") (pintype "power_in"))
    (pad "57" thru_hole circle (at 1.275 0 270) (size 0.6 0.6) (drill 0.35) (layers "*.Cu")
      (net 45 "GNDD") (pinfunction "GND") (pintype "power_in"))
    (pad "57" thru_hole circle (at 1.275 1.275 270) (size 0.6 0.6) (drill 0.35) (layers "*.Cu")
      (net 45 "GNDD") (pinfunction "GND") (pintype "power_in"))
    (model "${KISYS3DMOD}/Package_DFN_QFN.3dshapes/QFN-56-1EP_7x7mm_P0.4mm_EP5.6x5.6mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model "RP2040_QFN56_04.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0402_1005Metric" (layer "F.Cu")
    (at 119.46 86.36 -90)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "RP2040_Breakout.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R3" (at -1.96 -0.1 90) (layer "F.SilkS"))
    (fp_text value "0R" (at -2 -0.03 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.51 0 270) (size 0.54 0.64) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 45 "GNDD") (pintype "passive"))
    (pad "2" smd roundrect (at 0.51 0 270) (size 0.54 0.64) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 3 "Net-(X1-ID)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinHeader_2.54mm:PinHeader_1x03_P2.54mm_Vertical" (layer "F.Cu")
    (at 77.47 86.36)
    (descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x03 2.54mm single row")
    (property "Sheetfile" "RP2040_Breakout.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x03, script generated (kicad-library-utils/schlib/autogen/connector/)")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "J3" (at 2.921 5.08) (layer "F.SilkS"))
    (fp_text value "Conn_01x03" (at -2.794 2.54 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 2.54 90) (layer "F.Fab"))
    (pad "1" thru_hole roundrect (at 0 0) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask") (roundrect_rratio 0.25)
      (net 42 "SWCLK") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 45 "GNDD") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 44 "SWDIO") (pinfunction "Pin_3") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x03_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinHeader_2.54mm:PinHeader_1x20_P2.54mm_Vertical" (layer "F.Cu")
    (at 125.73 80.01 -90)
    (descr "Through hole straight pin header, 1x20, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x20 2.54mm single row")
    (property "Sheetfile" "RP2040_Breakout.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x20, script generated (kicad-library-utils/schlib/autogen/connector/)")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "J2" (at 3.048 48.514) (layer "F.SilkS"))
    (fp_text value "Conn_01x20" (at 2.794 24.13) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 24.13) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 35 "/QSPI.SCLK") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 2.54 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 37 "/QSPI.D0") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 5.08 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 36 "/QSPI.SS") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole oval (at 0 7.62 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 45 "GNDD") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" thru_hole oval (at 0 10.16 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 5 "/GPIO0") (pinfunction "Pin_5") (pintype "passive"))
    (pad "6" thru_hole oval (at 0 12.7 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 6 "/GPIO1") (pinfunction "Pin_6") (pintype "passive"))
    (pad "7" thru_hole oval (at 0 15.24 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 7 "/GPIO2") (pinfunction "Pin_7") (pintype "passive"))
    (pad "8" thru_hole oval (at 0 17.78 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 8 "/GPIO3") (pinfunction "Pin_8") (pintype "passive"))
    (pad "9" thru_hole oval (at 0 20.32 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 9 "/GPIO4") (pinfunction "Pin_9") (pintype "passive"))
    (pad "10" thru_hole oval (at 0 22.86 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 10 "/GPIO5") (pinfunction "Pin_10") (pintype "passive"))
    (pad "11" thru_hole oval (at 0 25.4 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 11 "/GPIO6") (pinfunction "Pin_11") (pintype "passive"))
    (pad "12" thru_hole oval (at 0 27.94 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 12 "/GPIO7") (pinfunction "Pin_12") (pintype "passive"))
    (pad "13" thru_hole oval (at 0 30.48 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 13 "/GPIO8") (pinfunction "Pin_13") (pintype "passive"))
    (pad "14" thru_hole oval (at 0 33.02 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 14 "/GPIO9") (pinfunction "Pin_14") (pintype "passive"))
    (pad "15" thru_hole oval (at 0 35.56 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 15 "/GPIO10") (pinfunction "Pin_15") (pintype "passive"))
    (pad "16" thru_hole oval (at 0 38.1 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 16 "/GPIO11") (pinfunction "Pin_16") (pintype "passive"))
    (pad "17" thru_hole oval (at 0 40.64 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 17 "/GPIO12") (pinfunction "Pin_17") (pintype "passive"))
    (pad "18" thru_hole oval (at 0 43.18 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 18 "/GPIO13") (pinfunction "Pin_18") (pintype "passive"))
    (pad "19" thru_hole oval (at 0 45.72 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 19 "/GPIO14") (pinfunction "Pin_19") (pintype "passive"))
    (pad "20" thru_hole oval (at 0 48.26 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 20 "/GPIO15") (pinfunction "Pin_20") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x20_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_USB:USB_Micro-B_Amphenol_10104110_Horizontal" (layer "F.Cu")
    (at 124.206 88.9 90)
    (descr "USB Micro-B, horizontal, https://cdn.amphenol-icc.com/media/wysiwyg/files/drawing/10104110.pdf")
    (tags "USB Micro B horizontal")
    (property "Sheetfile" "RP2040_Breakout.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "USB Micro Type B connector")
    (property "ki_keywords" "connector USB micro")
    (attr smd)
    (fp_text reference "X1" (at -2.54 -3.556 90) (layer "F.SilkS"))
    (fp_text value "USB_B_Micro" (at 0 5.35 90) (layer "F.Fab"))
    (fp_text user "PCB edge" (at 0 2.75 90) (layer "Dwgs.User"))
    (fp_text user "${REFERENCE}" (at 0 -0.2 90) (layer "F.Fab"))
    (pad "1" smd rect (at -1.3 -1.55 90) (size 0.4 1.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 51 "VBUS") (pinfunction "VBUS") (pintype "power_out"))
    (pad "2" smd rect (at -0.65 -1.55 90) (size 0.4 1.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 47 "DM") (pinfunction "D-") (pintype "bidirectional"))
    (pad "3" smd rect (at 0 -1.55 90) (size 0.4 1.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 48 "DP") (pinfunction "D+") (pintype "bidirectional"))
    (pad "4" smd rect (at 0.65 -1.55 90) (size 0.4 1.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 3 "Net-(X1-ID)") (pinfunction "ID") (pintype "passive"))
    (pad "5" smd rect (at 1.3 -1.55 90) (size 0.4 1.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 45 "GNDD") (pinfunction "GND") (pintype "power_out"))
    (pad "6" smd rect (at -3.75 1.3 90) (size 2.3 1.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 45 "GNDD") (pinfunction "Shield") (pintype "passive"))
    (pad "6" smd rect (at -1.15 1.3 90) (size 1.8 1.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 45 "GNDD") (pinfunction "Shield") (pintype "passive"))
    (pad "6" smd rect (at 1.15 1.3 90) (size 1.8 1.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 45 "GNDD") (pinfunction "Shield") (pintype "passive"))
    (pad "6" smd rect (at 3.75 1.3 90) (size 2.3 1.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 45 "GNDD") (pinfunction "Shield") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_USB.3dshapes/USB_Micro-B_Amphenol_10104110_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model "Amphenol_10104110.stp"
      (offset (xyz 0 1.27 6.985))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0402_1005Metric" (layer "F.Cu")
    (at 106.26 89.6)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "RP2040_Breakout.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R1" (at 2.4 -0.4) (layer "F.SilkS"))
    (fp_text value "27R" (at 0 -1.23) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.51 0) (size 0.54 0.64) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "Net-(U1-USB_DP)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.51 0) (size 0.54 0.64) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 48 "DP") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinHeader_2.54mm:PinHeader_1x20_P2.54mm_Vertical" (layer "F.Cu")
    (at 77.47 97.79 90)
    (descr "Through hole straight pin header, 1x20, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x20 2.54mm single row")
    (property "Sheetfile" "RP2040_Breakout.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x20, script generated (kicad-library-utils/schlib/autogen/connector/)")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "J1" (at 3.048 -0.254 180) (layer "F.SilkS"))
    (fp_text value "Conn_01x20" (at -2.794 24.13) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 24.13) (layer "F.Fab"))
    (pad "1" thru_hole roundrect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask") (roundrect_rratio 0.25)
      (net 21 "/GPIO16") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 22 "/GPIO17") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 23 "/GPIO18") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole oval (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 24 "/GPIO19") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" thru_hole oval (at 0 10.16 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 25 "/GPIO20") (pinfunction "Pin_5") (pintype "passive"))
    (pad "6" thru_hole oval (at 0 12.7 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 26 "/GPIO21") (pinfunction "Pin_6") (pintype "passive"))
    (pad "7" thru_hole oval (at 0 15.24 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 27 "/GPIO22") (pinfunction "Pin_7") (pintype "passive"))
    (pad "8" thru_hole oval (at 0 17.78 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 28 "/GPIO23") (pinfunction "Pin_8") (pintype "passive"))
    (pad "9" thru_hole oval (at 0 20.32 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 29 "/GPIO24") (pinfunction "Pin_9") (pintype "passive"))
    (pad "10" thru_hole oval (at 0 22.86 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 30 "/GPIO25") (pinfunction "Pin_10") (pintype "passive"))
    (pad "11" thru_hole oval (at 0 25.4 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 31 "/GPIO26") (pinfunction "Pin_11") (pintype "passive"))
    (pad "12" thru_hole oval (at 0 27.94 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 32 "/GPIO27") (pinfunction "Pin_12") (pintype "passive"))
    (pad "13" thru_hole oval (at 0 30.48 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 33 "/GPIO28") (pinfunction "Pin_13") (pintype "passive"))
    (pad "14" thru_hole oval (at 0 33.02 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 34 "/GPIO29") (pinfunction "Pin_14") (pintype "passive"))
    (pad "15" thru_hole oval (at 0 35.56 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 4 "IOVDD") (pinfunction "Pin_15") (pintype "passive"))
    (pad "16" thru_hole oval (at 0 38.1 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 49 "ADC_AVDD") (pinfunction "Pin_16") (pintype "passive"))
    (pad "17" thru_hole oval (at 0 40.64 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 45 "GNDD") (pinfunction "Pin_17") (pintype "passive"))
    (pad "18" thru_hole oval (at 0 43.18 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 4 "IOVDD") (pinfunction "Pin_18") (pintype "passive"))
    (pad "19" thru_hole oval (at 0 45.72 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 50 "VREG_IN") (pinfunction "Pin_19") (pintype "passive"))
    (pad "20" thru_hole oval (at 0 48.26 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 51 "VBUS") (pinfunction "Pin_20") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x20_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0402_1005Metric" (layer "F.Cu")
    (at 106.26 90.6)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "RP2040_Breakout.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R2" (at 2.4 0.4) (layer "F.SilkS"))
    (fp_text value "27R" (at 0 1.17) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.51 0) (size 0.54 0.64) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "Net-(U1-USB_DM)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.51 0) (size 0.54 0.64) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 47 "DM") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinHeader_2.54mm:PinHeader_1x03_P2.54mm_Vertical" (layer "F.Cu")
    (at 82.55 86.36 90)
    (descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x03 2.54mm single row")
    (property "Sheetfile" "RP2040_Breakout.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x03, script generated (kicad-library-utils/schlib/autogen/connector/)")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "J5" (at -0.889 7.874 180) (layer "F.SilkS"))
    (fp_text value "Conn_01x03" (at -3.048 2.54 180) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 2.54) (layer "F.Fab"))
    (pad "1" thru_hole roundrect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask") (roundrect_rratio 0.25)
      (net 41 "XIN") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 45 "GNDD") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 43 "RUN") (pinfunction "Pin_3") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x03_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinHeader_2.54mm:PinHeader_1x03_P2.54mm_Vertical" (layer "F.Cu")
    (at 110.49 86.36 90)
    (descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x03 2.54mm single row")
    (property "Sheetfile" "RP2040_Breakout.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x03, script generated (kicad-library-utils/schlib/autogen/connector/)")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "J4" (at -0.889 -2.794 180) (layer "F.SilkS"))
    (fp_text value "Conn_01x03" (at -3.048 2.54 180) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 2.54) (layer "F.Fab"))
    (pad "1" thru_hole roundrect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask") (roundrect_rratio 0.25)
      (net 40 "/QSPI.D1") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 39 "/QSPI.D2") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 38 "/QSPI.D3") (pinfunction "Pin_3") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x03_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0402_1005Metric" (layer "B.Cu")
    (at 101.46 87.7 90)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "RP2040_Breakout.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C9" (at 0 1.16 90) (layer "B.SilkS"))
    (fp_text value "100n" (at 0 -1.16 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.48 0 90) (size 0.56 0.62) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 46 "DVDD") (pintype "passive"))
    (pad "2" smd roundrect (at 0.48 0 90) (size 0.56 0.62) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 45 "GNDD") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0402_1005Metric" (layer "B.Cu")
    (at 96.06 94.7 -90)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "RP2040_Breakout.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C4" (at 0 1.16 90) (layer "B.SilkS"))
    (fp_text value "100n" (at 0 -1.16 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.48 0 270) (size 0.56 0.62) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 4 "IOVDD") (pintype "passive"))
    (pad "2" smd roundrect (at 0.48 0 270) (size 0.56 0.62) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 45 "GNDD") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0402_1005Metric" (layer "B.Cu")
    (at 106.26 91.9)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "RP2040_Breakout.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C12" (at 2.4 0) (layer "B.SilkS"))
    (fp_text value "1u" (at 0 -1.16) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.48 0) (size 0.56 0.62) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 50 "VREG_IN") (pintype "passive"))
    (pad "2" smd roundrect (at 0.48 0) (size 0.56 0.62) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 45 "GNDD") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0402_1005Metric" (layer "B.Cu")
    (at 102.06 83.1 90)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "RP2040_Breakout.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C1" (at 0 1.16 90) (layer "B.SilkS"))
    (fp_text value "100n" (at 0 -1.16 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.48 0 90) (size 0.56 0.62) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 4 "IOVDD") (pintype "passive"))
    (pad "2" smd roundrect (at 0.48 0 90) (size 0.56 0.62) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 45 "GNDD") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0402_1005Metric" (layer "B.Cu")
    (at 102.06 94.7 -90)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "RP2040_Breakout.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C5" (at 0 1.16 90) (layer "B.SilkS"))
    (fp_text value "100n" (at 0 -1.16 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.48 0 270) (size 0.56 0.62) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 4 "IOVDD") (pintype "passive"))
    (pad "2" smd roundrect (at 0.48 0 270) (size 0.56 0.62) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 45 "GNDD") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0402_1005Metric" (layer "B.Cu")
    (at 99.06 83.1 90)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "RP2040_Breakout.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C7" (at 0 1.16 90) (layer "B.SilkS"))
    (fp_text value "1u" (at 0 -1.16 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.48 0 90) (size 0.56 0.62) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 4 "IOVDD") (pintype "passive"))
    (pad "2" smd roundrect (at 0.48 0 90) (size 0.56 0.62) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 45 "GNDD") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0402_1005Metric" (layer "B.Cu")
    (at 99.06 91.78 -90)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "RP2040_Breakout.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C8" (at 0 1.16 90) (layer "B.SilkS"))
    (fp_text value "1u" (at 0 -1.16 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.48 0 270) (size 0.56 0.62) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 46 "DVDD") (pintype "passive"))
    (pad "2" smd roundrect (at 0.48 0 270) (size 0.56 0.62) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 45 "GNDD") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0402_1005Metric" (layer "B.Cu")
    (at 96.66 87.7 90)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "RP2040_Breakout.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C10" (at 0 -1.04 90) (layer "B.SilkS"))
    (fp_text value "100n" (at 0 -1.16 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.48 0 90) (size 0.56 0.62) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 46 "DVDD") (pintype "passive"))
    (pad "2" smd roundrect (at 0.48 0 90) (size 0.56 0.62) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 45 "GNDD") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0402_1005Metric" (layer "B.Cu")
    (at 103.66 87.7 90)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "RP2040_Breakout.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C14" (at 0 1.16 90) (layer "B.SilkS"))
    (fp_text value "100n" (at 0 -1.16 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.48 0 90) (size 0.56 0.62) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 4 "IOVDD") (pintype "passive"))
    (pad "2" smd roundrect (at 0.48 0 90) (size 0.56 0.62) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 45 "GNDD") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "B.Cu")
    (at 113.03 93.5 90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "RP2040_Breakout.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C13" (at 0 1.43 90) (layer "B.SilkS"))
    (fp_text value "10u" (at 0 -1.43 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.775 0 90) (size 0.9 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 4 "IOVDD") (pintype "passive"))
    (pad "2" smd roundrect (at 0.775 0 90) (size 0.9 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 45 "GNDD") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0402_1005Metric" (layer "B.Cu")
    (at 99.06 94.7 -90)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "RP2040_Breakout.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C6" (at 0 1.16 90) (layer "B.SilkS"))
    (fp_text value "1u" (at 0 -1.16 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.48 0 270) (size 0.56 0.62) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 4 "IOVDD") (pintype "passive"))
    (pad "2" smd roundrect (at 0.48 0 270) (size 0.56 0.62) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 45 "GNDD") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0402_1005Metric" (layer "B.Cu")
    (at 96.06 83.1 90)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "RP2040_Breakout.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C2" (at 0 1.16 90) (layer "B.SilkS"))
    (fp_text value "100n" (at 0 -1.16 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.48 0 90) (size 0.56 0.62) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 4 "IOVDD") (pintype "passive"))
    (pad "2" smd roundrect (at 0.48 0 90) (size 0.56 0.62) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 45 "GNDD") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0402_1005Metric" (layer "B.Cu")
    (at 93.26 88.9 180)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "RP2040_Breakout.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C3" (at 0 1.16) (layer "B.SilkS"))
    (fp_text value "100n" (at 0 -1.16) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.48 0 180) (size 0.56 0.62) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 4 "IOVDD") (pintype "passive"))
    (pad "2" smd roundrect (at 0.48 0 180) (size 0.56 0.62) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 45 "GNDD") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0402_1005Metric" (layer "B.Cu")
    (at 106.26 93.1)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "RP2040_Breakout.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C11" (at 2.4 0) (layer "B.SilkS"))
    (fp_text value "100n" (at 0 -1.16) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.48 0) (size 0.56 0.62) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 49 "ADC_AVDD") (pintype "passive"))
    (pad "2" smd roundrect (at 0.48 0) (size 0.56 0.62) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 45 "GNDD") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_arc (start 127 78.486) (mid 127.179605 78.560395) (end 127.254 78.74)
    (layer "Edge.Cuts"))
  (gr_arc (start 76.2 99.314) (mid 76.020395 99.239605) (end 75.946 99.06)
    (layer "Edge.Cuts"))
  (gr_line (start 75.946 99.06) (end 75.946 78.74)
    (layer "Edge.Cuts"))
  (gr_line (start 127.254 78.74) (end 127.254 99.06)
    (layer "Edge.Cuts"))
  (gr_line (start 76.2 78.486) (end 127 78.486)
    (layer "Edge.Cuts"))
  (gr_arc (start 75.946 78.74) (mid 76.020395 78.560395) (end 76.2 78.486)
    (layer "Edge.Cuts"))
  (gr_line (start 127 99.314) (end 76.2 99.314)
    (layer "Edge.Cuts"))
  (gr_arc (start 127.254 99.06) (mid 127.179605 99.239605) (end 127 99.314)
    (layer "Edge.Cuts"))
  (gr_text "© 2023\nH. Poetzl" (at 124.06 93.5) (layer "B.SilkS"))
  (gr_text "RP2040\nBreakout V1.0" (at 80.06 93.7) (layer "B.SilkS"))
  (zone (net 43) (net_name "RUN") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30057)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 87.902758 90.6238)
        (xy 87.865565 90.624421)
        (xy 87.834984 90.626108)
        (xy 87.80936 90.628595)
        (xy 87.787043 90.631614)
        (xy 87.766378 90.6349)
        (xy 87.745713 90.638185)
        (xy 87.723396 90.641204)
        (xy 87.697773 90.643691)
        (xy 87.667192 90.645378)
        (xy 87.63 90.646)
        (xy 87.629 90.9)
        (xy 87.884 90.9)
        (xy 87.882834 90.88132)
        (xy 87.87994 90.863083)
        (xy 87.876219 90.845649)
        (xy 87.872572 90.829376)
        (xy 87.869901 90.814622)
        (xy 87.869108 90.801746)
        (xy 87.871096 90.791108)
        (xy 87.876766 90.783064)
        (xy 87.887019 90.777976)
        (xy 87.902758 90.7762)
      )
    )
  )
  (zone (net 46) (net_name "DVDD") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30058)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 101.732758 88.6238)
        (xy 101.695565 88.624421)
        (xy 101.664984 88.626108)
        (xy 101.63936 88.628595)
        (xy 101.617043 88.631614)
        (xy 101.596378 88.6349)
        (xy 101.575713 88.638185)
        (xy 101.553396 88.641204)
        (xy 101.527773 88.643691)
        (xy 101.497192 88.645378)
        (xy 101.46 88.646)
        (xy 101.459 88.9)
        (xy 101.714 88.9)
        (xy 101.712834 88.88132)
        (xy 101.70994 88.863083)
        (xy 101.706219 88.845649)
        (xy 101.702572 88.829376)
        (xy 101.699901 88.814622)
        (xy 101.699108 88.801746)
        (xy 101.701096 88.791108)
        (xy 101.706766 88.783064)
        (xy 101.717019 88.777976)
        (xy 101.732758 88.7762)
      )
    )
  )
  (zone (net 28) (net_name "/GPIO23") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30014)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 95.1738 96.6)
        (xy 95.166635 96.704808)
        (xy 95.145991 96.78594)
        (xy 95.113148 96.848448)
        (xy 95.069382 96.897384)
        (xy 95.01597 96.937802)
        (xy 94.954192 96.974754)
        (xy 94.885323 97.013293)
        (xy 94.810643 97.058471)
        (xy 94.731429 97.115342)
        (xy 94.648959 97.188959)
        (xy 95.25 97.791)
        (xy 95.851041 97.188959)
        (xy 95.76857 97.115342)
        (xy 95.689355 97.058471)
        (xy 95.614675 97.013293)
        (xy 95.545807 96.974754)
        (xy 95.484028 96.937802)
        (xy 95.430617 96.897384)
        (xy 95.386851 96.848448)
        (xy 95.354008 96.78594)
        (xy 95.333364 96.704808)
        (xy 95.3262 96.6)
      )
    )
  )
  (zone (net 30) (net_name "/GPIO25") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30082)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 99.7362 92.815)
        (xy 99.738199 92.806306)
        (xy 99.740198 92.79797)
        (xy 99.742198 92.789991)
        (xy 99.744197 92.782369)
        (xy 99.746197 92.775104)
        (xy 99.748196 92.768196)
        (xy 99.750195 92.761645)
        (xy 99.752195 92.755451)
        (xy 99.754194 92.749614)
        (xy 99.756194 92.744134)
        (xy 99.66 92.3365)
        (xy 99.563806 92.744134)
        (xy 99.565805 92.749614)
        (xy 99.567804 92.755451)
        (xy 99.569804 92.761645)
        (xy 99.571803 92.768196)
        (xy 99.573803 92.775104)
        (xy 99.575802 92.782369)
        (xy 99.577801 92.789991)
        (xy 99.579801 92.79797)
        (xy 99.5818 92.806306)
        (xy 99.5838 92.815)
      )
    )
  )
  (zone (net 34) (net_name "/GPIO29") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30086)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 101.3362 92.815)
        (xy 101.338199 92.806306)
        (xy 101.340198 92.79797)
        (xy 101.342198 92.789991)
        (xy 101.344197 92.782369)
        (xy 101.346197 92.775104)
        (xy 101.348196 92.768196)
        (xy 101.350195 92.761645)
        (xy 101.352195 92.755451)
        (xy 101.354194 92.749614)
        (xy 101.356194 92.744134)
        (xy 101.26 92.3365)
        (xy 101.163806 92.744134)
        (xy 101.165805 92.749614)
        (xy 101.167804 92.755451)
        (xy 101.169804 92.761645)
        (xy 101.171803 92.768196)
        (xy 101.173803 92.775104)
        (xy 101.175802 92.782369)
        (xy 101.177801 92.789991)
        (xy 101.179801 92.79797)
        (xy 101.1818 92.806306)
        (xy 101.1838 92.815)
      )
    )
  )
  (zone (net 4) (net_name "IOVDD") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30048)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 101.754672 93.302435)
        (xy 101.781126 93.332949)
        (xy 101.797605 93.360801)
        (xy 101.806234 93.386901)
        (xy 101.809137 93.412162)
        (xy 101.808441 93.437497)
        (xy 101.80627 93.463818)
        (xy 101.804748 93.492036)
        (xy 101.806002 93.523065)
        (xy 101.812155 93.557816)
        (xy 101.825335 93.597202)
        (xy 102.060707 93.500707)
        (xy 102.157202 93.265335)
        (xy 102.117816 93.252155)
        (xy 102.083065 93.246002)
        (xy 102.052036 93.244748)
        (xy 102.023818 93.24627)
        (xy 101.997497 93.248441)
        (xy 101.972162 93.249137)
        (xy 101.946901 93.246234)
        (xy 101.920801 93.237605)
        (xy 101.892949 93.221126)
        (xy 101.862435 93.194672)
      )
    )
  )
  (zone (net 8) (net_name "/GPIO3") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30074)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 99.9838 84.985)
        (xy 99.9818 84.993693)
        (xy 99.979801 85.002029)
        (xy 99.977801 85.010008)
        (xy 99.975802 85.01763)
        (xy 99.973803 85.024895)
        (xy 99.971803 85.031803)
        (xy 99.969804 85.038354)
        (xy 99.967804 85.044548)
        (xy 99.965805 85.050385)
        (xy 99.963806 85.055866)
        (xy 100.06 85.4635)
        (xy 100.156194 85.055866)
        (xy 100.154194 85.050385)
        (xy 100.152195 85.044548)
        (xy 100.150195 85.038354)
        (xy 100.148196 85.031803)
        (xy 100.146197 85.024895)
        (xy 100.144197 85.01763)
        (xy 100.142198 85.010008)
        (xy 100.140198 85.002029)
        (xy 100.138199 84.993693)
        (xy 100.1362 84.985)
      )
    )
  )
  (zone (net 28) (net_name "/GPIO23") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30089)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 98.9362 92.815)
        (xy 98.938199 92.806306)
        (xy 98.940198 92.79797)
        (xy 98.942198 92.789991)
        (xy 98.944197 92.782369)
        (xy 98.946197 92.775104)
        (xy 98.948196 92.768196)
        (xy 98.950195 92.761645)
        (xy 98.952195 92.755451)
        (xy 98.954194 92.749614)
        (xy 98.956194 92.744134)
        (xy 98.86 92.3365)
        (xy 98.763806 92.744134)
        (xy 98.765805 92.749614)
        (xy 98.767804 92.755451)
        (xy 98.769804 92.761645)
        (xy 98.771803 92.768196)
        (xy 98.773803 92.775104)
        (xy 98.775802 92.782369)
        (xy 98.777801 92.789991)
        (xy 98.779801 92.79797)
        (xy 98.7818 92.806306)
        (xy 98.7838 92.815)
      )
    )
  )
  (zone (net 13) (net_name "/GPIO8") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30030)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 95.3262 81.2)
        (xy 95.333364 81.09519)
        (xy 95.354008 81.014058)
        (xy 95.386851 80.95155)
        (xy 95.430617 80.902614)
        (xy 95.484028 80.862196)
        (xy 95.545807 80.825244)
        (xy 95.614675 80.786706)
        (xy 95.689355 80.741527)
        (xy 95.76857 80.684657)
        (xy 95.851041 80.611041)
        (xy 95.25 80.009)
        (xy 94.648959 80.611041)
        (xy 94.731429 80.684657)
        (xy 94.810643 80.741527)
        (xy 94.885323 80.786706)
        (xy 94.954192 80.825244)
        (xy 95.01597 80.862196)
        (xy 95.069382 80.902614)
        (xy 95.113148 80.95155)
        (xy 95.145991 81.014058)
        (xy 95.166635 81.09519)
        (xy 95.1738 81.2)
      )
    )
  )
  (zone (net 48) (net_name "DP") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30045)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 107.148 89.5238)
        (xy 107.133944 89.512499)
        (xy 107.119889 89.499404)
        (xy 107.105834 89.484512)
        (xy 107.091779 89.467826)
        (xy 107.077724 89.449343)
        (xy 107.063668 89.429066)
        (xy 107.049613 89.406992)
        (xy 107.035558 89.383124)
        (xy 107.021503 89.357459)
        (xy 107.007448 89.33)
        (xy 106.769 89.6)
        (xy 107.007448 89.87)
        (xy 107.021503 89.84254)
        (xy 107.035558 89.816876)
        (xy 107.049613 89.793007)
        (xy 107.063668 89.770934)
        (xy 107.077724 89.750656)
        (xy 107.091779 89.732173)
        (xy 107.105834 89.715487)
        (xy 107.119889 89.700596)
        (xy 107.133944 89.6875)
        (xy 107.148 89.6762)
      )
    )
  )
  (zone (net 50) (net_name "VREG_IN") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30000)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 122.936 96.6)
        (xy 122.926366 96.734863)
        (xy 122.899387 96.839783)
        (xy 122.857941 96.921956)
        (xy 122.80491 96.988577)
        (xy 122.743173 97.046844)
        (xy 122.675609 97.103951)
        (xy 122.605101 97.167096)
        (xy 122.534526 97.243475)
        (xy 122.466767 97.340284)
        (xy 122.404702 97.464719)
        (xy 123.19 97.791)
        (xy 123.975298 97.464719)
        (xy 123.913232 97.340284)
        (xy 123.845472 97.243475)
        (xy 123.774898 97.167096)
        (xy 123.704389 97.103951)
        (xy 123.636826 97.046844)
        (xy 123.575089 96.988577)
        (xy 123.522057 96.921956)
        (xy 123.480612 96.839783)
        (xy 123.453633 96.734863)
        (xy 123.444 96.6)
      )
    )
  )
  (zone (net 4) (net_name "IOVDD") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30109)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 102.975 89.0238)
        (xy 102.967913 89.023407)
        (xy 102.960826 89.022657)
        (xy 102.95374 89.02155)
        (xy 102.946653 89.020086)
        (xy 102.939567 89.018265)
        (xy 102.93248 89.016087)
        (xy 102.925393 89.013552)
        (xy 102.918307 89.01066)
        (xy 102.91122 89.007411)
        (xy 102.904134 89.003806)
        (xy 102.4965 89.1)
        (xy 102.904134 89.196194)
        (xy 102.91122 89.192588)
        (xy 102.918307 89.189339)
        (xy 102.925393 89.186447)
        (xy 102.93248 89.183912)
        (xy 102.939567 89.181734)
        (xy 102.946653 89.179913)
        (xy 102.95374 89.178449)
        (xy 102.960826 89.177342)
        (xy 102.967913 89.176592)
        (xy 102.975 89.1762)
      )
    )
  )
  (zone (net 7) (net_name "/GPIO2") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30031)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 110.5662 81.2)
        (xy 110.573364 81.09519)
        (xy 110.594008 81.014058)
        (xy 110.626851 80.95155)
        (xy 110.670617 80.902614)
        (xy 110.724028 80.862196)
        (xy 110.785807 80.825244)
        (xy 110.854675 80.786706)
        (xy 110.929355 80.741527)
        (xy 111.00857 80.684657)
        (xy 111.091041 80.611041)
        (xy 110.49 80.009)
        (xy 109.888959 80.611041)
        (xy 109.971429 80.684657)
        (xy 110.050643 80.741527)
        (xy 110.125323 80.786706)
        (xy 110.194192 80.825244)
        (xy 110.25597 80.862196)
        (xy 110.309382 80.902614)
        (xy 110.353148 80.95155)
        (xy 110.385991 81.014058)
        (xy 110.406635 81.09519)
        (xy 110.4138 81.2)
      )
    )
  )
  (zone (net 42) (net_name "SWCLK") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30002)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 78.66 86.2838)
        (xy 78.613551 86.245812)
        (xy 78.567103 86.201836)
        (xy 78.520655 86.151873)
        (xy 78.474207 86.095922)
        (xy 78.42776 86.033984)
        (xy 78.381312 85.966058)
        (xy 78.334864 85.892145)
        (xy 78.288416 85.812244)
        (xy 78.241968 85.726356)
        (xy 78.19552 85.63448)
        (xy 77.469 86.36)
        (xy 78.19552 87.08552)
        (xy 78.241968 86.993643)
        (xy 78.288416 86.907755)
        (xy 78.334864 86.827854)
        (xy 78.381312 86.753941)
        (xy 78.42776 86.686015)
        (xy 78.474207 86.624077)
        (xy 78.520655 86.568126)
        (xy 78.567103 86.518163)
        (xy 78.613551 86.474187)
        (xy 78.66 86.4362)
      )
    )
  )
  (zone (net 4) (net_name "IOVDD") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30061)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 98.1362 83.972758)
        (xy 98.135578 83.935565)
        (xy 98.133891 83.904984)
        (xy 98.131404 83.87936)
        (xy 98.128385 83.857043)
        (xy 98.1251 83.836378)
        (xy 98.121814 83.815713)
        (xy 98.118795 83.793396)
        (xy 98.116308 83.767773)
        (xy 98.114621 83.737192)
        (xy 98.114 83.7)
        (xy 97.86 83.699)
        (xy 97.86 83.954)
        (xy 97.878679 83.952834)
        (xy 97.896915 83.94994)
        (xy 97.91435 83.946219)
        (xy 97.930623 83.942572)
        (xy 97.945377 83.939901)
        (xy 97.958252 83.939108)
        (xy 97.968891 83.941096)
        (xy 97.976934 83.946766)
        (xy 97.982023 83.957019)
        (xy 97.9838 83.972758)
      )
    )
  )
  (zone (net 18) (net_name "/GPIO13") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30021)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 82.6262 81.2)
        (xy 82.633364 81.09519)
        (xy 82.654008 81.014058)
        (xy 82.686851 80.95155)
        (xy 82.730617 80.902614)
        (xy 82.784028 80.862196)
        (xy 82.845807 80.825244)
        (xy 82.914675 80.786706)
        (xy 82.989355 80.741527)
        (xy 83.06857 80.684657)
        (xy 83.151041 80.611041)
        (xy 82.55 80.009)
        (xy 81.948959 80.611041)
        (xy 82.031429 80.684657)
        (xy 82.110643 80.741527)
        (xy 82.185323 80.786706)
        (xy 82.254192 80.825244)
        (xy 82.31597 80.862196)
        (xy 82.369382 80.902614)
        (xy 82.413148 80.95155)
        (xy 82.445991 81.014058)
        (xy 82.466635 81.09519)
        (xy 82.4738 81.2)
      )
    )
  )
  (zone (net 41) (net_name "XIN") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30004)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 82.6262 87.55)
        (xy 82.691132 87.476607)
        (xy 82.756064 87.409203)
        (xy 82.820996 87.347786)
        (xy 82.885928 87.292356)
        (xy 82.95086 87.242915)
        (xy 83.015792 87.199461)
        (xy 83.080724 87.161994)
        (xy 83.145656 87.130515)
        (xy 83.210588 87.105023)
        (xy 83.27552 87.08552)
        (xy 82.55 86.359)
        (xy 81.82448 87.08552)
        (xy 81.889412 87.105023)
        (xy 81.954344 87.130515)
        (xy 82.019275 87.161994)
        (xy 82.084208 87.199461)
        (xy 82.14914 87.242915)
        (xy 82.214072 87.292356)
        (xy 82.279004 87.347786)
        (xy 82.343936 87.409203)
        (xy 82.408868 87.476607)
        (xy 82.4738 87.55)
      )
    )
  )
  (zone (net 32) (net_name "/GPIO27") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30091)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 100.5362 92.815)
        (xy 100.538199 92.806306)
        (xy 100.540198 92.79797)
        (xy 100.542198 92.789991)
        (xy 100.544197 92.782369)
        (xy 100.546197 92.775104)
        (xy 100.548196 92.768196)
        (xy 100.550195 92.761645)
        (xy 100.552195 92.755451)
        (xy 100.554194 92.749614)
        (xy 100.556194 92.744134)
        (xy 100.46 92.3365)
        (xy 100.363806 92.744134)
        (xy 100.365805 92.749614)
        (xy 100.367804 92.755451)
        (xy 100.369804 92.761645)
        (xy 100.371803 92.768196)
        (xy 100.373803 92.775104)
        (xy 100.375802 92.782369)
        (xy 100.377801 92.789991)
        (xy 100.379801 92.79797)
        (xy 100.3818 92.806306)
        (xy 100.3838 92.815)
      )
    )
  )
  (zone (net 49) (net_name "ADC_AVDD") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30001)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 115.316 96.6)
        (xy 115.306366 96.734863)
        (xy 115.279387 96.839783)
        (xy 115.237941 96.921956)
        (xy 115.18491 96.988577)
        (xy 115.123173 97.046844)
        (xy 115.055609 97.103951)
        (xy 114.985101 97.167096)
        (xy 114.914526 97.243475)
        (xy 114.846767 97.340284)
        (xy 114.784702 97.464719)
        (xy 115.57 97.791)
        (xy 116.355298 97.464719)
        (xy 116.293232 97.340284)
        (xy 116.225472 97.243475)
        (xy 116.154898 97.167096)
        (xy 116.084389 97.103951)
        (xy 116.016826 97.046844)
        (xy 115.955089 96.988577)
        (xy 115.902057 96.921956)
        (xy 115.860612 96.839783)
        (xy 115.833633 96.734863)
        (xy 115.824 96.6)
      )
    )
  )
  (zone (net 4) (net_name "IOVDD") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30112)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 102.975 89.4238)
        (xy 102.967913 89.423407)
        (xy 102.960826 89.422657)
        (xy 102.95374 89.42155)
        (xy 102.946653 89.420086)
        (xy 102.939567 89.418265)
        (xy 102.93248 89.416087)
        (xy 102.925393 89.413552)
        (xy 102.918307 89.41066)
        (xy 102.91122 89.407411)
        (xy 102.904134 89.403806)
        (xy 102.4965 89.5)
        (xy 102.904134 89.596194)
        (xy 102.91122 89.592588)
        (xy 102.918307 89.589339)
        (xy 102.925393 89.586447)
        (xy 102.93248 89.583912)
        (xy 102.939567 89.581734)
        (xy 102.946653 89.579913)
        (xy 102.95374 89.578449)
        (xy 102.960826 89.577342)
        (xy 102.967913 89.576592)
        (xy 102.975 89.5762)
      )
    )
  )
  (zone (net 25) (net_name "/GPIO20") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30084)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 97.3362 92.815)
        (xy 97.338199 92.806306)
        (xy 97.340198 92.79797)
        (xy 97.342198 92.789991)
        (xy 97.344197 92.782369)
        (xy 97.346197 92.775104)
        (xy 97.348196 92.768196)
        (xy 97.350195 92.761645)
        (xy 97.352195 92.755451)
        (xy 97.354194 92.749614)
        (xy 97.356194 92.744134)
        (xy 97.26 92.3365)
        (xy 97.163806 92.744134)
        (xy 97.165805 92.749614)
        (xy 97.167804 92.755451)
        (xy 97.169804 92.761645)
        (xy 97.171803 92.768196)
        (xy 97.173803 92.775104)
        (xy 97.175802 92.782369)
        (xy 97.177801 92.789991)
        (xy 97.179801 92.79797)
        (xy 97.1818 92.806306)
        (xy 97.1838 92.815)
      )
    )
  )
  (zone (net 39) (net_name "/QSPI.D2") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30113)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 102.975 87.0238)
        (xy 102.967913 87.023407)
        (xy 102.960826 87.022657)
        (xy 102.95374 87.02155)
        (xy 102.946653 87.020086)
        (xy 102.939567 87.018265)
        (xy 102.93248 87.016087)
        (xy 102.925393 87.013552)
        (xy 102.918307 87.01066)
        (xy 102.91122 87.007411)
        (xy 102.904134 87.003806)
        (xy 102.4965 87.1)
        (xy 102.904134 87.196194)
        (xy 102.91122 87.192588)
        (xy 102.918307 87.189339)
        (xy 102.925393 87.186447)
        (xy 102.93248 87.183912)
        (xy 102.939567 87.181734)
        (xy 102.946653 87.179913)
        (xy 102.95374 87.178449)
        (xy 102.960826 87.177342)
        (xy 102.967913 87.176592)
        (xy 102.975 87.1762)
      )
    )
  )
  (zone (net 51) (net_name "VBUS") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30063)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 122.783 90.48)
        (xy 122.790299 90.468344)
        (xy 122.797599 90.457502)
        (xy 122.804899 90.447471)
        (xy 122.812199 90.438253)
        (xy 122.8195 90.429847)
        (xy 122.8268 90.422253)
        (xy 122.8341 90.415471)
        (xy 122.8414 90.409502)
        (xy 122.8487 90.404345)
        (xy 122.856 90.4)
        (xy 122.656 90.199)
        (xy 122.456 90.4)
        (xy 122.463299 90.404345)
        (xy 122.470599 90.409502)
        (xy 122.477899 90.415471)
        (xy 122.485199 90.422253)
        (xy 122.4925 90.429847)
        (xy 122.4998 90.438253)
        (xy 122.5071 90.447471)
        (xy 122.5144 90.457502)
        (xy 122.5217 90.468344)
        (xy 122.529 90.48)
      )
    )
  )
  (zone (net 24) (net_name "/GPIO19") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30080)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 96.9362 92.815)
        (xy 96.938199 92.806306)
        (xy 96.940198 92.79797)
        (xy 96.942198 92.789991)
        (xy 96.944197 92.782369)
        (xy 96.946197 92.775104)
        (xy 96.948196 92.768196)
        (xy 96.950195 92.761645)
        (xy 96.952195 92.755451)
        (xy 96.954194 92.749614)
        (xy 96.956194 92.744134)
        (xy 96.86 92.3365)
        (xy 96.763806 92.744134)
        (xy 96.765805 92.749614)
        (xy 96.767804 92.755451)
        (xy 96.769804 92.761645)
        (xy 96.771803 92.768196)
        (xy 96.773803 92.775104)
        (xy 96.775802 92.782369)
        (xy 96.777801 92.789991)
        (xy 96.779801 92.79797)
        (xy 96.7818 92.806306)
        (xy 96.7838 92.815)
      )
    )
  )
  (zone (net 44) (net_name "SWDIO") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30092)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 95.145 90.3762)
        (xy 95.152086 90.376592)
        (xy 95.159173 90.377342)
        (xy 95.166259 90.378449)
        (xy 95.173346 90.379913)
        (xy 95.180433 90.381734)
        (xy 95.187519 90.383912)
        (xy 95.194606 90.386447)
        (xy 95.201692 90.389339)
        (xy 95.208779 90.392588)
        (xy 95.215866 90.396194)
        (xy 95.6235 90.3)
        (xy 95.215866 90.203806)
        (xy 95.208779 90.207411)
        (xy 95.201692 90.21066)
        (xy 95.194606 90.213552)
        (xy 95.187519 90.216087)
        (xy 95.180433 90.218265)
        (xy 95.173346 90.220086)
        (xy 95.166259 90.22155)
        (xy 95.159173 90.222657)
        (xy 95.152086 90.223407)
        (xy 95.145 90.2238)
      )
    )
  )
  (zone (net 46) (net_name "DVDD") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30094)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 102.02 90.7762)
        (xy 102.027086 90.776592)
        (xy 102.034173 90.777342)
        (xy 102.041259 90.778449)
        (xy 102.048346 90.779913)
        (xy 102.055433 90.781734)
        (xy 102.062519 90.783912)
        (xy 102.069606 90.786447)
        (xy 102.076692 90.789339)
        (xy 102.083779 90.792588)
        (xy 102.090866 90.796194)
        (xy 102.4985 90.7)
        (xy 102.090866 90.603806)
        (xy 102.083779 90.607411)
        (xy 102.076692 90.61066)
        (xy 102.069606 90.613552)
        (xy 102.062519 90.616087)
        (xy 102.055433 90.618265)
        (xy 102.048346 90.620086)
        (xy 102.041259 90.62155)
        (xy 102.034173 90.622657)
        (xy 102.027086 90.623407)
        (xy 102.02 90.6238)
      )
    )
  )
  (zone (net 4) (net_name "IOVDD") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30064)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 97.9838 84.985)
        (xy 97.9818 84.993693)
        (xy 97.979801 85.002029)
        (xy 97.977801 85.010008)
        (xy 97.975802 85.01763)
        (xy 97.973803 85.024895)
        (xy 97.971803 85.031803)
        (xy 97.969804 85.038354)
        (xy 97.967804 85.044548)
        (xy 97.965805 85.050385)
        (xy 97.963806 85.055866)
        (xy 98.06 85.4635)
        (xy 98.156194 85.055866)
        (xy 98.154194 85.050385)
        (xy 98.152195 85.044548)
        (xy 98.150195 85.038354)
        (xy 98.148196 85.031803)
        (xy 98.146197 85.024895)
        (xy 98.144197 85.01763)
        (xy 98.142198 85.010008)
        (xy 98.140198 85.002029)
        (xy 98.138199 84.993693)
        (xy 98.1362 84.985)
      )
    )
  )
  (zone (net 26) (net_name "/GPIO21") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30012)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 90.0938 96.6)
        (xy 90.086635 96.704808)
        (xy 90.065991 96.78594)
        (xy 90.033148 96.848448)
        (xy 89.989382 96.897384)
        (xy 89.93597 96.937802)
        (xy 89.874192 96.974754)
        (xy 89.805323 97.013293)
        (xy 89.730643 97.058471)
        (xy 89.651429 97.115342)
        (xy 89.568959 97.188959)
        (xy 90.17 97.791)
        (xy 90.771041 97.188959)
        (xy 90.68857 97.115342)
        (xy 90.609355 97.058471)
        (xy 90.534675 97.013293)
        (xy 90.465807 96.974754)
        (xy 90.404028 96.937802)
        (xy 90.350617 96.897384)
        (xy 90.306851 96.848448)
        (xy 90.274008 96.78594)
        (xy 90.253364 96.704808)
        (xy 90.2462 96.6)
      )
    )
  )
  (zone (net 40) (net_name "/QSPI.D1") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30050)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 105.7044 85.5762)
        (xy 105.744683 85.579071)
        (xy 105.776029 85.587112)
        (xy 105.800587 85.599466)
        (xy 105.820502 85.615275)
        (xy 105.837925 85.633682)
        (xy 105.855 85.653829)
        (xy 105.873878 85.674858)
        (xy 105.896705 85.695912)
        (xy 105.925629 85.716133)
        (xy 105.962798 85.734665)
        (xy 106.061 85.5)
        (xy 105.962798 85.265335)
        (xy 105.925629 85.283865)
        (xy 105.896705 85.304086)
        (xy 105.873878 85.32514)
        (xy 105.855 85.34617)
        (xy 105.837925 85.366317)
        (xy 105.820502 85.384724)
        (xy 105.800587 85.400533)
        (xy 105.776029 85.412887)
        (xy 105.744683 85.420928)
        (xy 105.7044 85.4238)
      )
    )
  )
  (zone (net 17) (net_name "/GPIO12") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30103)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 95.145 86.3762)
        (xy 95.152086 86.376592)
        (xy 95.159173 86.377342)
        (xy 95.166259 86.378449)
        (xy 95.173346 86.379913)
        (xy 95.180433 86.381734)
        (xy 95.187519 86.383912)
        (xy 95.194606 86.386447)
        (xy 95.201692 86.389339)
        (xy 95.208779 86.392588)
        (xy 95.215866 86.396194)
        (xy 95.6235 86.3)
        (xy 95.215866 86.203806)
        (xy 95.208779 86.207411)
        (xy 95.201692 86.21066)
        (xy 95.194606 86.213552)
        (xy 95.187519 86.216087)
        (xy 95.180433 86.218265)
        (xy 95.173346 86.220086)
        (xy 95.166259 86.22155)
        (xy 95.159173 86.222657)
        (xy 95.152086 86.223407)
        (xy 95.145 86.2238)
      )
    )
  )
  (zone (net 17) (net_name "/GPIO12") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30022)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 85.1662 81.2)
        (xy 85.173364 81.09519)
        (xy 85.194008 81.014058)
        (xy 85.226851 80.95155)
        (xy 85.270617 80.902614)
        (xy 85.324028 80.862196)
        (xy 85.385807 80.825244)
        (xy 85.454675 80.786706)
        (xy 85.529355 80.741527)
        (xy 85.60857 80.684657)
        (xy 85.691041 80.611041)
        (xy 85.09 80.009)
        (xy 84.488959 80.611041)
        (xy 84.571429 80.684657)
        (xy 84.650643 80.741527)
        (xy 84.725323 80.786706)
        (xy 84.794192 80.825244)
        (xy 84.85597 80.862196)
        (xy 84.909382 80.902614)
        (xy 84.953148 80.95155)
        (xy 84.985991 81.014058)
        (xy 85.006635 81.09519)
        (xy 85.0138 81.2)
      )
    )
  )
  (zone (net 41) (net_name "XIN") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30098)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 95.145 88.3762)
        (xy 95.152086 88.376592)
        (xy 95.159173 88.377342)
        (xy 95.166259 88.378449)
        (xy 95.173346 88.379913)
        (xy 95.180433 88.381734)
        (xy 95.187519 88.383912)
        (xy 95.194606 88.386447)
        (xy 95.201692 88.389339)
        (xy 95.208779 88.392588)
        (xy 95.215866 88.396194)
        (xy 95.6235 88.3)
        (xy 95.215866 88.203806)
        (xy 95.208779 88.207411)
        (xy 95.201692 88.21066)
        (xy 95.194606 88.213552)
        (xy 95.187519 88.216087)
        (xy 95.180433 88.218265)
        (xy 95.173346 88.220086)
        (xy 95.166259 88.22155)
        (xy 95.159173 88.222657)
        (xy 95.152086 88.223407)
        (xy 95.145 88.2238)
      )
    )
  )
  (zone (net 3) (net_name "Net-(X1-ID)") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30042)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 121.876 88.3262)
        (xy 121.884 88.333605)
        (xy 121.892 88.342116)
        (xy 121.9 88.351732)
        (xy 121.908 88.362454)
        (xy 121.916 88.374282)
        (xy 121.923999 88.387214)
        (xy 121.931999 88.401252)
        (xy 121.939999 88.416396)
        (xy 121.947999 88.432645)
        (xy 121.956 88.45)
        (xy 122.657 88.25)
        (xy 121.956 88.05)
        (xy 121.947999 88.067354)
        (xy 121.939999 88.083603)
        (xy 121.931999 88.098747)
        (xy 121.923999 88.112785)
        (xy 121.916 88.125718)
        (xy 121.908 88.137545)
        (xy 121.9 88.148267)
        (xy 121.892 88.157883)
        (xy 121.884 88.166394)
        (xy 121.876 88.1738)
      )
    )
  )
  (zone (net 40) (net_name "/QSPI.D1") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30111)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 102.975 86.6238)
        (xy 102.967913 86.623407)
        (xy 102.960826 86.622657)
        (xy 102.95374 86.62155)
        (xy 102.946653 86.620086)
        (xy 102.939567 86.618265)
        (xy 102.93248 86.616087)
        (xy 102.925393 86.613552)
        (xy 102.918307 86.61066)
        (xy 102.91122 86.607411)
        (xy 102.904134 86.603806)
        (xy 102.4965 86.7)
        (xy 102.904134 86.796194)
        (xy 102.91122 86.792588)
        (xy 102.918307 86.789339)
        (xy 102.925393 86.786447)
        (xy 102.93248 86.783912)
        (xy 102.939567 86.781734)
        (xy 102.946653 86.779913)
        (xy 102.95374 86.778449)
        (xy 102.960826 86.777342)
        (xy 102.967913 86.776592)
        (xy 102.975 86.7762)
      )
    )
  )
  (zone (net 7) (net_name "/GPIO2") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30075)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 100.3838 84.985)
        (xy 100.3818 84.993693)
        (xy 100.379801 85.002029)
        (xy 100.377801 85.010008)
        (xy 100.375802 85.01763)
        (xy 100.373803 85.024895)
        (xy 100.371803 85.031803)
        (xy 100.369804 85.038354)
        (xy 100.367804 85.044548)
        (xy 100.365805 85.050385)
        (xy 100.363806 85.055866)
        (xy 100.46 85.4635)
        (xy 100.556194 85.055866)
        (xy 100.554194 85.050385)
        (xy 100.552195 85.044548)
        (xy 100.550195 85.038354)
        (xy 100.548196 85.031803)
        (xy 100.546197 85.024895)
        (xy 100.544197 85.01763)
        (xy 100.542198 85.010008)
        (xy 100.540198 85.002029)
        (xy 100.538199 84.993693)
        (xy 100.5362 84.985)
      )
    )
  )
  (zone (net 33) (net_name "/GPIO28") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30088)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 100.9362 92.815)
        (xy 100.938199 92.806306)
        (xy 100.940198 92.79797)
        (xy 100.942198 92.789991)
        (xy 100.944197 92.782369)
        (xy 100.946197 92.775104)
        (xy 100.948196 92.768196)
        (xy 100.950195 92.761645)
        (xy 100.952195 92.755451)
        (xy 100.954194 92.749614)
        (xy 100.956194 92.744134)
        (xy 100.86 92.3365)
        (xy 100.763806 92.744134)
        (xy 100.765805 92.749614)
        (xy 100.767804 92.755451)
        (xy 100.769804 92.761645)
        (xy 100.771803 92.768196)
        (xy 100.773803 92.775104)
        (xy 100.775802 92.782369)
        (xy 100.777801 92.789991)
        (xy 100.779801 92.79797)
        (xy 100.7818 92.806306)
        (xy 100.7838 92.815)
      )
    )
  )
  (zone (net 35) (net_name "/QSPI.SCLK") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30117)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 102.975 87.8238)
        (xy 102.967913 87.823407)
        (xy 102.960826 87.822657)
        (xy 102.95374 87.82155)
        (xy 102.946653 87.820086)
        (xy 102.939567 87.818265)
        (xy 102.93248 87.816087)
        (xy 102.925393 87.813552)
        (xy 102.918307 87.81066)
        (xy 102.91122 87.807411)
        (xy 102.904134 87.803806)
        (xy 102.4965 87.9)
        (xy 102.904134 87.996194)
        (xy 102.91122 87.992588)
        (xy 102.918307 87.989339)
        (xy 102.925393 87.986447)
        (xy 102.93248 87.983912)
        (xy 102.939567 87.981734)
        (xy 102.946653 87.979913)
        (xy 102.95374 87.978449)
        (xy 102.960826 87.977342)
        (xy 102.967913 87.976592)
        (xy 102.975 87.9762)
      )
    )
  )
  (zone (net 50) (net_name "VREG_IN") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30051)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 104.5044 91.9762)
        (xy 104.544683 91.979071)
        (xy 104.576029 91.987112)
        (xy 104.600587 91.999466)
        (xy 104.620502 92.015275)
        (xy 104.637925 92.033682)
        (xy 104.655 92.053829)
        (xy 104.673878 92.074858)
        (xy 104.696705 92.095912)
        (xy 104.725629 92.116133)
        (xy 104.762798 92.134665)
        (xy 104.861 91.9)
        (xy 104.762798 91.665335)
        (xy 104.725629 91.683865)
        (xy 104.696705 91.704086)
        (xy 104.673878 91.72514)
        (xy 104.655 91.74617)
        (xy 104.637925 91.766317)
        (xy 104.620502 91.784724)
        (xy 104.600587 91.800533)
        (xy 104.576029 91.812887)
        (xy 104.544683 91.820928)
        (xy 104.5044 91.8238)
      )
    )
  )
  (zone (net 44) (net_name "SWDIO") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30038)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 78.66 91.3638)
        (xy 78.55519 91.356635)
        (xy 78.474058 91.335991)
        (xy 78.41155 91.303148)
        (xy 78.362614 91.259382)
        (xy 78.322196 91.20597)
        (xy 78.285244 91.144192)
        (xy 78.246706 91.075323)
        (xy 78.201527 91.000643)
        (xy 78.144657 90.921429)
        (xy 78.071041 90.838959)
        (xy 77.469 91.44)
        (xy 78.071041 92.041041)
        (xy 78.144657 91.95857)
        (xy 78.201527 91.879355)
        (xy 78.246706 91.804675)
        (xy 78.285244 91.735807)
        (xy 78.322196 91.674028)
        (xy 78.362614 91.620617)
        (xy 78.41155 91.576851)
        (xy 78.474058 91.544008)
        (xy 78.55519 91.523364)
        (xy 78.66 91.5162)
      )
    )
  )
  (zone (net 27) (net_name "/GPIO22") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30078)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 98.5362 92.815)
        (xy 98.538199 92.806306)
        (xy 98.540198 92.79797)
        (xy 98.542198 92.789991)
        (xy 98.544197 92.782369)
        (xy 98.546197 92.775104)
        (xy 98.548196 92.768196)
        (xy 98.550195 92.761645)
        (xy 98.552195 92.755451)
        (xy 98.554194 92.749614)
        (xy 98.556194 92.744134)
        (xy 98.46 92.3365)
        (xy 98.363806 92.744134)
        (xy 98.365805 92.749614)
        (xy 98.367804 92.755451)
        (xy 98.369804 92.761645)
        (xy 98.371803 92.768196)
        (xy 98.373803 92.775104)
        (xy 98.375802 92.782369)
        (xy 98.377801 92.789991)
        (xy 98.379801 92.79797)
        (xy 98.3818 92.806306)
        (xy 98.3838 92.815)
      )
    )
  )
  (zone (net 15) (net_name "/GPIO10") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30068)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 96.7838 84.985)
        (xy 96.7818 84.993693)
        (xy 96.779801 85.002029)
        (xy 96.777801 85.010008)
        (xy 96.775802 85.01763)
        (xy 96.773803 85.024895)
        (xy 96.771803 85.031803)
        (xy 96.769804 85.038354)
        (xy 96.767804 85.044548)
        (xy 96.765805 85.050385)
        (xy 96.763806 85.055866)
        (xy 96.86 85.4635)
        (xy 96.956194 85.055866)
        (xy 96.954194 85.050385)
        (xy 96.952195 85.044548)
        (xy 96.950195 85.038354)
        (xy 96.948196 85.031803)
        (xy 96.946197 85.024895)
        (xy 96.944197 85.01763)
        (xy 96.942198 85.010008)
        (xy 96.940198 85.002029)
        (xy 96.938199 84.993693)
        (xy 96.9362 84.985)
      )
    )
  )
  (zone (net 6) (net_name "/GPIO1") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30076)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 100.7838 84.985)
        (xy 100.7818 84.993693)
        (xy 100.779801 85.002029)
        (xy 100.777801 85.010008)
        (xy 100.775802 85.01763)
        (xy 100.773803 85.024895)
        (xy 100.771803 85.031803)
        (xy 100.769804 85.038354)
        (xy 100.767804 85.044548)
        (xy 100.765805 85.050385)
        (xy 100.763806 85.055866)
        (xy 100.86 85.4635)
        (xy 100.956194 85.055866)
        (xy 100.954194 85.050385)
        (xy 100.952195 85.044548)
        (xy 100.950195 85.038354)
        (xy 100.948196 85.031803)
        (xy 100.946197 85.024895)
        (xy 100.944197 85.01763)
        (xy 100.942198 85.010008)
        (xy 100.940198 85.002029)
        (xy 100.938199 84.993693)
        (xy 100.9362 84.985)
      )
    )
  )
  (zone (net 12) (net_name "/GPIO7") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30026)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 97.8662 81.2)
        (xy 97.873364 81.09519)
        (xy 97.894008 81.014058)
        (xy 97.926851 80.95155)
        (xy 97.970617 80.902614)
        (xy 98.024028 80.862196)
        (xy 98.085807 80.825244)
        (xy 98.154675 80.786706)
        (xy 98.229355 80.741527)
        (xy 98.30857 80.684657)
        (xy 98.391041 80.611041)
        (xy 97.79 80.009)
        (xy 97.188959 80.611041)
        (xy 97.271429 80.684657)
        (xy 97.350643 80.741527)
        (xy 97.425323 80.786706)
        (xy 97.494192 80.825244)
        (xy 97.55597 80.862196)
        (xy 97.609382 80.902614)
        (xy 97.653148 80.95155)
        (xy 97.685991 81.014058)
        (xy 97.706635 81.09519)
        (xy 97.7138 81.2)
      )
    )
  )
  (zone (net 49) (net_name "ADC_AVDD") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30107)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 102.975 91.4238)
        (xy 102.967913 91.423407)
        (xy 102.960826 91.422657)
        (xy 102.95374 91.42155)
        (xy 102.946653 91.420086)
        (xy 102.939567 91.418265)
        (xy 102.93248 91.416087)
        (xy 102.925393 91.413552)
        (xy 102.918307 91.41066)
        (xy 102.91122 91.407411)
        (xy 102.904134 91.403806)
        (xy 102.4965 91.5)
        (xy 102.904134 91.596194)
        (xy 102.91122 91.592588)
        (xy 102.918307 91.589339)
        (xy 102.925393 91.586447)
        (xy 102.93248 91.583912)
        (xy 102.939567 91.581734)
        (xy 102.946653 91.579913)
        (xy 102.95374 91.578449)
        (xy 102.960826 91.577342)
        (xy 102.967913 91.576592)
        (xy 102.975 91.5762)
      )
    )
  )
  (zone (net 2) (net_name "Net-(U1-USB_DM)") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30044)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 105.372 90.6762)
        (xy 105.386055 90.6875)
        (xy 105.40011 90.700596)
        (xy 105.414165 90.715487)
        (xy 105.42822 90.732174)
        (xy 105.442276 90.750656)
        (xy 105.456331 90.770934)
        (xy 105.470386 90.793007)
        (xy 105.484441 90.816876)
        (xy 105.498496 90.84254)
        (xy 105.512552 90.87)
        (xy 105.751 90.6)
        (xy 105.512552 90.33)
        (xy 105.498496 90.357459)
        (xy 105.484441 90.383124)
        (xy 105.470386 90.406992)
        (xy 105.456331 90.429066)
        (xy 105.442276 90.449343)
        (xy 105.42822 90.467826)
        (xy 105.414165 90.484512)
        (xy 105.40011 90.499404)
        (xy 105.386055 90.512499)
        (xy 105.372 90.5238)
      )
    )
  )
  (zone (net 14) (net_name "/GPIO9") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30020)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 92.7862 81.2)
        (xy 92.793364 81.09519)
        (xy 92.814008 81.014058)
        (xy 92.846851 80.95155)
        (xy 92.890617 80.902614)
        (xy 92.944028 80.862196)
        (xy 93.005807 80.825244)
        (xy 93.074675 80.786706)
        (xy 93.149355 80.741527)
        (xy 93.22857 80.684657)
        (xy 93.311041 80.611041)
        (xy 92.71 80.009)
        (xy 92.108959 80.611041)
        (xy 92.191429 80.684657)
        (xy 92.270643 80.741527)
        (xy 92.345323 80.786706)
        (xy 92.414192 80.825244)
        (xy 92.47597 80.862196)
        (xy 92.529382 80.902614)
        (xy 92.573148 80.95155)
        (xy 92.605991 81.014058)
        (xy 92.626635 81.09519)
        (xy 92.6338 81.2)
      )
    )
  )
  (zone (net 46) (net_name "DVDD") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30053)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 96.7362 89.2556)
        (xy 96.739071 89.215316)
        (xy 96.747112 89.18397)
        (xy 96.759466 89.159412)
        (xy 96.775275 89.139496)
        (xy 96.793682 89.122074)
        (xy 96.813829 89.104998)
        (xy 96.834858 89.086121)
        (xy 96.855912 89.063294)
        (xy 96.876133 89.03437)
        (xy 96.894665 88.997202)
        (xy 96.66 88.899)
        (xy 96.425335 88.997202)
        (xy 96.443865 89.03437)
        (xy 96.464086 89.063294)
        (xy 96.48514 89.086121)
        (xy 96.50617 89.104998)
        (xy 96.526317 89.122074)
        (xy 96.544724 89.139496)
        (xy 96.560533 89.159412)
        (xy 96.572887 89.18397)
        (xy 96.580928 89.215316)
        (xy 96.5838 89.2556)
      )
    )
  )
  (zone (net 20) (net_name "/GPIO15") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30093)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 95.145 87.5762)
        (xy 95.152086 87.576592)
        (xy 95.159173 87.577342)
        (xy 95.166259 87.578449)
        (xy 95.173346 87.579913)
        (xy 95.180433 87.581734)
        (xy 95.187519 87.583912)
        (xy 95.194606 87.586447)
        (xy 95.201692 87.589339)
        (xy 95.208779 87.592588)
        (xy 95.215866 87.596194)
        (xy 95.6235 87.5)
        (xy 95.215866 87.403806)
        (xy 95.208779 87.407411)
        (xy 95.201692 87.41066)
        (xy 95.194606 87.413552)
        (xy 95.187519 87.416087)
        (xy 95.180433 87.418265)
        (xy 95.173346 87.420086)
        (xy 95.166259 87.42155)
        (xy 95.159173 87.422657)
        (xy 95.152086 87.423407)
        (xy 95.145 87.4238)
      )
    )
  )
  (zone (net 4) (net_name "IOVDD") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30059)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 97.9838 93.827242)
        (xy 97.982023 93.84298)
        (xy 97.976934 93.853233)
        (xy 97.968891 93.858902)
        (xy 97.958252 93.86089)
        (xy 97.945377 93.860098)
        (xy 97.930623 93.857427)
        (xy 97.91435 93.85378)
        (xy 97.896915 93.850059)
        (xy 97.878679 93.847165)
        (xy 97.86 93.846)
        (xy 97.86 94.101)
        (xy 98.114 94.1)
        (xy 98.114621 94.062807)
        (xy 98.116308 94.032226)
        (xy 98.118795 94.006602)
        (xy 98.121814 93.984285)
        (xy 98.1251 93.96362)
        (xy 98.128385 93.942955)
        (xy 98.131404 93.920638)
        (xy 98.133891 93.895015)
        (xy 98.135578 93.864434)
        (xy 98.1362 93.827242)
      )
    )
  )
  (zone (net 21) (net_name "/GPIO16") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30100)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 95.145 91.1762)
        (xy 95.152086 91.176592)
        (xy 95.159173 91.177342)
        (xy 95.166259 91.178449)
        (xy 95.173346 91.179913)
        (xy 95.180433 91.181734)
        (xy 95.187519 91.183912)
        (xy 95.194606 91.186447)
        (xy 95.201692 91.189339)
        (xy 95.208779 91.192588)
        (xy 95.215866 91.196194)
        (xy 95.6235 91.1)
        (xy 95.215866 91.003806)
        (xy 95.208779 91.007411)
        (xy 95.201692 91.01066)
        (xy 95.194606 91.013552)
        (xy 95.187519 91.016087)
        (xy 95.180433 91.018265)
        (xy 95.173346 91.020086)
        (xy 95.166259 91.02155)
        (xy 95.159173 91.022657)
        (xy 95.152086 91.023407)
        (xy 95.145 91.0238)
      )
    )
  )
  (zone (net 36) (net_name "/QSPI.SS") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30035)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 120.7262 81.2)
        (xy 120.733364 81.09519)
        (xy 120.754008 81.014058)
        (xy 120.786851 80.95155)
        (xy 120.830617 80.902614)
        (xy 120.884028 80.862196)
        (xy 120.945807 80.825244)
        (xy 121.014675 80.786706)
        (xy 121.089355 80.741527)
        (xy 121.16857 80.684657)
        (xy 121.251041 80.611041)
        (xy 120.65 80.009)
        (xy 120.048959 80.611041)
        (xy 120.131429 80.684657)
        (xy 120.210643 80.741527)
        (xy 120.285323 80.786706)
        (xy 120.354192 80.825244)
        (xy 120.41597 80.862196)
        (xy 120.469382 80.902614)
        (xy 120.513148 80.95155)
        (xy 120.545991 81.014058)
        (xy 120.566635 81.09519)
        (xy 120.5738 81.2)
      )
    )
  )
  (zone (net 31) (net_name "/GPIO26") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30006)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 102.738337 96.6861)
        (xy 102.790859 96.752711)
        (xy 102.806259 96.808439)
        (xy 102.790169 96.856004)
        (xy 102.748222 96.898127)
        (xy 102.68605 96.937529)
        (xy 102.609286 96.97693)
        (xy 102.523562 97.019053)
        (xy 102.434511 97.066618)
        (xy 102.347766 97.122346)
        (xy 102.268959 97.188959)
        (xy 102.870707 97.790707)
        (xy 103.471041 97.188959)
        (xy 103.386817 97.105136)
        (xy 103.31708 97.036487)
        (xy 103.258207 96.979218)
        (xy 103.206578 96.929536)
        (xy 103.15857 96.883647)
        (xy 103.110562 96.837758)
        (xy 103.058932 96.788076)
        (xy 103.00006 96.730807)
        (xy 102.930323 96.662159)
        (xy 102.8461 96.578337)
      )
    )
  )
  (zone (net 11) (net_name "/GPIO6") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30007)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 100.263674 81.204089)
        (xy 100.35054 81.119303)
        (xy 100.423987 81.051504)
        (xy 100.487368 80.996446)
        (xy 100.54404 80.949882)
        (xy 100.597357 80.907564)
        (xy 100.650673 80.865247)
        (xy 100.707345 80.818682)
        (xy 100.770727 80.763625)
        (xy 100.844174 80.695826)
        (xy 100.931041 80.611041)
        (xy 100.330707 80.009293)
        (xy 99.728959 80.611041)
        (xy 99.802615 80.67399)
        (xy 99.883053 80.727325)
        (xy 99.96515 80.77345)
        (xy 100.043783 80.814768)
        (xy 100.113828 80.853683)
        (xy 100.170161 80.892597)
        (xy 100.207659 80.933915)
        (xy 100.221199 80.980041)
        (xy 100.205657 81.033376)
        (xy 100.155911 81.096326)
      )
    )
  )
  (zone (net 29) (net_name "/GPIO24") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30015)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 97.7138 96.6)
        (xy 97.706635 96.704808)
        (xy 97.685991 96.78594)
        (xy 97.653148 96.848448)
        (xy 97.609382 96.897384)
        (xy 97.55597 96.937802)
        (xy 97.494192 96.974754)
        (xy 97.425323 97.013293)
        (xy 97.350643 97.058471)
        (xy 97.271429 97.115342)
        (xy 97.188959 97.188959)
        (xy 97.79 97.791)
        (xy 98.391041 97.188959)
        (xy 98.30857 97.115342)
        (xy 98.229355 97.058471)
        (xy 98.154675 97.013293)
        (xy 98.085807 96.974754)
        (xy 98.024028 96.937802)
        (xy 97.970617 96.897384)
        (xy 97.926851 96.848448)
        (xy 97.894008 96.78594)
        (xy 97.873364 96.704808)
        (xy 97.8662 96.6)
      )
    )
  )
  (zone (net 18) (net_name "/GPIO13") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30102)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 95.145 86.7762)
        (xy 95.152086 86.776592)
        (xy 95.159173 86.777342)
        (xy 95.166259 86.778449)
        (xy 95.173346 86.779913)
        (xy 95.180433 86.781734)
        (xy 95.187519 86.783912)
        (xy 95.194606 86.786447)
        (xy 95.201692 86.789339)
        (xy 95.208779 86.792588)
        (xy 95.215866 86.796194)
        (xy 95.6235 86.7)
        (xy 95.215866 86.603806)
        (xy 95.208779 86.607411)
        (xy 95.201692 86.61066)
        (xy 95.194606 86.613552)
        (xy 95.187519 86.616087)
        (xy 95.180433 86.618265)
        (xy 95.173346 86.620086)
        (xy 95.166259 86.62155)
        (xy 95.159173 86.622657)
        (xy 95.152086 86.623407)
        (xy 95.145 86.6238)
      )
    )
  )
  (zone (net 31) (net_name "/GPIO26") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30085)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 100.1362 92.815)
        (xy 100.138199 92.806306)
        (xy 100.140198 92.79797)
        (xy 100.142198 92.789991)
        (xy 100.144197 92.782369)
        (xy 100.146197 92.775104)
        (xy 100.148196 92.768196)
        (xy 100.150195 92.761645)
        (xy 100.152195 92.755451)
        (xy 100.154194 92.749614)
        (xy 100.156194 92.744134)
        (xy 100.06 92.3365)
        (xy 99.963806 92.744134)
        (xy 99.965805 92.749614)
        (xy 99.967804 92.755451)
        (xy 99.969804 92.761645)
        (xy 99.971803 92.768196)
        (xy 99.973803 92.775104)
        (xy 99.975802 92.782369)
        (xy 99.977801 92.789991)
        (xy 99.979801 92.79797)
        (xy 99.9818 92.806306)
        (xy 99.9838 92.815)
      )
    )
  )
  (zone (net 2) (net_name "Net-(U1-USB_DM)") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30106)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 102.975 90.2238)
        (xy 102.967913 90.223407)
        (xy 102.960826 90.222657)
        (xy 102.95374 90.22155)
        (xy 102.946653 90.220086)
        (xy 102.939567 90.218265)
        (xy 102.93248 90.216087)
        (xy 102.925393 90.213552)
        (xy 102.918307 90.21066)
        (xy 102.91122 90.207411)
        (xy 102.904134 90.203806)
        (xy 102.4965 90.3)
        (xy 102.904134 90.396194)
        (xy 102.91122 90.392588)
        (xy 102.918307 90.389339)
        (xy 102.925393 90.386447)
        (xy 102.93248 90.383912)
        (xy 102.939567 90.381734)
        (xy 102.946653 90.379913)
        (xy 102.95374 90.378449)
        (xy 102.960826 90.377342)
        (xy 102.967913 90.376592)
        (xy 102.975 90.3762)
      )
    )
  )
  (zone (net 39) (net_name "/QSPI.D2") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30056)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 105.174191 86.693572)
        (xy 105.198839 86.67301)
        (xy 105.221224 86.662247)
        (xy 105.242181 86.659483)
        (xy 105.262545 86.662921)
        (xy 105.283154 86.670763)
        (xy 105.304841 86.68121)
        (xy 105.328444 86.692466)
        (xy 105.354798 86.702732)
        (xy 105.384739 86.71021)
        (xy 105.419103 86.713103)
        (xy 105.41981 86.458396)
        (xy 105.184438 86.361901)
        (xy 105.171781 86.394165)
        (xy 105.162158 86.421493)
        (xy 105.154502 86.444913)
        (xy 105.147748 86.465453)
        (xy 105.140828 86.484142)
        (xy 105.132677 86.502007)
        (xy 105.122227 86.520079)
        (xy 105.108414 86.539384)
        (xy 105.090169 86.560951)
        (xy 105.066428 86.585809)
      )
    )
  )
  (zone (net 1) (net_name "Net-(U1-USB_DP)") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30043)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 105.372 89.6762)
        (xy 105.386055 89.6875)
        (xy 105.40011 89.700596)
        (xy 105.414165 89.715487)
        (xy 105.42822 89.732174)
        (xy 105.442276 89.750656)
        (xy 105.456331 89.770934)
        (xy 105.470386 89.793007)
        (xy 105.484441 89.816876)
        (xy 105.498496 89.84254)
        (xy 105.512552 89.87)
        (xy 105.751 89.6)
        (xy 105.512552 89.33)
        (xy 105.498496 89.357459)
        (xy 105.484441 89.383124)
        (xy 105.470386 89.406992)
        (xy 105.456331 89.429066)
        (xy 105.442276 89.449343)
        (xy 105.42822 89.467826)
        (xy 105.414165 89.484512)
        (xy 105.40011 89.499404)
        (xy 105.386055 89.512499)
        (xy 105.372 89.5238)
      )
    )
  )
  (zone (net 25) (net_name "/GPIO20") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30009)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 87.5538 96.6)
        (xy 87.546635 96.704808)
        (xy 87.525991 96.78594)
        (xy 87.493148 96.848448)
        (xy 87.449382 96.897384)
        (xy 87.39597 96.937802)
        (xy 87.334192 96.974754)
        (xy 87.265323 97.013293)
        (xy 87.190643 97.058471)
        (xy 87.111429 97.115342)
        (xy 87.028959 97.188959)
        (xy 87.63 97.791)
        (xy 88.231041 97.188959)
        (xy 88.14857 97.115342)
        (xy 88.069355 97.058471)
        (xy 87.994675 97.013293)
        (xy 87.925807 96.974754)
        (xy 87.864028 96.937802)
        (xy 87.810617 96.897384)
        (xy 87.766851 96.848448)
        (xy 87.734008 96.78594)
        (xy 87.713364 96.704808)
        (xy 87.7062 96.6)
      )
    )
  )
  (zone (net 26) (net_name "/GPIO21") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30090)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 97.7362 92.815)
        (xy 97.738199 92.806306)
        (xy 97.740198 92.79797)
        (xy 97.742198 92.789991)
        (xy 97.744197 92.782369)
        (xy 97.746197 92.775104)
        (xy 97.748196 92.768196)
        (xy 97.750195 92.761645)
        (xy 97.752195 92.755451)
        (xy 97.754194 92.749614)
        (xy 97.756194 92.744134)
        (xy 97.66 92.3365)
        (xy 97.563806 92.744134)
        (xy 97.565805 92.749614)
        (xy 97.567804 92.755451)
        (xy 97.569804 92.761645)
        (xy 97.571803 92.768196)
        (xy 97.573803 92.775104)
        (xy 97.575802 92.782369)
        (xy 97.577801 92.789991)
        (xy 97.579801 92.79797)
        (xy 97.5818 92.806306)
        (xy 97.5838 92.815)
      )
    )
  )
  (zone (net 4) (net_name "IOVDD") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30104)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 95.145 89.1762)
        (xy 95.152086 89.176592)
        (xy 95.159173 89.177342)
        (xy 95.166259 89.178449)
        (xy 95.173346 89.179913)
        (xy 95.180433 89.181734)
        (xy 95.187519 89.183912)
        (xy 95.194606 89.186447)
        (xy 95.201692 89.189339)
        (xy 95.208779 89.192588)
        (xy 95.215866 89.196194)
        (xy 95.6235 89.1)
        (xy 95.215866 89.003806)
        (xy 95.208779 89.007411)
        (xy 95.201692 89.01066)
        (xy 95.194606 89.013552)
        (xy 95.187519 89.016087)
        (xy 95.180433 89.018265)
        (xy 95.173346 89.020086)
        (xy 95.166259 89.02155)
        (xy 95.159173 89.022657)
        (xy 95.152086 89.023407)
        (xy 95.145 89.0238)
      )
    )
  )
  (zone (net 47) (net_name "DM") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30040)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 121.876 89.6262)
        (xy 121.884 89.633605)
        (xy 121.892 89.642116)
        (xy 121.9 89.651732)
        (xy 121.908 89.662454)
        (xy 121.916 89.674282)
        (xy 121.923999 89.687214)
        (xy 121.931999 89.701252)
        (xy 121.939999 89.716396)
        (xy 121.947999 89.732645)
        (xy 121.956 89.75)
        (xy 122.657 89.55)
        (xy 121.956 89.35)
        (xy 121.947999 89.367354)
        (xy 121.939999 89.383603)
        (xy 121.931999 89.398747)
        (xy 121.923999 89.412785)
        (xy 121.916 89.425718)
        (xy 121.908 89.437545)
        (xy 121.9 89.448267)
        (xy 121.892 89.457883)
        (xy 121.884 89.466394)
        (xy 121.876 89.4738)
      )
    )
  )
  (zone (net 32) (net_name "/GPIO27") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30018)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 105.3338 96.6)
        (xy 105.326635 96.704808)
        (xy 105.305991 96.78594)
        (xy 105.273148 96.848448)
        (xy 105.229382 96.897384)
        (xy 105.17597 96.937802)
        (xy 105.114192 96.974754)
        (xy 105.045323 97.013293)
        (xy 104.970643 97.058471)
        (xy 104.891429 97.115342)
        (xy 104.808959 97.188959)
        (xy 105.41 97.791)
        (xy 106.011041 97.188959)
        (xy 105.92857 97.115342)
        (xy 105.849355 97.058471)
        (xy 105.774675 97.013293)
        (xy 105.705807 96.974754)
        (xy 105.644028 96.937802)
        (xy 105.590617 96.897384)
        (xy 105.546851 96.848448)
        (xy 105.514008 96.78594)
        (xy 105.493364 96.704808)
        (xy 105.4862 96.6)
      )
    )
  )
  (zone (net 9) (net_name "/GPIO4") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30025)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 105.4862 81.2)
        (xy 105.493364 81.09519)
        (xy 105.514008 81.014058)
        (xy 105.546851 80.95155)
        (xy 105.590617 80.902614)
        (xy 105.644028 80.862196)
        (xy 105.705807 80.825244)
        (xy 105.774675 80.786706)
        (xy 105.849355 80.741527)
        (xy 105.92857 80.684657)
        (xy 106.011041 80.611041)
        (xy 105.41 80.009)
        (xy 104.808959 80.611041)
        (xy 104.891429 80.684657)
        (xy 104.970643 80.741527)
        (xy 105.045323 80.786706)
        (xy 105.114192 80.825244)
        (xy 105.17597 80.862196)
        (xy 105.229382 80.902614)
        (xy 105.273148 80.95155)
        (xy 105.305991 81.014058)
        (xy 105.326635 81.09519)
        (xy 105.3338 81.2)
      )
    )
  )
  (zone (net 29) (net_name "/GPIO24") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30083)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 99.3362 92.815)
        (xy 99.338199 92.806306)
        (xy 99.340198 92.79797)
        (xy 99.342198 92.789991)
        (xy 99.344197 92.782369)
        (xy 99.346197 92.775104)
        (xy 99.348196 92.768196)
        (xy 99.350195 92.761645)
        (xy 99.352195 92.755451)
        (xy 99.354194 92.749614)
        (xy 99.356194 92.744134)
        (xy 99.26 92.3365)
        (xy 99.163806 92.744134)
        (xy 99.165805 92.749614)
        (xy 99.167804 92.755451)
        (xy 99.169804 92.761645)
        (xy 99.171803 92.768196)
        (xy 99.173803 92.775104)
        (xy 99.175802 92.782369)
        (xy 99.177801 92.789991)
        (xy 99.179801 92.79797)
        (xy 99.1818 92.806306)
        (xy 99.1838 92.815)
      )
    )
  )
  (zone (net 11) (net_name "/GPIO6") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30071)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 98.7838 84.985)
        (xy 98.7818 84.993693)
        (xy 98.779801 85.002029)
        (xy 98.777801 85.010008)
        (xy 98.775802 85.01763)
        (xy 98.773803 85.024895)
        (xy 98.771803 85.031803)
        (xy 98.769804 85.038354)
        (xy 98.767804 85.044548)
        (xy 98.765805 85.050385)
        (xy 98.763806 85.055866)
        (xy 98.86 85.4635)
        (xy 98.956194 85.055866)
        (xy 98.954194 85.050385)
        (xy 98.952195 85.044548)
        (xy 98.950195 85.038354)
        (xy 98.948196 85.031803)
        (xy 98.946197 85.024895)
        (xy 98.944197 85.01763)
        (xy 98.942198 85.010008)
        (xy 98.940198 85.002029)
        (xy 98.938199 84.993693)
        (xy 98.9362 84.985)
      )
    )
  )
  (zone (net 24) (net_name "/GPIO19") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30008)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 85.0138 96.6)
        (xy 85.006635 96.704808)
        (xy 84.985991 96.78594)
        (xy 84.953148 96.848448)
        (xy 84.909382 96.897384)
        (xy 84.85597 96.937802)
        (xy 84.794192 96.974754)
        (xy 84.725323 97.013293)
        (xy 84.650643 97.058471)
        (xy 84.571429 97.115342)
        (xy 84.488959 97.188959)
        (xy 85.09 97.791)
        (xy 85.691041 97.188959)
        (xy 85.60857 97.115342)
        (xy 85.529355 97.058471)
        (xy 85.454675 97.013293)
        (xy 85.385807 96.974754)
        (xy 85.324028 96.937802)
        (xy 85.270617 96.897384)
        (xy 85.226851 96.848448)
        (xy 85.194008 96.78594)
        (xy 85.173364 96.704808)
        (xy 85.1662 96.6)
      )
    )
  )
  (zone (net 16) (net_name "/GPIO11") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30070)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 96.3838 84.985)
        (xy 96.3818 84.993693)
        (xy 96.379801 85.002029)
        (xy 96.377801 85.010008)
        (xy 96.375802 85.01763)
        (xy 96.373803 85.024895)
        (xy 96.371803 85.031803)
        (xy 96.369804 85.038354)
        (xy 96.367804 85.044548)
        (xy 96.365805 85.050385)
        (xy 96.363806 85.055866)
        (xy 96.46 85.4635)
        (xy 96.556194 85.055866)
        (xy 96.554194 85.050385)
        (xy 96.552195 85.044548)
        (xy 96.550195 85.038354)
        (xy 96.548196 85.031803)
        (xy 96.546197 85.024895)
        (xy 96.544197 85.01763)
        (xy 96.542198 85.010008)
        (xy 96.540198 85.002029)
        (xy 96.538199 84.993693)
        (xy 96.5362 84.985)
      )
    )
  )
  (zone (net 27) (net_name "/GPIO22") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30013)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 92.6338 96.6)
        (xy 92.626635 96.704808)
        (xy 92.605991 96.78594)
        (xy 92.573148 96.848448)
        (xy 92.529382 96.897384)
        (xy 92.47597 96.937802)
        (xy 92.414192 96.974754)
        (xy 92.345323 97.013293)
        (xy 92.270643 97.058471)
        (xy 92.191429 97.115342)
        (xy 92.108959 97.188959)
        (xy 92.71 97.791)
        (xy 93.311041 97.188959)
        (xy 93.22857 97.115342)
        (xy 93.149355 97.058471)
        (xy 93.074675 97.013293)
        (xy 93.005807 96.974754)
        (xy 92.944028 96.937802)
        (xy 92.890617 96.897384)
        (xy 92.846851 96.848448)
        (xy 92.814008 96.78594)
        (xy 92.793364 96.704808)
        (xy 92.7862 96.6)
      )
    )
  )
  (zone (net 47) (net_name "DM") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30046)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 107.148 90.5238)
        (xy 107.133944 90.512499)
        (xy 107.119889 90.499404)
        (xy 107.105834 90.484512)
        (xy 107.091779 90.467826)
        (xy 107.077724 90.449343)
        (xy 107.063668 90.429066)
        (xy 107.049613 90.406992)
        (xy 107.035558 90.383124)
        (xy 107.021503 90.357459)
        (xy 107.007448 90.33)
        (xy 106.769 90.6)
        (xy 107.007448 90.87)
        (xy 107.021503 90.84254)
        (xy 107.035558 90.816876)
        (xy 107.049613 90.793007)
        (xy 107.063668 90.770934)
        (xy 107.077724 90.750656)
        (xy 107.091779 90.732173)
        (xy 107.105834 90.715487)
        (xy 107.119889 90.700596)
        (xy 107.133944 90.6875)
        (xy 107.148 90.6762)
      )
    )
  )
  (zone (net 21) (net_name "/GPIO16") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30003)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 77.3938 96.6)
        (xy 77.328868 96.673392)
        (xy 77.263936 96.740796)
        (xy 77.199003 96.802213)
        (xy 77.134072 96.857643)
        (xy 77.06914 96.907084)
        (xy 77.004208 96.950538)
        (xy 76.939276 96.988005)
        (xy 76.874344 97.019484)
        (xy 76.809412 97.044976)
        (xy 76.74448 97.06448)
        (xy 77.47 97.791)
        (xy 78.19552 97.06448)
        (xy 78.130588 97.044976)
        (xy 78.065656 97.019484)
        (xy 78.000724 96.988005)
        (xy 77.935792 96.950538)
        (xy 77.87086 96.907084)
        (xy 77.805928 96.857643)
        (xy 77.740996 96.802213)
        (xy 77.676064 96.740796)
        (xy 77.611132 96.673392)
        (xy 77.5462 96.6)
      )
    )
  )
  (zone (net 4) (net_name "IOVDD") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30081)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 98.1362 92.815)
        (xy 98.138199 92.806306)
        (xy 98.140198 92.79797)
        (xy 98.142198 92.789991)
        (xy 98.144197 92.782369)
        (xy 98.146197 92.775104)
        (xy 98.148196 92.768196)
        (xy 98.150195 92.761645)
        (xy 98.152195 92.755451)
        (xy 98.154194 92.749614)
        (xy 98.156194 92.744134)
        (xy 98.06 92.3365)
        (xy 97.963806 92.744134)
        (xy 97.965805 92.749614)
        (xy 97.967804 92.755451)
        (xy 97.969804 92.761645)
        (xy 97.971803 92.768196)
        (xy 97.973803 92.775104)
        (xy 97.975802 92.782369)
        (xy 97.977801 92.789991)
        (xy 97.979801 92.79797)
        (xy 97.9818 92.806306)
        (xy 97.9838 92.815)
      )
    )
  )
  (zone (net 15) (net_name "/GPIO10") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30027)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 90.2462 81.2)
        (xy 90.253364 81.09519)
        (xy 90.274008 81.014058)
        (xy 90.306851 80.95155)
        (xy 90.350617 80.902614)
        (xy 90.404028 80.862196)
        (xy 90.465807 80.825244)
        (xy 90.534675 80.786706)
        (xy 90.609355 80.741527)
        (xy 90.68857 80.684657)
        (xy 90.771041 80.611041)
        (xy 90.17 80.009)
        (xy 89.568959 80.611041)
        (xy 89.651429 80.684657)
        (xy 89.730643 80.741527)
        (xy 89.805323 80.786706)
        (xy 89.874192 80.825244)
        (xy 89.93597 80.862196)
        (xy 89.989382 80.902614)
        (xy 90.033148 80.95155)
        (xy 90.065991 81.014058)
        (xy 90.086635 81.09519)
        (xy 90.0938 81.2)
      )
    )
  )
  (zone (net 49) (net_name "ADC_AVDD") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30049)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 104.5044 93.1762)
        (xy 104.544683 93.179071)
        (xy 104.576029 93.187112)
        (xy 104.600587 93.199466)
        (xy 104.620502 93.215275)
        (xy 104.637925 93.233682)
        (xy 104.655 93.253829)
        (xy 104.673878 93.274858)
        (xy 104.696705 93.295912)
        (xy 104.725629 93.316133)
        (xy 104.762798 93.334665)
        (xy 104.861 93.1)
        (xy 104.762798 92.865335)
        (xy 104.725629 92.883865)
        (xy 104.696705 92.904086)
        (xy 104.673878 92.92514)
        (xy 104.655 92.94617)
        (xy 104.637925 92.966317)
        (xy 104.620502 92.984724)
        (xy 104.600587 93.000533)
        (xy 104.576029 93.012887)
        (xy 104.544683 93.020928)
        (xy 104.5044 93.0238)
      )
    )
  )
  (zone (net 5) (net_name "/GPIO0") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30033)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 115.6462 81.2)
        (xy 115.653364 81.09519)
        (xy 115.674008 81.014058)
        (xy 115.706851 80.95155)
        (xy 115.750617 80.902614)
        (xy 115.804028 80.862196)
        (xy 115.865807 80.825244)
        (xy 115.934675 80.786706)
        (xy 116.009355 80.741527)
        (xy 116.08857 80.684657)
        (xy 116.171041 80.611041)
        (xy 115.57 80.009)
        (xy 114.968959 80.611041)
        (xy 115.051429 80.684657)
        (xy 115.130643 80.741527)
        (xy 115.205323 80.786706)
        (xy 115.274192 80.825244)
        (xy 115.33597 80.862196)
        (xy 115.389382 80.902614)
        (xy 115.433148 80.95155)
        (xy 115.465991 81.014058)
        (xy 115.486635 81.09519)
        (xy 115.4938 81.2)
      )
    )
  )
  (zone (net 4) (net_name "IOVDD") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30062)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 94.732758 89.0238)
        (xy 94.717019 89.022023)
        (xy 94.706766 89.016934)
        (xy 94.701096 89.008891)
        (xy 94.699108 88.998252)
        (xy 94.699901 88.985377)
        (xy 94.702572 88.970623)
        (xy 94.706219 88.95435)
        (xy 94.70994 88.936915)
        (xy 94.712834 88.918679)
        (xy 94.714 88.9)
        (xy 94.459 88.9)
        (xy 94.46 89.154)
        (xy 94.497192 89.154621)
        (xy 94.527773 89.156308)
        (xy 94.553396 89.158795)
        (xy 94.575713 89.161814)
        (xy 94.596378 89.1651)
        (xy 94.617043 89.168385)
        (xy 94.63936 89.171404)
        (xy 94.664984 89.173891)
        (xy 94.695565 89.175578)
        (xy 94.732758 89.1762)
      )
    )
  )
  (zone (net 3) (net_name "Net-(X1-ID)") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30047)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 119.5362 87.248)
        (xy 119.55558 87.225864)
        (xy 119.57496 87.205525)
        (xy 119.594339 87.186981)
        (xy 119.61372 87.170233)
        (xy 119.6331 87.15528)
        (xy 119.65248 87.142122)
        (xy 119.67186 87.13076)
        (xy 119.69124 87.121194)
        (xy 119.71062 87.113423)
        (xy 119.73 87.107448)
        (xy 119.46 86.869)
        (xy 119.19 87.107448)
        (xy 119.20938 87.113423)
        (xy 119.22876 87.121194)
        (xy 119.24814 87.13076)
        (xy 119.26752 87.142122)
        (xy 119.2869 87.15528)
        (xy 119.30628 87.170233)
        (xy 119.32566 87.186981)
        (xy 119.34504 87.205525)
        (xy 119.36442 87.225864)
        (xy 119.3838 87.248)
      )
    )
  )
  (zone (net 30) (net_name "/GPIO25") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30016)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 100.2538 96.6)
        (xy 100.246635 96.704808)
        (xy 100.225991 96.78594)
        (xy 100.193148 96.848448)
        (xy 100.149382 96.897384)
        (xy 100.09597 96.937802)
        (xy 100.034192 96.974754)
        (xy 99.965323 97.013293)
        (xy 99.890643 97.058471)
        (xy 99.811429 97.115342)
        (xy 99.728959 97.188959)
        (xy 100.33 97.791)
        (xy 100.931041 97.188959)
        (xy 100.84857 97.115342)
        (xy 100.769355 97.058471)
        (xy 100.694675 97.013293)
        (xy 100.625807 96.974754)
        (xy 100.564028 96.937802)
        (xy 100.510617 96.897384)
        (xy 100.466851 96.848448)
        (xy 100.434008 96.78594)
        (xy 100.413364 96.704808)
        (xy 100.4062 96.6)
      )
    )
  )
  (zone (net 38) (net_name "/QSPI.D3") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30037)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 115.6462 87.55)
        (xy 115.653364 87.44519)
        (xy 115.674008 87.364058)
        (xy 115.706851 87.30155)
        (xy 115.750617 87.252614)
        (xy 115.804028 87.212196)
        (xy 115.865807 87.175244)
        (xy 115.934675 87.136706)
        (xy 116.009355 87.091527)
        (xy 116.08857 87.034657)
        (xy 116.171041 86.961041)
        (xy 115.57 86.359)
        (xy 114.968959 86.961041)
        (xy 115.051429 87.034657)
        (xy 115.130643 87.091527)
        (xy 115.205323 87.136706)
        (xy 115.274192 87.175244)
        (xy 115.33597 87.212196)
        (xy 115.389382 87.252614)
        (xy 115.433148 87.30155)
        (xy 115.465991 87.364058)
        (xy 115.486635 87.44519)
        (xy 115.4938 87.55)
      )
    )
  )
  (zone (net 46) (net_name "DVDD") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30105)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 96.1 89.4238)
        (xy 96.092913 89.423407)
        (xy 96.085826 89.422657)
        (xy 96.07874 89.42155)
        (xy 96.071653 89.420086)
        (xy 96.064567 89.418265)
        (xy 96.05748 89.416087)
        (xy 96.050393 89.413552)
        (xy 96.043307 89.41066)
        (xy 96.03622 89.407411)
        (xy 96.029134 89.403806)
        (xy 95.6215 89.5)
        (xy 96.029134 89.596194)
        (xy 96.03622 89.592588)
        (xy 96.043307 89.589339)
        (xy 96.050393 89.586447)
        (xy 96.05748 89.583912)
        (xy 96.064567 89.581734)
        (xy 96.071653 89.579913)
        (xy 96.07874 89.578449)
        (xy 96.085826 89.577342)
        (xy 96.092913 89.576592)
        (xy 96.1 89.5762)
      )
    )
  )
  (zone (net 23) (net_name "/GPIO18") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30079)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 96.5362 92.815)
        (xy 96.538199 92.806306)
        (xy 96.540198 92.79797)
        (xy 96.542198 92.789991)
        (xy 96.544197 92.782369)
        (xy 96.546197 92.775104)
        (xy 96.548196 92.768196)
        (xy 96.550195 92.761645)
        (xy 96.552195 92.755451)
        (xy 96.554194 92.749614)
        (xy 96.556194 92.744134)
        (xy 96.46 92.3365)
        (xy 96.363806 92.744134)
        (xy 96.365805 92.749614)
        (xy 96.367804 92.755451)
        (xy 96.369804 92.761645)
        (xy 96.371803 92.768196)
        (xy 96.373803 92.775104)
        (xy 96.375802 92.782369)
        (xy 96.377801 92.789991)
        (xy 96.379801 92.79797)
        (xy 96.3818 92.806306)
        (xy 96.3838 92.815)
      )
    )
  )
  (zone (net 4) (net_name "IOVDD") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30060)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 103.387242 89.1762)
        (xy 103.424434 89.175578)
        (xy 103.455015 89.173891)
        (xy 103.480638 89.171404)
        (xy 103.502955 89.168385)
        (xy 103.52362 89.1651)
        (xy 103.544285 89.161814)
        (xy 103.566602 89.158795)
        (xy 103.592226 89.156308)
        (xy 103.622807 89.154621)
        (xy 103.66 89.154)
        (xy 103.661 88.9)
        (xy 103.406 88.9)
        (xy 103.407165 88.918679)
        (xy 103.410059 88.936915)
        (xy 103.41378 88.95435)
        (xy 103.417427 88.970623)
        (xy 103.420098 88.985377)
        (xy 103.42089 88.998252)
        (xy 103.418902 89.008891)
        (xy 103.413233 89.016934)
        (xy 103.40298 89.022023)
        (xy 103.387242 89.0238)
      )
    )
  )
  (zone (net 19) (net_name "/GPIO14") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30101)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 95.145 87.1762)
        (xy 95.152086 87.176592)
        (xy 95.159173 87.177342)
        (xy 95.166259 87.178449)
        (xy 95.173346 87.179913)
        (xy 95.180433 87.181734)
        (xy 95.187519 87.183912)
        (xy 95.194606 87.186447)
        (xy 95.201692 87.189339)
        (xy 95.208779 87.192588)
        (xy 95.215866 87.196194)
        (xy 95.6235 87.1)
        (xy 95.215866 87.003806)
        (xy 95.208779 87.007411)
        (xy 95.201692 87.01066)
        (xy 95.194606 87.013552)
        (xy 95.187519 87.016087)
        (xy 95.180433 87.018265)
        (xy 95.173346 87.020086)
        (xy 95.166259 87.02155)
        (xy 95.159173 87.022657)
        (xy 95.152086 87.023407)
        (xy 95.145 87.0238)
      )
    )
  )
  (zone (net 48) (net_name "DP") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30041)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 121.876 88.9762)
        (xy 121.884 88.983605)
        (xy 121.892 88.992116)
        (xy 121.9 89.001732)
        (xy 121.908 89.012454)
        (xy 121.916 89.024282)
        (xy 121.923999 89.037214)
        (xy 121.931999 89.051252)
        (xy 121.939999 89.066396)
        (xy 121.947999 89.082645)
        (xy 121.956 89.1)
        (xy 122.657 88.9)
        (xy 121.956 88.7)
        (xy 121.947999 88.717354)
        (xy 121.939999 88.733603)
        (xy 121.931999 88.748747)
        (xy 121.923999 88.762785)
        (xy 121.916 88.775718)
        (xy 121.908 88.787545)
        (xy 121.9 88.798267)
        (xy 121.892 88.807883)
        (xy 121.884 88.816394)
        (xy 121.876 88.8238)
      )
    )
  )
  (zone (net 43) (net_name "RUN") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30095)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 95.145 90.7762)
        (xy 95.152086 90.776592)
        (xy 95.159173 90.777342)
        (xy 95.166259 90.778449)
        (xy 95.173346 90.779913)
        (xy 95.180433 90.781734)
        (xy 95.187519 90.783912)
        (xy 95.194606 90.786447)
        (xy 95.201692 90.789339)
        (xy 95.208779 90.792588)
        (xy 95.215866 90.796194)
        (xy 95.6235 90.7)
        (xy 95.215866 90.603806)
        (xy 95.208779 90.607411)
        (xy 95.201692 90.61066)
        (xy 95.194606 90.613552)
        (xy 95.187519 90.616087)
        (xy 95.180433 90.618265)
        (xy 95.173346 90.620086)
        (xy 95.166259 90.62155)
        (xy 95.159173 90.622657)
        (xy 95.152086 90.623407)
        (xy 95.145 90.6238)
      )
    )
  )
  (zone (net 23) (net_name "/GPIO18") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30010)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 82.4738 96.6)
        (xy 82.466635 96.704808)
        (xy 82.445991 96.78594)
        (xy 82.413148 96.848448)
        (xy 82.369382 96.897384)
        (xy 82.31597 96.937802)
        (xy 82.254192 96.974754)
        (xy 82.185323 97.013293)
        (xy 82.110643 97.058471)
        (xy 82.031429 97.115342)
        (xy 81.948959 97.188959)
        (xy 82.55 97.791)
        (xy 83.151041 97.188959)
        (xy 83.06857 97.115342)
        (xy 82.989355 97.058471)
        (xy 82.914675 97.013293)
        (xy 82.845807 96.974754)
        (xy 82.784028 96.937802)
        (xy 82.730617 96.897384)
        (xy 82.686851 96.848448)
        (xy 82.654008 96.78594)
        (xy 82.633364 96.704808)
        (xy 82.6262 96.6)
      )
    )
  )
  (zone (net 34) (net_name "/GPIO29") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30017)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 110.4138 96.6)
        (xy 110.406635 96.704808)
        (xy 110.385991 96.78594)
        (xy 110.353148 96.848448)
        (xy 110.309382 96.897384)
        (xy 110.25597 96.937802)
        (xy 110.194192 96.974754)
        (xy 110.125323 97.013293)
        (xy 110.050643 97.058471)
        (xy 109.971429 97.115342)
        (xy 109.888959 97.188959)
        (xy 110.49 97.791)
        (xy 111.091041 97.188959)
        (xy 111.00857 97.115342)
        (xy 110.929355 97.058471)
        (xy 110.854675 97.013293)
        (xy 110.785807 96.974754)
        (xy 110.724028 96.937802)
        (xy 110.670617 96.897384)
        (xy 110.626851 96.848448)
        (xy 110.594008 96.78594)
        (xy 110.573364 96.704808)
        (xy 110.5662 96.6)
      )
    )
  )
  (zone (net 51) (net_name "VBUS") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30005)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 125.603 96.6)
        (xy 125.596943 96.701131)
        (xy 125.57936 96.780749)
        (xy 125.551126 96.843401)
        (xy 125.513119 96.893634)
        (xy 125.466216 96.935998)
        (xy 125.411294 96.975041)
        (xy 125.34923 97.01531)
        (xy 125.280901 97.061354)
        (xy 125.207185 97.11772)
        (xy 125.128959 97.188959)
        (xy 125.73 97.791)
        (xy 126.331041 97.188959)
        (xy 126.252814 97.11772)
        (xy 126.179097 97.061354)
        (xy 126.110769 97.01531)
        (xy 126.048705 96.975041)
        (xy 125.993783 96.935998)
        (xy 125.94688 96.893634)
        (xy 125.908873 96.843401)
        (xy 125.880639 96.780749)
        (xy 125.863056 96.701131)
        (xy 125.857 96.6)
      )
    )
  )
  (zone (net 4) (net_name "IOVDD") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30065)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 101.5838 84.985)
        (xy 101.5818 84.993693)
        (xy 101.579801 85.002029)
        (xy 101.577801 85.010008)
        (xy 101.575802 85.01763)
        (xy 101.573803 85.024895)
        (xy 101.571803 85.031803)
        (xy 101.569804 85.038354)
        (xy 101.567804 85.044548)
        (xy 101.565805 85.050385)
        (xy 101.563806 85.055866)
        (xy 101.66 85.4635)
        (xy 101.756194 85.055866)
        (xy 101.754194 85.050385)
        (xy 101.752195 85.044548)
        (xy 101.750195 85.038354)
        (xy 101.748196 85.031803)
        (xy 101.746197 85.024895)
        (xy 101.744197 85.01763)
        (xy 101.742198 85.010008)
        (xy 101.740198 85.002029)
        (xy 101.738199 84.993693)
        (xy 101.7362 84.985)
      )
    )
  )
  (zone (net 4) (net_name "IOVDD") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30055)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 103.7362 89.2556)
        (xy 103.739071 89.215316)
        (xy 103.747112 89.18397)
        (xy 103.759466 89.159412)
        (xy 103.775275 89.139496)
        (xy 103.793682 89.122074)
        (xy 103.813829 89.104998)
        (xy 103.834858 89.086121)
        (xy 103.855912 89.063294)
        (xy 103.876133 89.03437)
        (xy 103.894665 88.997202)
        (xy 103.66 88.899)
        (xy 103.425335 88.997202)
        (xy 103.443865 89.03437)
        (xy 103.464086 89.063294)
        (xy 103.48514 89.086121)
        (xy 103.50617 89.104998)
        (xy 103.526317 89.122074)
        (xy 103.544724 89.139496)
        (xy 103.560533 89.159412)
        (xy 103.572887 89.18397)
        (xy 103.580928 89.215316)
        (xy 103.5838 89.2556)
      )
    )
  )
  (zone (net 9) (net_name "/GPIO4") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30073)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 99.5838 84.985)
        (xy 99.5818 84.993693)
        (xy 99.579801 85.002029)
        (xy 99.577801 85.010008)
        (xy 99.575802 85.01763)
        (xy 99.573803 85.024895)
        (xy 99.571803 85.031803)
        (xy 99.569804 85.038354)
        (xy 99.567804 85.044548)
        (xy 99.565805 85.050385)
        (xy 99.563806 85.055866)
        (xy 99.66 85.4635)
        (xy 99.756194 85.055866)
        (xy 99.754194 85.050385)
        (xy 99.752195 85.044548)
        (xy 99.750195 85.038354)
        (xy 99.748196 85.031803)
        (xy 99.746197 85.024895)
        (xy 99.744197 85.01763)
        (xy 99.742198 85.010008)
        (xy 99.740198 85.002029)
        (xy 99.738199 84.993693)
        (xy 99.7362 84.985)
      )
    )
  )
  (zone (net 22) (net_name "/GPIO17") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30096)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 95.145 91.5762)
        (xy 95.152086 91.576592)
        (xy 95.159173 91.577342)
        (xy 95.166259 91.578449)
        (xy 95.173346 91.579913)
        (xy 95.180433 91.581734)
        (xy 95.187519 91.583912)
        (xy 95.194606 91.586447)
        (xy 95.201692 91.589339)
        (xy 95.208779 91.592588)
        (xy 95.215866 91.596194)
        (xy 95.6235 91.5)
        (xy 95.215866 91.403806)
        (xy 95.208779 91.407411)
        (xy 95.201692 91.41066)
        (xy 95.194606 91.413552)
        (xy 95.187519 91.416087)
        (xy 95.180433 91.418265)
        (xy 95.173346 91.420086)
        (xy 95.166259 91.42155)
        (xy 95.159173 91.422657)
        (xy 95.152086 91.423407)
        (xy 95.145 91.4238)
      )
    )
  )
  (zone (net 42) (net_name "SWCLK") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30097)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 95.145 89.9762)
        (xy 95.152086 89.976592)
        (xy 95.159173 89.977342)
        (xy 95.166259 89.978449)
        (xy 95.173346 89.979913)
        (xy 95.180433 89.981734)
        (xy 95.187519 89.983912)
        (xy 95.194606 89.986447)
        (xy 95.201692 89.989339)
        (xy 95.208779 89.992588)
        (xy 95.215866 89.996194)
        (xy 95.6235 89.9)
        (xy 95.215866 89.803806)
        (xy 95.208779 89.807411)
        (xy 95.201692 89.81066)
        (xy 95.194606 89.813552)
        (xy 95.187519 89.816087)
        (xy 95.180433 89.818265)
        (xy 95.173346 89.820086)
        (xy 95.166259 89.82155)
        (xy 95.159173 89.822657)
        (xy 95.152086 89.823407)
        (xy 95.145 89.8238)
      )
    )
  )
  (zone (net 50) (net_name "VREG_IN") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30110)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 102.975 91.0238)
        (xy 102.967913 91.023407)
        (xy 102.960826 91.022657)
        (xy 102.95374 91.02155)
        (xy 102.946653 91.020086)
        (xy 102.939567 91.018265)
        (xy 102.93248 91.016087)
        (xy 102.925393 91.013552)
        (xy 102.918307 91.01066)
        (xy 102.91122 91.007411)
        (xy 102.904134 91.003806)
        (xy 102.4965 91.1)
        (xy 102.904134 91.196194)
        (xy 102.91122 91.192588)
        (xy 102.918307 91.189339)
        (xy 102.925393 91.186447)
        (xy 102.93248 91.183912)
        (xy 102.939567 91.181734)
        (xy 102.946653 91.179913)
        (xy 102.95374 91.178449)
        (xy 102.960826 91.177342)
        (xy 102.967913 91.176592)
        (xy 102.975 91.1762)
      )
    )
  )
  (zone (net 37) (net_name "/QSPI.D0") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30036)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 123.2662 81.2)
        (xy 123.273364 81.09519)
        (xy 123.294008 81.014058)
        (xy 123.326851 80.95155)
        (xy 123.370617 80.902614)
        (xy 123.424028 80.862196)
        (xy 123.485807 80.825244)
        (xy 123.554675 80.786706)
        (xy 123.629355 80.741527)
        (xy 123.70857 80.684657)
        (xy 123.791041 80.611041)
        (xy 123.19 80.009)
        (xy 122.588959 80.611041)
        (xy 122.671429 80.684657)
        (xy 122.750643 80.741527)
        (xy 122.825323 80.786706)
        (xy 122.894192 80.825244)
        (xy 122.95597 80.862196)
        (xy 123.009382 80.902614)
        (xy 123.053148 80.95155)
        (xy 123.085991 81.014058)
        (xy 123.106635 81.09519)
        (xy 123.1138 81.2)
      )
    )
  )
  (zone (net 46) (net_name "DVDD") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30099)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 102.02 88.7762)
        (xy 102.027086 88.776592)
        (xy 102.034173 88.777342)
        (xy 102.041259 88.778449)
        (xy 102.048346 88.779913)
        (xy 102.055433 88.781734)
        (xy 102.062519 88.783912)
        (xy 102.069606 88.786447)
        (xy 102.076692 88.789339)
        (xy 102.083779 88.792588)
        (xy 102.090866 88.796194)
        (xy 102.4985 88.7)
        (xy 102.090866 88.603806)
        (xy 102.083779 88.607411)
        (xy 102.076692 88.61066)
        (xy 102.069606 88.613552)
        (xy 102.062519 88.616087)
        (xy 102.055433 88.618265)
        (xy 102.048346 88.620086)
        (xy 102.041259 88.62155)
        (xy 102.034173 88.622657)
        (xy 102.027086 88.623407)
        (xy 102.02 88.6238)
      )
    )
  )
  (zone (net 33) (net_name "/GPIO28") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30019)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 107.8738 96.6)
        (xy 107.866635 96.704808)
        (xy 107.845991 96.78594)
        (xy 107.813148 96.848448)
        (xy 107.769382 96.897384)
        (xy 107.71597 96.937802)
        (xy 107.654192 96.974754)
        (xy 107.585323 97.013293)
        (xy 107.510643 97.058471)
        (xy 107.431429 97.115342)
        (xy 107.348959 97.188959)
        (xy 107.95 97.791)
        (xy 108.551041 97.188959)
        (xy 108.46857 97.115342)
        (xy 108.389355 97.058471)
        (xy 108.314675 97.013293)
        (xy 108.245807 96.974754)
        (xy 108.184028 96.937802)
        (xy 108.130617 96.897384)
        (xy 108.086851 96.848448)
        (xy 108.054008 96.78594)
        (xy 108.033364 96.704808)
        (xy 108.0262 96.6)
      )
    )
  )
  (zone (net 5) (net_name "/GPIO0") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30077)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 101.1838 84.985)
        (xy 101.1818 84.993693)
        (xy 101.179801 85.002029)
        (xy 101.177801 85.010008)
        (xy 101.175802 85.01763)
        (xy 101.173803 85.024895)
        (xy 101.171803 85.031803)
        (xy 101.169804 85.038354)
        (xy 101.167804 85.044548)
        (xy 101.165805 85.050385)
        (xy 101.163806 85.055866)
        (xy 101.26 85.4635)
        (xy 101.356194 85.055866)
        (xy 101.354194 85.050385)
        (xy 101.352195 85.044548)
        (xy 101.350195 85.038354)
        (xy 101.348196 85.031803)
        (xy 101.346197 85.024895)
        (xy 101.344197 85.01763)
        (xy 101.342198 85.010008)
        (xy 101.340198 85.002029)
        (xy 101.338199 84.993693)
        (xy 101.3362 84.985)
      )
    )
  )
  (zone (net 6) (net_name "/GPIO1") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30032)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 113.1062 81.2)
        (xy 113.113364 81.09519)
        (xy 113.134008 81.014058)
        (xy 113.166851 80.95155)
        (xy 113.210617 80.902614)
        (xy 113.264028 80.862196)
        (xy 113.325807 80.825244)
        (xy 113.394675 80.786706)
        (xy 113.469355 80.741527)
        (xy 113.54857 80.684657)
        (xy 113.631041 80.611041)
        (xy 113.03 80.009)
        (xy 112.428959 80.611041)
        (xy 112.511429 80.684657)
        (xy 112.590643 80.741527)
        (xy 112.665323 80.786706)
        (xy 112.734192 80.825244)
        (xy 112.79597 80.862196)
        (xy 112.849382 80.902614)
        (xy 112.893148 80.95155)
        (xy 112.925991 81.014058)
        (xy 112.946635 81.09519)
        (xy 112.9538 81.2)
      )
    )
  )
  (zone (net 14) (net_name "/GPIO9") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30066)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 97.1838 84.985)
        (xy 97.1818 84.993693)
        (xy 97.179801 85.002029)
        (xy 97.177801 85.010008)
        (xy 97.175802 85.01763)
        (xy 97.173803 85.024895)
        (xy 97.171803 85.031803)
        (xy 97.169804 85.038354)
        (xy 97.167804 85.044548)
        (xy 97.165805 85.050385)
        (xy 97.163806 85.055866)
        (xy 97.26 85.4635)
        (xy 97.356194 85.055866)
        (xy 97.354194 85.050385)
        (xy 97.352195 85.044548)
        (xy 97.350195 85.038354)
        (xy 97.348196 85.031803)
        (xy 97.346197 85.024895)
        (xy 97.344197 85.01763)
        (xy 97.342198 85.010008)
        (xy 97.340198 85.002029)
        (xy 97.338199 84.993693)
        (xy 97.3362 84.985)
      )
    )
  )
  (zone (net 46) (net_name "DVDD") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30054)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 101.8156 90.6238)
        (xy 101.775316 90.620928)
        (xy 101.74397 90.612887)
        (xy 101.719412 90.600533)
        (xy 101.699496 90.584724)
        (xy 101.682074 90.566317)
        (xy 101.664998 90.54617)
        (xy 101.646121 90.52514)
        (xy 101.623294 90.504086)
        (xy 101.59437 90.483865)
        (xy 101.557202 90.465335)
        (xy 101.459 90.7)
        (xy 101.557202 90.934665)
        (xy 101.59437 90.916133)
        (xy 101.623294 90.895912)
        (xy 101.646121 90.874858)
        (xy 101.664998 90.853829)
        (xy 101.682074 90.833682)
        (xy 101.699496 90.815275)
        (xy 101.719412 90.799466)
        (xy 101.74397 90.787112)
        (xy 101.775316 90.779071)
        (xy 101.8156 90.7762)
      )
    )
  )
  (zone (net 38) (net_name "/QSPI.D3") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30114)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 102.975 88.2238)
        (xy 102.967913 88.223407)
        (xy 102.960826 88.222657)
        (xy 102.95374 88.22155)
        (xy 102.946653 88.220086)
        (xy 102.939567 88.218265)
        (xy 102.93248 88.216087)
        (xy 102.925393 88.213552)
        (xy 102.918307 88.21066)
        (xy 102.91122 88.207411)
        (xy 102.904134 88.203806)
        (xy 102.4965 88.3)
        (xy 102.904134 88.396194)
        (xy 102.91122 88.392588)
        (xy 102.918307 88.389339)
        (xy 102.925393 88.386447)
        (xy 102.93248 88.383912)
        (xy 102.939567 88.381734)
        (xy 102.946653 88.379913)
        (xy 102.95374 88.378449)
        (xy 102.960826 88.377342)
        (xy 102.967913 88.376592)
        (xy 102.975 88.3762)
      )
    )
  )
  (zone (net 8) (net_name "/GPIO3") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30029)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 108.0262 81.2)
        (xy 108.033364 81.09519)
        (xy 108.054008 81.014058)
        (xy 108.086851 80.95155)
        (xy 108.130617 80.902614)
        (xy 108.184028 80.862196)
        (xy 108.245807 80.825244)
        (xy 108.314675 80.786706)
        (xy 108.389355 80.741527)
        (xy 108.46857 80.684657)
        (xy 108.551041 80.611041)
        (xy 107.95 80.009)
        (xy 107.348959 80.611041)
        (xy 107.431429 80.684657)
        (xy 107.510643 80.741527)
        (xy 107.585323 80.786706)
        (xy 107.654192 80.825244)
        (xy 107.71597 80.862196)
        (xy 107.769382 80.902614)
        (xy 107.813148 80.95155)
        (xy 107.845991 81.014058)
        (xy 107.866635 81.09519)
        (xy 107.8738 81.2)
      )
    )
  )
  (zone (net 10) (net_name "/GPIO5") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30072)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 99.1838 84.985)
        (xy 99.1818 84.993693)
        (xy 99.179801 85.002029)
        (xy 99.177801 85.010008)
        (xy 99.175802 85.01763)
        (xy 99.173803 85.024895)
        (xy 99.171803 85.031803)
        (xy 99.169804 85.038354)
        (xy 99.167804 85.044548)
        (xy 99.165805 85.050385)
        (xy 99.163806 85.055866)
        (xy 99.26 85.4635)
        (xy 99.356194 85.055866)
        (xy 99.354194 85.050385)
        (xy 99.352195 85.044548)
        (xy 99.350195 85.038354)
        (xy 99.348196 85.031803)
        (xy 99.346197 85.024895)
        (xy 99.344197 85.01763)
        (xy 99.342198 85.010008)
        (xy 99.340198 85.002029)
        (xy 99.338199 84.993693)
        (xy 99.3362 84.985)
      )
    )
  )
  (zone (net 4) (net_name "IOVDD") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30052)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 101.862435 84.605328)
        (xy 101.892949 84.578873)
        (xy 101.920801 84.562394)
        (xy 101.946901 84.553765)
        (xy 101.972162 84.550861)
        (xy 101.997497 84.551557)
        (xy 102.023818 84.553729)
        (xy 102.052036 84.55525)
        (xy 102.083065 84.553997)
        (xy 102.117816 84.547843)
        (xy 102.157202 84.534665)
        (xy 102.060707 84.299293)
        (xy 101.825335 84.202798)
        (xy 101.812155 84.242183)
        (xy 101.806002 84.276933)
        (xy 101.804748 84.307962)
        (xy 101.80627 84.33618)
        (xy 101.808441 84.362501)
        (xy 101.809137 84.387836)
        (xy 101.806234 84.413097)
        (xy 101.797605 84.439198)
        (xy 101.781126 84.46705)
        (xy 101.754672 84.497565)
      )
    )
  )
  (zone (net 37) (net_name "/QSPI.D0") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30115)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 102.975 87.4238)
        (xy 102.967913 87.423407)
        (xy 102.960826 87.422657)
        (xy 102.95374 87.42155)
        (xy 102.946653 87.420086)
        (xy 102.939567 87.418265)
        (xy 102.93248 87.416087)
        (xy 102.925393 87.413552)
        (xy 102.918307 87.41066)
        (xy 102.91122 87.407411)
        (xy 102.904134 87.403806)
        (xy 102.4965 87.5)
        (xy 102.904134 87.596194)
        (xy 102.91122 87.592588)
        (xy 102.918307 87.589339)
        (xy 102.925393 87.586447)
        (xy 102.93248 87.583912)
        (xy 102.939567 87.581734)
        (xy 102.946653 87.579913)
        (xy 102.95374 87.578449)
        (xy 102.960826 87.577342)
        (xy 102.967913 87.576592)
        (xy 102.975 87.5762)
      )
    )
  )
  (zone (net 12) (net_name "/GPIO7") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30069)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 98.3838 84.985)
        (xy 98.3818 84.993693)
        (xy 98.379801 85.002029)
        (xy 98.377801 85.010008)
        (xy 98.375802 85.01763)
        (xy 98.373803 85.024895)
        (xy 98.371803 85.031803)
        (xy 98.369804 85.038354)
        (xy 98.367804 85.044548)
        (xy 98.365805 85.050385)
        (xy 98.363806 85.055866)
        (xy 98.46 85.4635)
        (xy 98.556194 85.055866)
        (xy 98.554194 85.050385)
        (xy 98.552195 85.044548)
        (xy 98.550195 85.038354)
        (xy 98.548196 85.031803)
        (xy 98.546197 85.024895)
        (xy 98.544197 85.01763)
        (xy 98.542198 85.010008)
        (xy 98.540198 85.002029)
        (xy 98.538199 84.993693)
        (xy 98.5362 84.985)
      )
    )
  )
  (zone (net 13) (net_name "/GPIO8") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30067)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 97.5838 84.985)
        (xy 97.5818 84.993693)
        (xy 97.579801 85.002029)
        (xy 97.577801 85.010008)
        (xy 97.575802 85.01763)
        (xy 97.573803 85.024895)
        (xy 97.571803 85.031803)
        (xy 97.569804 85.038354)
        (xy 97.567804 85.044548)
        (xy 97.565805 85.050385)
        (xy 97.563806 85.055866)
        (xy 97.66 85.4635)
        (xy 97.756194 85.055866)
        (xy 97.754194 85.050385)
        (xy 97.752195 85.044548)
        (xy 97.750195 85.038354)
        (xy 97.748196 85.031803)
        (xy 97.746197 85.024895)
        (xy 97.744197 85.01763)
        (xy 97.742198 85.010008)
        (xy 97.740198 85.002029)
        (xy 97.738199 84.993693)
        (xy 97.7362 84.985)
      )
    )
  )
  (zone (net 16) (net_name "/GPIO11") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30024)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 87.7062 81.2)
        (xy 87.713364 81.09519)
        (xy 87.734008 81.014058)
        (xy 87.766851 80.95155)
        (xy 87.810617 80.902614)
        (xy 87.864028 80.862196)
        (xy 87.925807 80.825244)
        (xy 87.994675 80.786706)
        (xy 88.069355 80.741527)
        (xy 88.14857 80.684657)
        (xy 88.231041 80.611041)
        (xy 87.63 80.009)
        (xy 87.028959 80.611041)
        (xy 87.111429 80.684657)
        (xy 87.190643 80.741527)
        (xy 87.265323 80.786706)
        (xy 87.334192 80.825244)
        (xy 87.39597 80.862196)
        (xy 87.449382 80.902614)
        (xy 87.493148 80.95155)
        (xy 87.525991 81.014058)
        (xy 87.546635 81.09519)
        (xy 87.5538 81.2)
      )
    )
  )
  (zone (net 4) (net_name "IOVDD") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30087)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 101.7362 92.815)
        (xy 101.738199 92.806306)
        (xy 101.740198 92.79797)
        (xy 101.742198 92.789991)
        (xy 101.744197 92.782369)
        (xy 101.746197 92.775104)
        (xy 101.748196 92.768196)
        (xy 101.750195 92.761645)
        (xy 101.752195 92.755451)
        (xy 101.754194 92.749614)
        (xy 101.756194 92.744134)
        (xy 101.66 92.3365)
        (xy 101.563806 92.744134)
        (xy 101.565805 92.749614)
        (xy 101.567804 92.755451)
        (xy 101.569804 92.761645)
        (xy 101.571803 92.768196)
        (xy 101.573803 92.775104)
        (xy 101.575802 92.782369)
        (xy 101.577801 92.789991)
        (xy 101.579801 92.79797)
        (xy 101.5818 92.806306)
        (xy 101.5838 92.815)
      )
    )
  )
  (zone (net 36) (net_name "/QSPI.SS") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30116)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 102.975 86.2238)
        (xy 102.967913 86.223407)
        (xy 102.960826 86.222657)
        (xy 102.95374 86.22155)
        (xy 102.946653 86.220086)
        (xy 102.939567 86.218265)
        (xy 102.93248 86.216087)
        (xy 102.925393 86.213552)
        (xy 102.918307 86.21066)
        (xy 102.91122 86.207411)
        (xy 102.904134 86.203806)
        (xy 102.4965 86.3)
        (xy 102.904134 86.396194)
        (xy 102.91122 86.392588)
        (xy 102.918307 86.389339)
        (xy 102.925393 86.386447)
        (xy 102.93248 86.383912)
        (xy 102.939567 86.381734)
        (xy 102.946653 86.379913)
        (xy 102.95374 86.378449)
        (xy 102.960826 86.377342)
        (xy 102.967913 86.376592)
        (xy 102.975 86.3762)
      )
    )
  )
  (zone (net 10) (net_name "/GPIO5") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30023)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 102.9462 81.2)
        (xy 102.953364 81.09519)
        (xy 102.974008 81.014058)
        (xy 103.006851 80.95155)
        (xy 103.050617 80.902614)
        (xy 103.104028 80.862196)
        (xy 103.165807 80.825244)
        (xy 103.234675 80.786706)
        (xy 103.309355 80.741527)
        (xy 103.38857 80.684657)
        (xy 103.471041 80.611041)
        (xy 102.87 80.009)
        (xy 102.268959 80.611041)
        (xy 102.351429 80.684657)
        (xy 102.430643 80.741527)
        (xy 102.505323 80.786706)
        (xy 102.574192 80.825244)
        (xy 102.63597 80.862196)
        (xy 102.689382 80.902614)
        (xy 102.733148 80.95155)
        (xy 102.765991 81.014058)
        (xy 102.786635 81.09519)
        (xy 102.7938 81.2)
      )
    )
  )
  (zone (net 1) (net_name "Net-(U1-USB_DP)") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30108)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 102.975 89.8238)
        (xy 102.967913 89.823407)
        (xy 102.960826 89.822657)
        (xy 102.95374 89.82155)
        (xy 102.946653 89.820086)
        (xy 102.939567 89.818265)
        (xy 102.93248 89.816087)
        (xy 102.925393 89.813552)
        (xy 102.918307 89.81066)
        (xy 102.91122 89.807411)
        (xy 102.904134 89.803806)
        (xy 102.4965 89.9)
        (xy 102.904134 89.996194)
        (xy 102.91122 89.992588)
        (xy 102.918307 89.989339)
        (xy 102.925393 89.986447)
        (xy 102.93248 89.983912)
        (xy 102.939567 89.981734)
        (xy 102.946653 89.979913)
        (xy 102.95374 89.978449)
        (xy 102.960826 89.977342)
        (xy 102.967913 89.976592)
        (xy 102.975 89.9762)
      )
    )
  )
  (zone (net 20) (net_name "/GPIO15") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30028)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 77.5462 81.2)
        (xy 77.553364 81.09519)
        (xy 77.574008 81.014058)
        (xy 77.606851 80.95155)
        (xy 77.650617 80.902614)
        (xy 77.704028 80.862196)
        (xy 77.765807 80.825244)
        (xy 77.834675 80.786706)
        (xy 77.909355 80.741527)
        (xy 77.98857 80.684657)
        (xy 78.071041 80.611041)
        (xy 77.47 80.009)
        (xy 76.868959 80.611041)
        (xy 76.951429 80.684657)
        (xy 77.030643 80.741527)
        (xy 77.105323 80.786706)
        (xy 77.174192 80.825244)
        (xy 77.23597 80.862196)
        (xy 77.289382 80.902614)
        (xy 77.333148 80.95155)
        (xy 77.365991 81.014058)
        (xy 77.386635 81.09519)
        (xy 77.3938 81.2)
      )
    )
  )
  (zone (net 19) (net_name "/GPIO14") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30039)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 80.0862 81.2)
        (xy 80.093364 81.09519)
        (xy 80.114008 81.014058)
        (xy 80.146851 80.95155)
        (xy 80.190617 80.902614)
        (xy 80.244028 80.862196)
        (xy 80.305807 80.825244)
        (xy 80.374675 80.786706)
        (xy 80.449355 80.741527)
        (xy 80.52857 80.684657)
        (xy 80.611041 80.611041)
        (xy 80.01 80.009)
        (xy 79.408959 80.611041)
        (xy 79.491429 80.684657)
        (xy 79.570643 80.741527)
        (xy 79.645323 80.786706)
        (xy 79.714192 80.825244)
        (xy 79.77597 80.862196)
        (xy 79.829382 80.902614)
        (xy 79.873148 80.95155)
        (xy 79.905991 81.014058)
        (xy 79.926635 81.09519)
        (xy 79.9338 81.2)
      )
    )
  )
  (zone (net 22) (net_name "/GPIO17") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30011)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 79.9338 96.6)
        (xy 79.926635 96.704808)
        (xy 79.905991 96.78594)
        (xy 79.873148 96.848448)
        (xy 79.829382 96.897384)
        (xy 79.77597 96.937802)
        (xy 79.714192 96.974754)
        (xy 79.645323 97.013293)
        (xy 79.570643 97.058471)
        (xy 79.491429 97.115342)
        (xy 79.408959 97.188959)
        (xy 80.01 97.791)
        (xy 80.611041 97.188959)
        (xy 80.52857 97.115342)
        (xy 80.449355 97.058471)
        (xy 80.374675 97.013293)
        (xy 80.305807 96.974754)
        (xy 80.244028 96.937802)
        (xy 80.190617 96.897384)
        (xy 80.146851 96.848448)
        (xy 80.114008 96.78594)
        (xy 80.093364 96.704808)
        (xy 80.0862 96.6)
      )
    )
  )
  (zone (net 35) (net_name "/QSPI.SCLK") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30034)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 125.8062 81.2)
        (xy 125.813364 81.09519)
        (xy 125.834008 81.014058)
        (xy 125.866851 80.95155)
        (xy 125.910617 80.902614)
        (xy 125.964028 80.862196)
        (xy 126.025807 80.825244)
        (xy 126.094675 80.786706)
        (xy 126.169355 80.741527)
        (xy 126.24857 80.684657)
        (xy 126.331041 80.611041)
        (xy 125.73 80.009)
        (xy 125.128959 80.611041)
        (xy 125.211429 80.684657)
        (xy 125.290643 80.741527)
        (xy 125.365323 80.786706)
        (xy 125.434192 80.825244)
        (xy 125.49597 80.862196)
        (xy 125.549382 80.902614)
        (xy 125.593148 80.95155)
        (xy 125.625991 81.014058)
        (xy 125.646635 81.09519)
        (xy 125.6538 81.2)
      )
    )
  )
  (zone (net 45) (net_name "GNDD") (layers "F&B.Cu") (name "GND") (hatch edge 0.508)
    (connect_pads (clearance 0.2))
    (min_thickness 0.2) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.22) (thermal_bridge_width 0.4))
    (polygon
      (pts
        (xy 127 99.06)
        (xy 76.2 99.06)
        (xy 76.2 78.74)
        (xy 127 78.74)
      )
    )
  )
  (zone (net 4) (net_name "IOVDD") (layer "B.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30005)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 113.284 94.905)
        (xy 113.303599 94.861992)
        (xy 113.323199 94.821718)
        (xy 113.342799 94.784175)
        (xy 113.362399 94.749366)
        (xy 113.382 94.717288)
        (xy 113.4016 94.687943)
        (xy 113.4212 94.66133)
        (xy 113.4408 94.63745)
        (xy 113.4604 94.616302)
        (xy 113.48 94.597887)
        (xy 113.03 94.274)
        (xy 112.58 94.597887)
        (xy 112.599599 94.616302)
        (xy 112.619199 94.63745)
        (xy 112.638799 94.66133)
        (xy 112.658399 94.687943)
        (xy 112.678 94.717288)
        (xy 112.6976 94.749366)
        (xy 112.7172 94.784175)
        (xy 112.7368 94.821718)
        (xy 112.7564 94.861992)
        (xy 112.776 94.905)
      )
    )
  )
  (zone (net 43) (net_name "RUN") (layer "B.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30003)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 87.7062 87.55)
        (xy 87.713364 87.44519)
        (xy 87.734008 87.364058)
        (xy 87.766851 87.30155)
        (xy 87.810617 87.252614)
        (xy 87.864028 87.212196)
        (xy 87.925807 87.175244)
        (xy 87.994675 87.136706)
        (xy 88.069355 87.091527)
        (xy 88.14857 87.034657)
        (xy 88.231041 86.961041)
        (xy 87.63 86.359)
        (xy 87.028959 86.961041)
        (xy 87.111429 87.034657)
        (xy 87.190643 87.091527)
        (xy 87.265323 87.136706)
        (xy 87.334192 87.175244)
        (xy 87.39597 87.212196)
        (xy 87.449382 87.252614)
        (xy 87.493148 87.30155)
        (xy 87.525991 87.364058)
        (xy 87.546635 87.44519)
        (xy 87.5538 87.55)
      )
    )
  )
  (zone (net 40) (net_name "/QSPI.D1") (layer "B.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30002)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 109.3 86.4362)
        (xy 109.346448 86.474187)
        (xy 109.392896 86.518163)
        (xy 109.439344 86.568126)
        (xy 109.485792 86.624077)
        (xy 109.53224 86.686015)
        (xy 109.578687 86.753941)
        (xy 109.625135 86.827854)
        (xy 109.671583 86.907755)
        (xy 109.718031 86.993643)
        (xy 109.76448 87.08552)
        (xy 110.491 86.36)
        (xy 109.76448 85.63448)
        (xy 109.718031 85.726356)
        (xy 109.671583 85.812244)
        (xy 109.625135 85.892145)
        (xy 109.578687 85.966058)
        (xy 109.53224 86.033984)
        (xy 109.485792 86.095922)
        (xy 109.439344 86.151873)
        (xy 109.392896 86.201836)
        (xy 109.346448 86.245812)
        (xy 109.3 86.2838)
      )
    )
  )
  (zone (net 4) (net_name "IOVDD") (layer "B.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30001)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 120.396 96.6)
        (xy 120.386366 96.734863)
        (xy 120.359387 96.839783)
        (xy 120.317941 96.921956)
        (xy 120.26491 96.988577)
        (xy 120.203173 97.046844)
        (xy 120.135609 97.103951)
        (xy 120.065101 97.167096)
        (xy 119.994526 97.243475)
        (xy 119.926767 97.340284)
        (xy 119.864702 97.464719)
        (xy 120.65 97.791)
        (xy 121.435298 97.464719)
        (xy 121.373232 97.340284)
        (xy 121.305472 97.243475)
        (xy 121.234898 97.167096)
        (xy 121.164389 97.103951)
        (xy 121.096826 97.046844)
        (xy 121.035089 96.988577)
        (xy 120.982057 96.921956)
        (xy 120.940612 96.839783)
        (xy 120.913633 96.734863)
        (xy 120.904 96.6)
      )
    )
  )
  (zone (net 39) (net_name "/QSPI.D2") (layer "B.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30008)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 105.774703 86.382903)
        (xy 105.734419 86.380031)
        (xy 105.703073 86.37199)
        (xy 105.678515 86.359636)
        (xy 105.658599 86.343827)
        (xy 105.641177 86.32542)
        (xy 105.624101 86.305273)
        (xy 105.605224 86.284243)
        (xy 105.582397 86.263189)
        (xy 105.553473 86.242968)
        (xy 105.516305 86.224438)
        (xy 105.418103 86.459103)
        (xy 105.516305 86.693768)
        (xy 105.553473 86.675236)
        (xy 105.582397 86.655015)
        (xy 105.605224 86.633961)
        (xy 105.624101 86.612932)
        (xy 105.641177 86.592785)
        (xy 105.658599 86.574378)
        (xy 105.678515 86.558569)
        (xy 105.703073 86.546215)
        (xy 105.734419 86.538174)
        (xy 105.774703 86.535303)
      )
    )
  )
  (zone (net 4) (net_name "IOVDD") (layer "B.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30000)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 112.776 96.6)
        (xy 112.766366 96.734863)
        (xy 112.739387 96.839783)
        (xy 112.697941 96.921956)
        (xy 112.64491 96.988577)
        (xy 112.583173 97.046844)
        (xy 112.515609 97.103951)
        (xy 112.445101 97.167096)
        (xy 112.374526 97.243475)
        (xy 112.306767 97.340284)
        (xy 112.244702 97.464719)
        (xy 113.03 97.791)
        (xy 113.815298 97.464719)
        (xy 113.753232 97.340284)
        (xy 113.685472 97.243475)
        (xy 113.614898 97.167096)
        (xy 113.544389 97.103951)
        (xy 113.476826 97.046844)
        (xy 113.415089 96.988577)
        (xy 113.362057 96.921956)
        (xy 113.320612 96.839783)
        (xy 113.293633 96.734863)
        (xy 113.284 96.6)
      )
    )
  )
  (zone (net 39) (net_name "/QSPI.D2") (layer "B.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30004)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 113.1062 87.55)
        (xy 113.113364 87.44519)
        (xy 113.134008 87.364058)
        (xy 113.166851 87.30155)
        (xy 113.210617 87.252614)
        (xy 113.264028 87.212196)
        (xy 113.325807 87.175244)
        (xy 113.394675 87.136706)
        (xy 113.469355 87.091527)
        (xy 113.54857 87.034657)
        (xy 113.631041 86.961041)
        (xy 113.03 86.359)
        (xy 112.428959 86.961041)
        (xy 112.511429 87.034657)
        (xy 112.590643 87.091527)
        (xy 112.665323 87.136706)
        (xy 112.734192 87.175244)
        (xy 112.79597 87.212196)
        (xy 112.849382 87.252614)
        (xy 112.893148 87.30155)
        (xy 112.925991 87.364058)
        (xy 112.946635 87.44519)
        (xy 112.9538 87.55)
      )
    )
  )
  (zone (net 40) (net_name "/QSPI.D1") (layer "B.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30007)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 106.4156 85.4238)
        (xy 106.375316 85.420928)
        (xy 106.34397 85.412887)
        (xy 106.319412 85.400533)
        (xy 106.299496 85.384724)
        (xy 106.282074 85.366317)
        (xy 106.264998 85.34617)
        (xy 106.246121 85.32514)
        (xy 106.223294 85.304086)
        (xy 106.19437 85.283865)
        (xy 106.157202 85.265335)
        (xy 106.059 85.5)
        (xy 106.157202 85.734665)
        (xy 106.19437 85.716133)
        (xy 106.223294 85.695912)
        (xy 106.246121 85.674858)
        (xy 106.264998 85.653829)
        (xy 106.282074 85.633682)
        (xy 106.299496 85.615275)
        (xy 106.319412 85.599466)
        (xy 106.34397 85.587112)
        (xy 106.375316 85.579071)
        (xy 106.4156 85.5762)
      )
    )
  )
  (zone (net 43) (net_name "RUN") (layer "B.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30006)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 87.5538 90.5444)
        (xy 87.550928 90.584683)
        (xy 87.542887 90.616029)
        (xy 87.530533 90.640587)
        (xy 87.514724 90.660502)
        (xy 87.496317 90.677925)
        (xy 87.47617 90.695)
        (xy 87.45514 90.713878)
        (xy 87.434086 90.736705)
        (xy 87.413865 90.765629)
        (xy 87.395335 90.802798)
        (xy 87.63 90.901)
        (xy 87.864665 90.802798)
        (xy 87.846133 90.765629)
        (xy 87.825912 90.736705)
        (xy 87.804858 90.713878)
        (xy 87.783829 90.695)
        (xy 87.763682 90.677925)
        (xy 87.745275 90.660502)
        (xy 87.729466 90.640587)
        (xy 87.717112 90.616029)
        (xy 87.709071 90.584683)
        (xy 87.7062 90.5444)
      )
    )
  )
)
